     The files in this directory should be copied to LB:[1,1]. You may only
     use them if you have a processor with:

           - I/D Space
           - EIS
           - Floating Point processor

     This version of the DECUS-C Compiler Library was built under

                        RSX11M-PLUS V4.0

     So be careful with older versions of RSX. If your system fails, use
     [5,3]MBUILD.CMD instead to rebuild this library and the compiler.
