RSX11-M/M+ Conditional assembly symbols. Extracted from SYSGEN commandfiles.
-----------------------------------------------------------------------------
( RSX11M 4.3, RSX11M+ 4.0 )				For the DECUS RSX-SIG

    J.H.Hamakers, Asea Brown Boveri b.v., Rotterdam, The Netherlands.

A$$BIO          ; Asynchronous buffered I/O
A$$BRT          ; Specify requested exit AST directive
A$$CHK          ; Address checking
A$$CLI          ; Alternate CLI support ; Max num of CLIs
A$$CNT          ; Accounting - requires P$$OOL
A$$CPS          ; ACP support
A$$D01          ; AD01 A/D converters
A$$F11          ; AFC11 A/D converters
A$$HDR          ; Alternate task header refresh
A$$NSI          ; ANSI magtape support
A$$PRI          ; Alter Priority directive (ALTP$)
A$$R11          ; AR11 lab peripheral systems
A$$RDA          ; AR11 D/A option
A$$TRP          ; AST support
B$$LIN          ; Baseline system
B$$LV1          ; Baselevel 
B$$LV2          ; Baselevel revision
B$$MAP          ; Bitmap system (PRO)
B$$OOT          ; Address of the reboot entry point in the boot ROM
C$$CDA          ; Loadable crash driver support
C$$CHE          ; Cache memory support
C$$CKP          ; Checkpointing support
C$$CSR          ; CSR address of crash device
C$$CTC          ; CTRL/C abort support
C$$DFB          ; Deferred binding of LUT and window blocks
C$$INT          ; Connect to interrupt directive
C$$ODB          ; Overridable default to use deferred binding
C$$ONS          ; Console driver
C$$ORE          ; Size of dynamic storage region
C$$PCR          ; Checkpoint Common Region directive (CPCR$)
C$$R11          ; CR11 card readers
C$$RSH          ; Crash notification device CSR
C$$RTO          ; Time-out count for CR11 card reader
C$$RUN          ; Physical unit number of crash unit
C$$SMT          ; Cancel selective mark times
C$$TTY          ; Register/stack dump device csr address
D$$B11          ; DA11-B par. line iinterfaces
D$$CHE          ; Disk data caching - requires R$$IIC
D$$DCL          ; DCL is default CLI
D$$DDS          ; Named directory mode is the default
D$$DXD          ; Dynamic Exec debugger interface
D$$E11          ; DL11-E line interface
D$$H11          ; DH11 asynchronous line multiplexers
D$$IAG          ; User mode diagnostics
D$$ISK          ; Nonresident task support
D$$J11          ; DJ11 asynchronous line multiplexers
D$$L11          ; DL11 A/B/C/D \DLV11 line interfaces
D$$LMD          ; DL11/DLV11 modem support
D$$M11          ; DM11BB modem control interfaces
D$$MND          ; Diamond support
D$$P11          ; DP11 line interfaces
D$$PAR          ; Directive common support
D$$Q11          ; DQ11 sync. line interfaces
D$$R11          ; DR11-K option present
D$$SHF          ; Automatic dynamic memory compaction
D$$U11          ; DU11 line interfaces
D$$V11          ; DHU11/DHV11 asynchronous line multiplexers
D$$VMD          ; DHU11/DHV11 modem support
D$$W11          ; DUP11 line interfaces
D$$WCK          ; Disk writecheck support
D$$YNC          ; Dynamic checkpoint allocation
D$$YNM          ; Dynamic memory allocation support
D$$Z11          ; DZ11/DZQ11/DZV11 asynch line multiplexers
D$$ZMD          ; DZ11/DZQ11/DZV11 modem support
E$$ACT          ; Logging of concurrent I/O
E$$BUF          ; Number of event logging buffers
E$$DVC          ; Device error logging support
E$$EAE          ; EAE support
E$$ICM          ; ERRLOG: inhibit console messages
E$$LOG          ; Error logging support
E$$MOU          ; ERRLOG: log mounts and dismounts
E$$NSI          ; Nonsense interrupt error logging
E$$PER          ; Log parity error traps
E$$SEF          ; ERRLOG: use special file formats
E$$VNT          ; Turn on event logging routines
E$$XPR          ; Extend Task directive (EXTK$)
F$$DVN          ; Decimal version numbers
F$$LPP          ; Floating point processor support
F$$LTP          ; FIS support
F$$LVL          ; File structure level support
F$$MAP          ; Fast map facility
F$$NIM          ; Deleted disk image of fixed task support
G$$DVI          ; Get Device Information directive (GDVI$) not supported
G$$EFN          ; Group global event flags
G$$GEF          ; Group global event flag support
G$$SPA          ; Constant, set by Exec
G$$TPP          ; Get Partition Parameters directive (GPRT$)
G$$TSS          ; Get Sense Switches directive (GSSW$)
G$$TTK          ; Get Task Parameters directive (GTSK$)
G$$WRD          ; Include $GTWRD code
H$$FME          ; Number of fast map extension entries
H$$FMS          ; Size of a fast map extension entry
H$$FMX          ; Size of a fast map extension in 32-word blocks
H$$GEN          ;
H$$HNM          ; Number of hash cells in each hash table, set by Exec
H$$RTZ          ; Line frequency
I$$Cxx          ; ICS/ICR-11 xx modules
I$$C11          ; ICS/ICR-11 indus control subsystem
I$$CAD          ; ICS/ICR-11 a/d converter modules
I$$CLK          ; ICS/ICR task activation from interrupts
I$$CR           ; ICR/11 remote unit
I$$CSZ          ; ICB pool size in words
I$$CWD          ; ICS/ICR-11 error count
I$$P11          ; IP11/IP300 industrial I/O subsystem support
I$$P14          ;
I$$PAD          ;
I$$PFS          ; IP11 power fail support
I$$PFS          ; IP11/IP300 power fail
I$$RAR          ; Install, request, and remove on exit
I$$RDN          ; I/O rundown
I$$S11          ; DRS/DSS-11 input/output modules
I$$SCM          ;
I$$SDR          ; DRS-11 output modules
I$$SDS          ; DSS-11 input modules
I$$SLK          ; Task activation from interrupts
I$$SPW          ; DRS-11 power recovery
I$$SSC          ; DSS-11 command register address
K$$AST          ;
K$$CNT          ; Count register address
K$$CSR          ; Clock CSR address
K$$DAS          ; Kernel data space support
K$$IEN          ; Clock interrupt enable (KW11-P at line freq)
K$$LDC          ; Load count value
K$$TPS          ; Ticks per second
K$$W11          ; KW11-Y support
L$$11R          ; Fast printer support
L$$50H          ; 50HZ line frequency (for TTDRV)
L$$A11          ; LPA11 lab peripheral accelators
L$$ASG          ; Logical unit/device assignment support
L$$CDA          ; Loadable crash driver
L$$DBG          ; Enable MP lock debugging code
L$$DRV          ; Loadable driver support
L$$GCL          ; Logical name support
L$$KPC          ; KMC11 polling count
L$$LDR          ; Loadable loader support
L$$NAM          ; Named directory support in DCL
L$$P11          ; LP/LS/LV11/LA180 line printers
L$$PS1          ; LPS11 lab peripheral system
L$$PTO          ; Time-out period for LP11 printers
L$$R11          ; PCL11 receivers
L$$SBF          ; LPS11 bandwidth filtering
L$$SDA          ; LPS11 D/A option
L$$SDR          ; LPSDR-A present
L$$SGR          ; LPS11 gain ranging option
L$$SI1          ; LSI-11 processor
L$$T11          ; PCL11 transmitters
M$$ACD          ; Multiaccess Exec support
M$$ANS          ; Seconds to wait for carrier after ring
M$$CAR          ; Seconds to wait for lost carrier to return
M$$CLI          ; Multiple CLI support (never defined w/a$$cli)
M$$CRB          ; Number of characters in an MCR buffer
M$$CRI          ; Number of bytes of information
M$$CRX          ; External MCR functions
M$$DIS          ; Seconds to wait for disconnect to occur
M$$EIS          ; Extend instruction set support
M$$EXT          ; Extended memory support
M$$FCS          ; FCS/file system support
M$$K11          ; MK11 MOS ECC memory is a possibility
M$$L11          ; ML11 memory disk controllers
M$$MGE          ; Memory management support
M$$MUP          ; Multi-user protection
M$$NET          ; DECnet support - requires S$$WST
M$$OVR          ; Overlayed MCR
M$$PRO          ; Multiprocessor support
M$$XLN          ; Total length of MCR lines
N$$DIR          ; Named directory support
N$$LDV          ; Null device
N$$MOV          ; Size of BLXIO move table
N$$UMR          ; Number of bytes of statically allocated UMRS
N$$VRC          ; Ticks per NVR update cycle (for PRO)
O$$LAP          ; Overlapped device operation support
P$$BPR          ; PMT: Pool base priority task control
P$$CTL          ; Pool monitoring task support
P$$D70          ; 11/70 or 11/60 cache parity support
P$$FRS          ; PMT: Lowest permissible size of largest pool fragment
P$$GEN          ; Pregenned system
P$$GMX          ; Get mapping context - requires P$$LAS
P$$HIL          ; PMT: High pool limit
P$$LAS          ; Program logical address extentions
P$$LOL          ; PMT: Low pool limit
P$$MAX          ; Maximum size of send/receive packets
P$$MON          ; SPM-11 support
P$$NIC          ; CSR address of panic dump device
P$$OFF          ; Parent/Offspring tasking support
P$$OOL          ; Secondary pool
P$$P11          ; PC11 paper tape punch
P$$P45          ; Rotating pattern in data lights
P$$R11          ; PR11 paper tape reader plus any PC11 readers
P$$RFL          ; Power fail recovery support
P$$RTY          ; Parity memory support
P$$SRF          ; Send/Receive by reference - requires P$$LAS
P$$WND          ; Secondary pool FCP - requires P$$OOL
P$$WRD          ; Include $PTWRD code
Q$$CRC          ; DQ11 CRC option support
Q$$HPT          ; DQ11 protocol option support
Q$$MGR          ; Queue manager support
Q$$OPT          ; Number of pre-allocate I/O packets
R$$11M          ; RSX-11M system (as opposed to 11D or IAS)
R$$11S          ; RSX-11S system
R$$611          ; RK611/RK711 disk controllers
R$$6OF          ; RK06 offset recovery support
R$$AMD          ; Auto mount/dismount support
R$$CON          ; Reconfiguration support
R$$DER          ; CORAL deallocation error checking
R$$DSP          ; Executive level dispatching
R$$EIS          ; EIS instructions - required for DECNET support
R$$EXV          ; Extend executive to 20K
R$$F11          ; RF11 fixed head disk controllers
R$$FEA          ; Test Feature Mask directive (FEAT$)
R$$FRK          ; Catch double forks
R$$GIN          ; General Information directive (GIN$)
R$$H11          ; RH controllers
R$$HDV          ; RH driver used
R$$IIC          ; Internal I/O completion - required for T$$TSA, D$$CHE
R$$JP1          ; RJ/RWP04-05-06 disk controllers
R$$JPO          ; RP04/05/06 offset recovery support
R$$JS1          ; RJ/RWS03-04 disk controllers
R$$K11          ; RK11 disk controllers
R$$K11          ; RK11 RK05 disk controllers
R$$L11          ; RL11/RLV11 Disk Cartridge controllers
R$$LKL          ; RMS record locking and place Ctl.
R$$M11          ; RJ/RWM03 disk controllers
R$$MIC          ; Micro/RSX system
R$$MOF          ; RM03 offset recovery support
R$$MPL          ; RSX-11M-PLUS system
R$$MYA          ; TMSCP-class tape controllers
R$$NDC          ; Round robin sched: Clock ticks per scheduling interval
R$$NDH          ; Round robin sched: Highest priority class to consider
R$$NDL          ; Round robin sched: Lowest priority class to consider
R$$P11          ; RP11-C/E disk controllers
R$$POI          ; Request and pass offspring info
R$$PRO          ; P/OS system
R$$RSV          ; Check registers on return from interrupt service routine
R$$SND          ; Receive/Send directives
R$$TPR          ; Processor type (for NETGEN)
R$$UDA          ; MSCP-class disk controllers
R$$UDA          ; UDA disk controller
R$$WPT          ; Watcher location
R$$X11          ; RX11 disk controllers
R$$X21          ; RX211/RXV21 disk controllers
S$$ECC          ; Shared Exec ECC support
S$$EXC          ; Full-functionality Exec
S$$HDW          ; Shadow recording
S$$HFC          ; Minimum time interval between shuffler requests
S$$IEN          ; Clock parameter, set by Exec
S$$LDC          ; Clock parameter, set by Exec
S$$LIB          ; Supervisor-mode library support
S$$MAP          ; SMAP$ and MVTS$ directives
S$$NM1          ; First 2 chars of system name
S$$NM2          ; Second 2 chars of system name
S$$NM3          ; Third 2 chars of system name
S$$OPT          ; Disk seek optimization
S$$RTZ          ; Clock parameter, set by Exec
S$$SPA          ; Constant, set by Exec
S$$SPC          ; Constant, set by Exec
S$$TIM          ; Set system time directive
S$$TOP          ; Stop bit directives
S$$TPS          ; Clock parameter, set by Exec
S$$WLK          ; Software writelock support
S$$WPC          ; Clock ticks per swapping interval
S$$WPR          ; Swapping priority
S$$WRG          ; Console switch register present
S$$WST          ; Switch State directive (SWST$)
S$$YDF          ;
S$$YSZ          ; Size of phys. memory in 32W blocks
S$$YSZ          ; Size of physical memory in 32W blocks
T$$30P          ; LA30P support
T$$A11          ; TA11 dual cassettes
T$$ACD          ; Ancillary control driver support in TTDRV - requires T$$EIO
T$$ACR          ; Automatic CR/LF
T$$BFL          ; Typeahead buffer length - also length
T$$BTW          ; Breakthrough write - required for M$$MUP
T$$BUF          ; Buffered term i/o; ckp during input
T$$C11          ; TC11 DECtape controllers
T$$CCA          ; Unsolicited input AST
T$$CCO          ; Write with Control/O cancellation
T$$COM          ; Separate terminal buffer pool
T$$CON          ; Serial console support
T$$CPW          ; Full duplex terminal driver
T$$CTR          ; Control/R support
T$$CTX          ; ^X flushes typeahead
T$$CUP          ; Device independent cursor positioning
T$$DMA          ; IO.WAL from a task buffer for I/D-space systems
T$$EIO          ; Extended I/O function support
T$$ESC          ; Escape sequence support
T$$GMC          ; Get terminal characteristics
T$$GTS          ; Get terminal driver support
T$$HFF          ; LA180S terminal support
T$$HLD          ; Hold screen mode
T$$ICS          ; Input count state recognition
T$$J16          ; TM02/03 magtape controllers
T$$KMG          ; Task termination/device not ready messages
T$$LTH          ; LAT support
T$$LWC          ; Settable case conversion (lowercase)
T$$M03          ; TM02/03 magtape formatters
T$$M11          ; TM/TMA/TMB11 magtape controllers
T$$M78          ; TU78 magtape controllers
T$$MHU          ; Modem hang-up notification AST
T$$MIN          ; Baseline terminal driver
T$$MOD          ; Modem support       ( D$$M11!D$$ZMD!D$$LMD!D$$VMD )
T$$MUX          ; Multiplexer support ( D$$H11!D$$J11!D$$Z11!D$$V11 )
T$$ONI          ; Overlaid/non-I/D Driver
T$$OOB          ; Out-of-band character handling
T$$OVL          ; Overlaid driver (uses TTEXT)
T$$RED          ; Hardware receive error support
T$$RNE          ; Read with no echo - required for M$$MUP
T$$RPR          ; Read after prompt
T$$RST          ; Read with special terminator - required for M$$MUP
T$$RUB          ; Crt rubout support
T$$S11          ; TS11/TU80/TSV05/TK25 controllers
T$$SCA          ; Switch character recognition
T$$SER          ; Serial command processing (CLI TABUF)
T$$SMC          ; Set terminal characteristics
T$$SPC          ; Use secondary pool CLI command buffers
T$$SPL          ; Use secondary pool for UCBX and tabuf
T$$SYN          ; Terminal-host synchronization
T$$TRW          ; Transparent read/write
T$$TSA          ; Network command terminal support
T$$U58          ; TU58 controllers
T$$UMR          ; Establish unibus mapping to TTDRV
T$$USP          ; User-written ports
T$$UTB          ; User terminal input buffering
T$$UTO          ; Time-out on unsolicited input
T$$UXL          ; UCB extension length
T$$VBF          ; Variable length input buffering
U$$ACH          ; Number of channels per module
U$$ADM          ; ADU01/IAD-IA analog input
U$$AOM          ; Analog output
U$$CIM          ; Digital interrupt
U$$CSM          ; Digital sense
U$$D11          ; UDC11 universal digital controller
U$$DAS          ; User data space support
U$$LTM          ; Bi-stable output
U$$MHI          ; High 2 bits of 18 bit UNIBUS address in bits 4 and 5
U$$MLO          ; Low 16 bits of 18 bit UNIBUS address
U$$MRN          ; Address of first free UMR
U$$NCT          ; DEUNA Ethernet controllers
U$$NIP          ; AR11 uni-polar A/D sampling
U$$NPC          ; DEUNA - Number of ports per controller
U$$NRS          ; DEUNA - Number of receive ring entries
U$$NTS          ; DEUNA - Number of transmit ring entries
U$$SSM          ; Single shot output
U$$TIM          ; I/O counter
U$$UMD          ; User mode diagnostics support
U$$UMR          ; UMR support (as separate from M$$EXT)
V$$CTR          ; Address of highest vector + 4
V$$RSN          ; RSX version
V$$S2S          ; VS60 drives 2 CRT monitors
V$$S60          ; VS60 graphics display subsystem
V$$T11          ; VT11 graphics display subsystem
V$$TLD          ; Default VT: unit buffer size
V$$TLM          ; Maximum VT: unit buffer size
V$$TRM          ; Virtual terminal support
X$$ACC          ; Define all extended accounting
X$$DBT          ; Executive debugging tool
X$$DXD          ; Incorporate loadable XDT hooks
X$$HDR          ; External header support
X$$M11          ; DMC11/DMR11 line interfaces
X$$SEC          ; Extensible secondary pool
XA$$xx          ; Extended Accounting subfunctions
xx$$CD          ; xx crash driver selected
