This is an update to the program BRUDIR. It has been modified to allow for MCR 
and DCL input type calls. Also a spooling and rewind switch has been added. If 
the -rewind switch is used then the progran will not look for the volume header 
which is normally found as the first record of a tape. This was done so that one
could position a tape to a BRU dataset and do a directory of that data set 
rather than doing the whole tape set. A copy of the backup command file that We 
use to backup our disk is included to show how the BRUDIR may be used to do a
directory of an incremental backup set. The other programs to manuplate the 
Mag-tape are in other UIC's on the distribution tape. You need POS and REC to 
position the magtape for the directory process.

To run the program:
	run brudir

It will prompt for the proper info or one may place it all on one line.


See the source listing for further information on the program.

Sorry, the program will only built on I/D Space machines. You will have to
write an overlay file if you intend to use it elsewhere.

		Dan L. Eisner
		Perkin-Elmer Corporation
		Applied Optics Operation
		Garden Grove, California
		714-895-1667
