This is file
RECFIL.TXT
 
RECFIL is a somewhat improved version of UICREC combined
with LAZRUS from [307,22] of RSX Spring 80 tape. Date selection
and command input is included. Switches and usage is described in
 
RECFIL.HLP
 
which can be used with the RSX11M help facilty. The distributed
OBJ files are for IAS only!(There is a difference concerning the
length of the DPB's of the QIO between IAS which has variable
length and RSX, which has fixed length).
 
 
Installation:
 
Assembly:	@RECFILASM
		(Should have SUPER.MAC in your RSXMAC.SML)
		(You should reassemble for RSX11M, OBJ's are for IAS!)
Task built:	IAS:	@RFILIAS
		RSX11M:	@RFIL11M
 
Specials for IAS:
 
If you want to create a multiuser version of the program
you have to edit the sources
RECFIL,CMDINP,BLOCKN,CNVDAT
and to change the line P$SECT=0 to 1
before assembly.
 
Use TKB @RCFIASMU.CMD. This binds also to SYSRES. But the task is not
privileged. It could therefore only be used on FOREIGN mounted
volumes. To remove this restriction patch the task header with ZAP
	ZAP
	ZAP>RECFIL.TSK/AB
	_0:10/20100 TO 20300		(200 is privileged)
	_X
 
This lengthy procedure is necessary because the IAS-TKB doesn't
have the /PR:0 switch like RSX11M. this means that at INSstall time
IAS still maps parts of the SCOM to the task(APR 4,5), although
we don't like it. The APR 6,7 are used by SYSRES and the readonly
part of the task.
 
For IAS which doesn't have BRU till now one can also do some
incremental backup. E.g.
	RCF>DK3:=DR:/GR/AF:20-DEC-80
collects all files after created from that date on with owner
UICs [g,*] and writes them to the corresponding UICs on DK3,
if one has logged on under [g,s], s means one single owner
in that group.
 
 
9-FEB-81	O.Titze, Kernphysik THD
			 D-6100 Darmstadt, W. Germany
			 
