		TEM - Installation Guide and Release Notes

	The TEM distribution occupies about 860 blocks in directory
	[10,10]. The ".TEM" files must be moved to LB:[1,5] unless you
	modify TEM or define TEM$DIRECTORY to point somewhere else; the
	other files can go anywhere you want. The only file required on
	the running system is TEM.TSK. The ".TEM" files are included as
	samples only.

	The TEM distribution contains the following files:

	   README.1ST	- A "text file" version of TEMABS.RNO.
	   README.2ND	- This text file.
	   TEM.COM	- A "Shell" for TEM.CMD, for VMS users.
	   TEM.CMD	- A command file to assemble and taskbuild TEM.
	   TEMBLD.CMD	- Taskbuild command file for TEM.
	   TEMRUN.CMD	- A sample command file used to drive TEM.
	   TEM.MAC	- Source for TEM.
	   TEM.RNO	- User's manual for TEM (*)
	   TEM11S.CMD	- Taskbuild command file for 11S version of TEM.
	   TEMABS.RNO	- "Thumbnail description" of TEM. (*)
	   HAYINI.TEM	- Sample setup file for a HAYES Smartmodem 1200.
	   HAYKIL.BIN	- Sample shutdown file for HAYES Smartmodem.
	   NL0INI.TEM	- Setup file for use with null device.
	   TEMACT.TEM	- Sample accounting information log. (*)
	   TT7INI.TEM	- Sample setup file. Uses HAYESINI.TEM.
	   TT7KIL.TEM	- Sample shutdown file. Uses HAYESKIL.TEM.
	   TEM.TSK	- Pre-built task image.
	   TEM32.TSK	- Pre-built task image for M V3.2. (*)
	   TEM.TXT	- User's manual for TEM, in text format.

		* - These files are not on the RX01 distribution.

	The installation procedure is:

	     1)	Copy all files on the distribution to your desired UIC.

	     2)	Make TEM.TSK contiguous, if needed.

	     3)	Create HAYKIL.TEM by the following procedure:
		    >RUN TEM
		    TEM>NL:/SE:NL:/LO:HAYKIL.TEM/-EO/TE/EC/CO/EX/-LI
		    TEM>^Z
		    >PIP HAYKIL.TEM/EOF:1:0
		    >PIP HAYKIL.TEM/AP=HAYKIL.BIN
		You can now delete HAYKIL.BIN, if you want.

	     4) Create directory [1,5] on LB0:, OR create system logical
		name TEM$DIRECTORY to point to your desired TEM home
		directory. If you do not wish to use the logical name
		TEM$DIRECTORY and you wish to use a directory OTHER
		than LB:[1,5] as your tem home directort, rebuild TEM
		using @TEM.

	     5)	Copy *.TEM from the installation UIC to the TEM home
		directory.

	     6)	Install TEM if desired.

	The pre-built task image has all defaults as described in the
	manual. It is not mapped to any library, and occupies about
	16KW. If you wish to map TEM to a resident FCS library, make
	suitable modifications to TEMBLD.CMD and retaskbuild. If you
	wish to modify the switch defaults, see the user's manual, and
	rebuild using
		>@TEM

	It MAY be possible to build TEM to run under RSX-11M V3.2 and
	RSX-11M+ V1.0, if your system has the full-duplex TT: driver
	with the usual SYSgen options. You must reassemble and rebuild
	TEM on a supported system (ie: M+ V2.0 and up, or M V4.0 and
	up), using the TEMBLD command file, and answering the questions
	appropriately. One person has done this OK, but I can't
	guarantee that it will continue to work.
