 BRU [qualifiers] file(s)

 Qualifiers:
 /COPY	(default) copy files to disk
 /LIST[=filespec] makes listing of backup set, implies /NOCOPY
 /LOG
 /REWIND rewind tape before operation
 /TOTAL  (default) lists/logs total number of files processed / total blocks
 /SELECT=(File[,File[,...]])
 /EXCLUDE=(File[,File[,...]])
	* and % wildcard allowed
	Specify directories with leading zeroes and without ","
	Example: /SELECT=[002005]*.*   copies all files from [2,5]
 /HELP   types this file to the screen

 Parameter: TAPE
 File Specification of tape or TPC copy of tape and backup_set label(s)
	 specify [device name:][Backup_set-label][,Backup_set-label]
    Defaults 	   Device name:		MUA0:
		   Backup_set-label:	the first label
    (No wildcards allowed for Backup_set-label !!!)
*** Note: BRUread automatically creates subdirectories for save-set name
    and directory name.    Example:   [.RSXMPL.001054] for [1,54] from RSXMPL
    If the directories already exist, they should be empty. (At least,
    the created files must not already exist. 
    BRU replaces files that already exists!!!

 Tape must be mounted /FOREIGN!
