110757     DACON: D/A Conversions Package for Use with AAV11-C and
KWV11-C  Version: V1.0, August 1984
 
Submitted by: G. C. Scott
 
Operating System: RT-11SJ V4.0  Source Language: FORTRAN IV, MACRO-11
Memory Required: 4.928KW  Hardware Required: AAV11-C
digital-to-analog-conversion pc board, KWV11-C programmable realtime
clock pc board.  Keywords: Conversions - Analog/Digital
 
Abstract: DACON is a software package which can be used with
Digital Equipment Corporation's AAV11-C
digital-to-analog conversion and KWV11-C programmable
realtime clock boards. The characteristics of this
software package include:
 
. D/A conversion from 4 differential digital input
  channels
. Up to 1 KHz sampling rate
. 12 bit data resolution
. DC offset corrections and calibrations of the data
 
The package includes the following:
 
. DY1:DOCD.TXT, user instructions and programming
  example
. DY1:DACONF.FOR, a FORTRAN IV program which sets up
  for the D/A conversions and performs corrections and
  calibrations of the input digital data
. DY1:DACONM.MAC, a MACRO-11 program which controls
  the D/A conversions
. Listing files for the above FORTRAN IV and MACRO-11
  programs
 
Error checking is performed throughout DY1:DACONF.FOR
and DY1:DACONM.MAC. Suggestions for software and
hardware setup are included for users who require more
customized A/D conversion schemes.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
