110925     DECnet/RSX Utilities  Version: 1.0, February 1990
 
Submitted by: Digital Equipment Corporation
 
Operating System: Micro/RSX, RSX-11M, RSX-11M-PLUS, RSX-11S  Source
Language: MACRO-11  Software Required: DECnet/RSX  Keywords:
Networking, Utilities - RSX-11
 
Abstract: The DECnet/RSX Utilities package includes:
 
. RSX-to-VMS, RSX-to-RSTS, and RSX-to-TOPS-20 terminal
  communications utilities (RVT, RRS, HOST, respectively).
  They provide functions similar to those of RMT, the
  RSX-to-RSX terminal communications utility, which predates
  the current SET HOST functionality.
. The CEDUMP utility compiles and analyzes information from
  the active network Communications Executive, DECnet,
  and/or PSI databases.
. The Poor Mans Routing utility, PMR, supports the
  passthrough protocol.  Connect information and all data
  passed can be written into a file with the PMR logging
  facility.
. The remote task utilities (RNT, ANT, and CNT) are used to
  run, abort, and cancel tasks on remote nodes.
. The Transport trace utility, TRC, logs all messages sent
  or received by the local node.  TRC will print a
  human-readable form of the trace in real-time or write the
  messages to a file in binary format for later analysis by
  the trace analyzer utility, ANA.
. The RMDemo utility is built with two additional network
  display pages.
. The virtual device server utilities allow a local user to
  set up virtual devices (disk, magnetic tape, or printer)
  on a remote system.  The virtual device host utilities
  allow a remote user to set up virtual devices on the local
  system.
 
Notes: Executable and/or object code is included.
 
Changes and Improvements: Fixed problem which caused system crash on
RSX-11M systems.
 
Media (Service Charge Code): 600' Magnetic Tape (MC)  Format: BRU
 
 
