PRO163     PROPLOT  Version: 3.1, December 1987
 
Submitted by: Ronald Getts, BFGoodrich R&D, Brecksville, OH
 
Operating System: P/OS V2.0A  Source Language: FORTRAN 77  Memory
Required: Standard  Hardware Required: LA50 or LVP16 (HP7475 or
HP7470) if hard copy desired. EBO and color monitor helpful, but not
required.  Keywords: Graphics, Plotting
 
Abstract: This diskette contains software developed at BFGoodrich R&D
in Brecksville, OH, for the PRO-350.
 
PROPLOT does least squares curve fitting to polynomial
equations, graphs the resulting curves on the monitor, and
has provisions for hard copy to an LA50, LA100 or Digital
Equipment Corporation (HP) two or six pen plotter.
 
PROPLOT V3.1 automatically supports color monitor and/or
HP7475, HP7470, HP7440 or Digital Equipment Corporation LVP16
plotters, if present.  This provides color graphics support.
 
Data can be input from the keyboard or from a data file.
The program asks the user questions regarding parameters
and allows creation of data files for later recall.  Scaling
is automatic or controlled by the user.
 
PROPLOT V3.1 supports .CTL file for repetitive
re-plotting of same data sets.  The .CTL file contains the
answers to the questions PROPLOT asks. See CTL.DOC for
details.
 
Changes and Improvements: Control files, additional plotter support.
 
Restrictions: Operating System P/OS V2.0 or later is required.
 
Media (Service Charge Code): User's Manual (EA), One RX50 Diskette
(JA)  Format: FILES-11
 
 
