PRO149      CAMERA - Test of a Hamamatsu C1000 Camera on the PRO's RTI
 Version: V1.0, December 1985
 
Submitted by: R. J. Wilden, Philips GmbH  Forschungslab.Aachen,
Postfach 1980, West Germany 51 Aachen
 
Operating System: P/OS V1.7A  Source Language: FORTRAN 77  Memory
Required: 512MB  Software Required: PRO/Toolkit, PRTIL  Hardware
Required: PRTI, Hamamatsu C1000 Camera  Keywords: Utilities - P/OS
 
Abstract: The task CAMTS1 provides a menu from which you can select
tests to check all functions of the C1000 camera.  The data
acquisition task CAMTST allows you to input video data to a
diskfile.  The camera must be connected to the RTI with the
IEEE-488 interface.
 
The tasks and all subroutines needed are written in
FORTRAN 77.  They work well with P/OS V1.7A; later releases
are supposed to function too.  Sources are included.
 
All action needed to start the tasks can be found in the two
indirect command-files CAMTS1RUN.CMD and CAMTSTRUN.CMD.  One
point is important; if you use the PRTI-Software V2.0, you
must change the RTI-Driver name from HG1.0 to HG1.A in the
indirect command-files mentioned.
 
Media (Service Charge Code): One RX50 Diskette (JA)  Format: FILES-11
 
 
