110520     ASM65: Cross Assembler for the 6502 Microprocessor
Version: June 1983
 
Submitted by: Eben Gay
 
Operating System: RT-11 V4.0, V5.0  Source Language: MACRO-11  Memory
Required: 28KW  Keywords: Cross-Assemblers, Microprocessors
 
Abstract: This is a debugged and slightly extended version of
ASM65. ASM65 is a simple cross-assembler for the 6502
microprocessor. It has no macro or conditional assembly
capability. It accepts source code in a form consistant
with most 6502 resident assemblers, and produces both a
listing with symbol table and object code in the paper
tape format used by the single board (SYM,AIM) 6502
computers. These are ASCII records designed to be
directly downloaded to the object computer on a serial
interface.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
