11S097 Nashville Spring 1987 RT SIG Tape

                   SPRING, 1987, RT SIG TAPE DIRECTORY






                  Summary of the Spring, 1987, RT-11 SIG Tape



         SIG tape copy instructions  . . . . . . . . . . . . . . . . .  1

         VIRTUL - Subdevice retriever for RSTS . . . . . . . . . . . .  2

         DIRTWO - Annotated tape directories, part 2 . . . . . . . . .  3

         WSHLST - RT-11 Wish List Survey . . . . . . . . . . . . . . .  4

         FONT - Downloadable VT-200 character font . . . . . . . . . .  5

         SPELL  - Spelling Checker with Dictionary . . . . . . . . . .  5

         CALEND - Calendar Display Program . . . . . . . . . . . . . .  5

         DFIND - Subdevice Directory Program . . . . . . . . . . . . .  6

         RDMF77 - Directory and Other Utilities  . . . . . . . . . . .  7

         MAIL - On-Line Message Facility for TSX+  . . . . . . . . . .  8

         TAPE - Tape Utilities . . . . . . . . . . . . . . . . . . . .  8

         ACODES - On-Line Telephone Area Codes Retriever . . . . . . .  9

         TIMING - RT-11/TSX+ System Timing Studies . . . . . . . . . . 10

         TSXLIB - Fortran-Callable TSX+ EMT's  . . . . . . . . . . . . 11

         DROIDS - The new Game Sensation . . . . . . . . . . . . . . . 12

         UCLPLS - User Command Language (UCL) Program  . . . . . . . . 13

         PM - RT-11 Monitor Prompt Handleroid  . . . . . . . . . . . . 13

         PLT - File-Oriented Plotting Utility for RT . . . . . . . . . 14

         FLXIND - IND Control Files for FLECS Processing . . . . . . . 15

         F77IND - IND Control Files for Fortran-77 Compilations  . . . 15

         BAKALL - IND Control File to Automate Backups . . . . . . . . 16

         THESIS - RUNOFF Macros for Formatting a Thesis  . . . . . . . 17



                                        i  



                   SPRING, 1987, RT SIG TAPE DIRECTORY


         GKS - RT-11 Implementation of GKS Plotting Standard . . . . . 18

         INDFIL - IND Control Files for Subdevices . . . . . . . . . . 19

         DIAL - Terminal Emulator Front End  . . . . . . . . . . . . . 20

         KERMIT - File transfer protocol for PDP-11's  . . . . . . . . 21

         Tape Distribution Information . . . . . . . . . . . . . . . . 22

         Cross-Reference Index . . . . . . . . . . . . . . . . . . . . 23











































                                        ii 






        *************************************************************

                         DECUS Symposium RT-11 SIG Tape

                                  Spring, 1987
                                  Nashville, TN

                               Annotated Directory

        *************************************************************

                                    IMPORTANT
                                 NEW INFORMATION

        Subdevice files on this tape are now allowed to be as large as
        800 blocks (the size of a RX-50).  (For the sake of convenience,
        the data files for the TIMING submission are in slightly larger
        subdevices).  This improves efficiency.  If you need to copy a
        file larger than 494 blocks to a RX01, use the COPY/MULTIVOLUME
        command.

        Read the file TAPCOP.TXT if you need SIG Tape copy instructions
        or information for retrieving files using RT-11 version 4, or
        RSTS.


        If you have any comments, corrections or contentions with any of
        the submissions on this tape, please discuss them directly with
        the authors.




                  ****************************************
                  * Please look at the WSHLST submission *
                  *          and respond to it!          *
                  ****************************************




        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 2


        VIRTUL - Subdevice retriever for RSTS.

        E.F.Beadel, Jr., Manager
        CAUSE Instructional Computer Center
        SUNY at Oswego
        Oswego, NY 13126
        (315) 341-3055

             This program allows RSTS/E users to break down the subdevice
        files from this tape after they have been copied to disk.  It has
        been modified by David Smith, Galileo Computer Center, to remove
        a few bugs and to be able to read multi-segment directories.  See
        TAPCOP.TXT for details.

        VIRTUL.BAS   1 File,   43 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 3


        DIRTWO - Annotated tape directories, part 2.

        R. W. Barnard
        Sandia National Laboratories
        Minicomputer Software Division 7523
        P. O. Box 5800
        Albuquerque, NM 87185
        (505) 844-5115

             DIRTWO contains annotated directories of the DECUS Symposia
        RT-11 tapes from the Fall of 1981 through the Fall of 1986.  The
        most recent SIG tape on which the directory of previous tapes is
        located is the Spring, 1985, and is called DIR1.DSK.

        DIRTWO.DSK  11 Files, 558 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 4


        WSHLST - RT-11 Wish List Survey.

        Robert Walraven
        Multiware, Inc.
        2121-B Second Street, Suite 107
        Davis, CA 95616
        (916) 756-3291

             The RT-11 SIG is very interested in your responses to the
        wish list items contained in WSHLST.  From your responses will be
        determined some of the new features of RT-11.  Please take the
        time to review and respond to this submission.

        WSHLST.DSK   2 Files, 101 Blocks
        ***************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 5


        FONT - Downloadable VT-200 character font.
        SPELL  - Spelling-Checker with Dictionary.
        CALEND - Calendar Display Program.

        Harold Z. Bencowitz
        810 Hospital Drive, Suite 240
        Beaumont, Texas 77701
        (409) 835-3770

             FONT is a program written in Whitesmith's C to allow one to
        easily create or alter downloadable fonts/character sets for
        VT200 series terminals. It can be used to edit a previous
        character set (stored as a disk file). One character at a time is
        edited while each pixel change is observed both at the normal
        size and double high/double wide.

             CALEND is a program written in Whitesmith's C to display the
        calender for a selected month. It will accept any month and year
        from 1583 - 32000.

             SPELL is a spelling checker written in Whitesmith's C. 
        Words in the input file are compared to one or more dictionaries
        (files of alphabetized words) and an alphabetized list of the
        unmatched words is sent to the output file(s).  The output list
        can include each word as many times as it is used or optionally
        only once.

             The file README.1st and the common files are contained in
        the VTFONT.DSK file.

        VTFONT.DSK  12 Files, 406 Blocks
        CALEND.DSK   3 Files,  50 Blocks
        SPELLR.DSK   6 Files, 475 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 6


        DFIND - Subdevice Directory Program.

        Carl Lowenstein
        U. C. San Diego
        Marine Physical Lab, P-004
        La Jolla, CA 92093

             DFIND is a utility for searching through an RT-11 structured
        file system and the subdevices on it.  Upon a successful match,
        the filename, size, and date are printed, as well as the file
        path (sequence of subdevices) leading up to it.

        DFIND0.DSK   7 Files, 122 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 7


        RDMF77 - Directory and Other Utilities.

        Walt Shpuntoff
        Institute for Resource Management, Inc.
        PO Box 869
        Arnold, MD 21012
        (301) 757-6503

             This submission provides Fortran-77 interface subroutines
        that make it possible to read and write RDM database file records
        from an F77 application.   The routines allow you to retrieve and
        write back out active records, convert dates to and from RDM
        format, and open and close RDM files.

        (RDM is a trademark of Interactive Technology, Inc.)

        RDMF77.DSK  18 Files, 154 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 8


        MAIL - On-Line Message Facility for TSX+.
        TAPE - Tape Utilities.

        Mike Marak, David Gaudine, Dr. S. J. Kubina
        EMC Lab, Room AD-532
        Loyola Campus
        Concordia University
        7141 Sherbrooke St. W.
        Montreal, Que. H4B 1R6
        Canada
        (514) 848-3118

             MAIL is on online message sending system which allows users
        to send messages to other users and to read messages that have
        been sent to them.  It is designed to run under TSX-PLUS.  Mail
        can be run from a logon command file or as a keyboard command. 
        The system consists of a common file that contains the list of
        current users and any messages for each user, a maintenance
        program that allows the postmaster to maintain the mail file, and
        a MAIL utility which allows users to read, delete, or send mail
        to another user.  A system command file is used to tell the
        utility program if MAIL has been invoked from LOGON or by the
        user.

             The programs TAPE%% are utilities to back up specific disk
        devices to magtape.  TAPERK backs up 4800-block devices (RK05's),
        TAPEDL does RL02's, and TAPEDU does RD52's.  Once a disk is
        backed up by these utilities it can easily be restored; in
        addition, the directory name can also be changed.  Individual
        files from the backup can be retreived.  These programs run under
        TSX+; they are too big to run under RT, but may work using
        VBGEXE.  This submission also includes ANSIR and ANSIW, for
        reading and writing unlabelled ANSI magnetic tapes, and T20IBM,
        for reading EBCIDIC IBM tapes.

        TAPUTL.DSK  10 Files, 500 Blocks
        MAILUT.DSK  10 Files, 289 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 9


        ACODES - On-Line Telephone Area Codes Retriever.

        Bill Leroy
        The Software House, Inc.
        P. O. Box 52661
        Atlanta, GA 30355
        (404) 231-1484

             ACODES.TXT is a list of North American telephone area codes
        and major cities in those area codes.  It also lists FTS on-net
        to off-net phone numbers.  The file is accessed by means of the
        GREP program.  Combined with a UCL symbol, you can retrieve area
        codes by state or city, or retrieve all the area codes in a
        particular state.

             Editor's Note: In typical UNIX/C fashion, the documentation
        for GREP is so abysmal that most people will not be able to
        decipher it.  To implement an on-line retrieval of area codes,
        define the following UCL+ symbol:

        ACODES == r GREP\-f '^' SY:ACODES.TXT

        You can then type

        aco 505      to get the information about area code 505, or

        aco texas    to find out all the area codes in Texas, etc.

        ACODES.DSK   4 Files,  49 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 10


        TIMING - RT-11/TSX+ System Timing Studies.

        Jim Crapuchettes
        Omnex Corporation
        2483 Old Middlefield Way
        Mountain View, CA 94043
        (415) 966-8400

             This submission contains the data files generated for RT-11/
        TSX-Plus System Timing tests that were described in the session
        presented at the Spring, 1987, DECUS Symposium in Nashville TN. 
        It also includes files describing the test procedure and some
        data reduction programs.  These tests are to determine the
        EMT-level responses of RT-11 and TSX+, and include tests on 11/23
        and 11/73 processors, RT-11 SJ, FB and XM monitors and TSX+.

        TIMING.DSK  10 Files,  94 Blocks
        TMNG01.DAT  21 Files, 861 Blocks
        TMNG02.DAT  23 Files, 943 Blocks
        TMNG03.DAT  23 Files, 943 Blocks
        TMNG04.DAT  23 Files, 943 Blocks
        TMNG05.DAT  23 Files, 943 Blocks
        TMNG06.DAT  23 Files, 943 Blocks
        TMNG07.DAT  23 Files, 943 Blocks
        TMNG08.DAT  23 Files, 943 Blocks
        TMNG09.DAT  23 Files, 943 Blocks
        TMNG10.DAT  23 Files, 943 Blocks
        TMNG11.DAT   3 Files, 123 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 11


        TSXLIB - Fortran-Callable TSX+ EMT's.

        N. A. Bourgeois, Jr.
        NAB Software Services, Inc.
        P. O. Box 20009
        Albuquerque, NM 87154

             TSXLIB is a library of FORTRAN callable routines that
        implement the TSX-Plus system services which are unique to
        TSX-Plus.  The library has been updated to include all TSX-Plus
        unique services through TSX-Plus V6.2.  The TSXLIB distribution
        kit includes the MACRO-11 source modules for all the routines, a
        user's manual in machine readable form, an indirect command file
        to build the library, and the implemented library.

        TSXLB1.DSK   4 Files, 500 Blocks
        TSXLB2.DSK  12 Files, 448 Blocks
        *************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 12


        DROIDS - The new Game Sensation.

        Robert Walraven
        Multiware, Inc.
        2121-B Second Street, Suite 107
        Davis, CA 95616
        (916) 756-3291

             DROIDS is a game which pits your (or your kid's) skills
        against a planetfull of droids bent on your destruction.  Future
        Symposia will include sessions on current DROIDS strategy and
        reports on the current champion status as recorded in DROIDS.SCR.

        Note added in proof:
        It is necessary to SET TERM NOCRLF for proper operation of
        DROIDS.

        DROIDS.DSK   4 Files,  92 Blocks
        ***************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 13


        UCLPLS - User Command Language (UCL) Program.
        PM - RT-11 Monitor Prompt Handleroid.

        William K. Walker
        Monsanto Research Corp.
        P. O. Box 32
        MS  A-152
        Miamisburg, OH 45342
        (513) 865-3557

             UCL+ is upward-compatible with the UCL distributed with
        RT-11, Version 5.1B and later. The version submitted to this tape
        is V07.55 b, an update from all previous versions.  This version
        of UCL+ includes a fix of an obscure bug.  Otherwise it still
        includes all the extra features which make it so useful.

             PM is a RT-11 "handleroid" which permits user-defined KMON
        prompts (replacing the ".").  Read the documentation before using
        it!

        UCLPLS.DSK  22 Files, 698 Blocks
        PMHDLR.DSK   4 Files,  37 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 14


        PLT - File-Oriented Plotting Utility for RT.

        Peter E. Bodmer
        Boys' Town National Institute
        555 N. 30th
        Omaha, NE 68131
        (402) 449-6711

             PLT is a RT-11 program that translates a user-specified text
        file consisting of plotting commands into Tektronix 4662
        language.  The set of Tektronix 4662 language commands are placed
        into an output file which can then be sent directly to a
        Retro-Graphic terminal.  The output files or .TEK files can also
        be sent to a DataSouth Line Printer or to a HP 7475A pen plotter.
        The typical input to PLT is a standard ASCII text file that
        contains plotting parameters, keywords, data, and comments.  The
        user may obtain data from another program, or may call another
        text file as a virtual subroutine, or have PLT request
        parameter/data entry during execution.  PLT files may be created
        by entering the text into a file manually, using an editing
        program, or by writing and executing a program that creates,
        writes into, and closes the file.

        RTPLT1.DSK  11 Files, 540 Blocks
        RTPLT2.DSK  64 Files, 600 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 15


        FLXIND - IND Control Files for FLECS Processing.
        F77IND - IND Control Files for Fortran-77 Compilations.

        Edward L. Hendrickson
        258K Metals Development
        Ames Laboratory ISU/USDOE
        Ames, IA  50011
        (515) 294-3590

             FLECS.IND is an IND command file that automates the use of
        FLECS.  Without FLECS.IND the user must remember the FLECS
        command string syntax, then wait for the source to be translated
        to Fortran, then compile the .FTX (Fortran) code into object code
        using the correct Fortran command string syntax.  With FLECS.IND
        the user types one command string and the entire process is
        completed transparently.

             F77.IND is an IND command procedure that simulates all of
        the FORTRAN switches available.  F77.IND can either be used as a
        stand alone command procedure or as an /F77 switch with FLECS.IND
        file.  This also inlcudes a resubmission of the INDEX program.

             Compiler switches may go either before or after the file
        name; there is an on-line display of the F77.IND help
        documentation.

             If F77.IND is used as without FLECS, then there are 17
        switches available:

        /A*ssemblylist[=<filespec>]
                      -- Same as /L but with a listing of assembly code.
        /B*ounds      -- Checks for array references out of bounds.
        /C*ontinue=n  -- Sets the maximum number of continuation lines.
        /D*ebug       -- Lines with D in column 1 are compiled.
        /E*xtendlines -- Compiler interprets source text in cols 73-132
        /F*ulltrace   -- Generates very detailed traceback (see Trace)
        /L*ist[=<filespec>]
                      -- Creates a list file with source listing, program
                         section summary, and storage map.
        /Nos*wap      -- Inhibits swapping of USR over the program.
        /Noo*bject    -- Suppresses creation of an object file.
        /O*bject=<filespec>
                   -- Change the default device, name, and/or extension
                         of the object file.
        /R*ecordlength=n
                      -- Specifies the maximum record length (in bytes)
                         for run time I/O (4 < n < 4095).
        /S*tatistics  -- Produces a stat report.
        /T*race       -- Generates extra code for OTS error traceback.
        /U*nits=n     -- Sets the number of logical units available.
        /Wa*rnings    -- Enables printing of W-class warning diagnostics.
        /Wi*demap     -- Produces a 132-column map listing.
        /Wo*rkfile=n  -- Sets the length of the workfile in disk blocks.

        FLXIND.DSK  10 Files, 622 Blocks
        F77IND.DSK   4 Files,  76 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 16


        BAKALL - IND Control File to Automate Backups.

        Edward L. Hendrickson
        258K Metals Development
        Ames Laboratory ISU/USDOE
        Ames, IA  50011
        (515) 294-3590

        Paul Lustgraaf
        32 Carver Hall
        Iowa State University
        Ames, IA 50011
        (515) 294-1832

             BAKALL.IND is an IND command file that automates the backup
        process. It backs up a complete device to magnetic tape using the
        BACKUP/DEVICE command. The code currently keeps track of 5
        complete backup tape sets and 2 devices, DU0 and DU1.  BAKALL
        will open a LOG file and record all necessary data needed to
        document each individual tape.

             BUPRES is a FORTRAN IV program which reads individual files
        from a magnetic tape created by the RT-11 version 5 BACKUP
        command.  The program has been modified since it was originally
        submitted to the tape.  The DIR function has been changed so that
        it is compatible with the output from DIR/COL:1 which allows you
        to look for differences without restoring the whole volume.  The
        program now works directly with the magtape handler instead of
        using EXTMT.

        BAKALL.DSK   5 Files,  46 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 17


        THESIS - RUNOFF Macros for Formatting a Thesis.

        Mark M. Mehl
        Department of Biomedical Eng
        IOWA STATE UNIVERSITY (ISU)
        Ames, IA  50011

        ISU RNOTHESIS is a collection of Bonner Lab RUNOFF macro commands
        that can be used to format a thesis.  There are commands for
        generating floating tables and figures, in-line equation lists,
        footnotes, points, quotations, and a bibliography.  Although
        RNOTHESIS is being used to format theses according to the Iowa
        State University thesis office requirements, its macros can be
        adjusted to support any large document layout.

        THESIS.DSK  15 Files, 427 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 18


        GKS - RT-11 Implementation of GKS Plotting Standard.

        James V.  Flatten
        258I  Metals  Development
        Ames Laboratory, ISU/DOE
        Ames, IA  50011 

             This document describes an implementation of the Graphical
        Kernel System (GKS) for the RT-11 operating system running on a
        PDP-11 computer.  This implementation is the lowest level of GKS,
        which was chosen to keep the graphical subroutine library small
        and efficient for applications running under RT-11.  Three device
        drivers are provided for the HP7475 6 pen plotter, the Tektronix
        4107 color terminal and the Visual 550 terminal.  

        GKS020.DSK  20 Files, 560 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 19


        INDFIL - IND Control Files for Manipulating Subdevices.

        R. W. Barnard
        Sandia National Laboratories
        Division 7523
        P. O. Box 5800
        Albuquerque, NM 87185
        (505) 844-5115

             The following IND control files have been extensively
        updated since they were last included on the SIG Tape.

        DOWN and UP can be used to conveniently move among subdevices. 
        Using these facilities, you can have the equivalent of
        subdirectories on a VAX.  DOWN will mount a subdevice file using
        the Logical Disk handler and assign either the default or a
        user-selected logical name to that device.  If the device is not
        specified, DOWN will search through a predetermined list of
        devices to look for the file.  UP moves "up" one level of
        subdevice nesting.  DOWN uses PARSE, an IND procedure which is a
        comprehensive filespec parser.  It also uses the program READLD
        to determine the LD units currently associated with files, and
        the corresponding logical assignments.  HOME is a special case of
        UP which is implemented with a UCL+ symbol.  OVER is a UCL+
        symbol to move from one subdevice assignment to another.  CUR is
        a UCL+ symbol to report what your current subdevice assignment
        is.  The file UCL.UCJ provides UCL+ symbol definitions for DOWN,
        UP, HOME, OVER and CUR.

        NEWLD can be used to easily create a new file to be used as a
        subdevice.  NEWLD accepts the parameters file name, size, logical
        name, number of directory segments, and whether the file is to be
        "net" or "gross" size.  Defaults can be used for many of the
        parameters.  File sizes can be specified in either of two ways -
        as a numerical value or as a disk type (RX01, RX02, RX50, RL01,
        etc).

        INCBUP does incremental backups (i.e., backs up only files
        created since the previous backup) and catalogs the directories
        of the backed-up files for rapid retrieval.  Backups can be done
        from any size or type of disk (including LD's) to any other disk.
        The backup target device can be a subdevice file on a larger
        disk, thereby permitting several "backup sets" to be on one
        physical disk.  The volumes on which the backed-up files are
        copied are identified by a unique name and extension as the
        "backup set identifier".  A printed directory of the backed-up
        files is also made.  Backups of several devices can be done in
        one INCBUP "session".  You have the option to use the same
        parameters for subsequent backups.  File cataloging is done with
        the DSKLIB program.  This package has been included on previous
        tapes, such as the Fall, 1986 RT SIG tape.

        INDFIL.DSK  18 Files, 258 Blocks
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 20


        DIAL - Terminal Emulator Front End.

        Maarten van Swaay
        Kansas State University
        Department of Computer Science
        Nichols Hall, CS
        Manhattan, KS 66506

             DIAL is a package that can be used in front of terminal
        emulators. DIAL is designed to retrieve its input from a command
        file, which can direct it to initialize a HAYES-type modem and to
        penetrate through a layer of data switches, transport services,
        logon dialogs, etc.

        DIALER.DSK   3 Files,  38 Blocks
        *****************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 21


        KERMIT - File transfer protocol for PDP-11's.

        Brian Nelson
        Computer Services, University of Toledo
        2801 West Bancroft
        Toledo, OH 43606
        (419) 537-2841

             The Kermit files for RT-11 which are included on this tape
        have been taken from the Fall, 1986, SIG Tape.  This is not a new
        submission.

             This is release 2.44 of Kermit-11.  Major changes from
        previous versions include long packet support, BREAK and DTR
        control for RT, a DIAL command, and other small fix-ups.  It runs
        on all PDP-11 operating systems.  For RT-11, you must have
        multiterminal support if you are using version 4.0.  For RT
        version 5.1 and later, multiterminal support is not needed if you
        use the XL or XC handler.  For TSX+, you must use the CL facility
        for outgoing lines.  See the files K11AAA.AAA, and K11INS.DOC for
        more information.  Edit history is given in the file K11CMD.MAC.

        KERDC1.DSK   9 Files, 355 Blocks  (Documentation Files)
        KERDC2.DSK   5 Files, 428 Blocks  (Documentation Files)
        KERCM1.DSK  12 Files, 486 Blocks  (Common Files)
        KERCM2.DSK   6 Files, 486 Blocks  (Common Files)
        KERCM3.DSK  17 Files, 222 Blocks  (Common Files)
        KERRT1.DSK  18 Files, 380 Blocks  (RT Files)
        KERRT2.DSK   2 Files, 390 Blocks  (RT Files)
        ************************************************************



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 22


        The Spring, 1987, RT SIG tape contains 46 Files, 20417 Blocks.


        It was prepared by:

        R. W. Barnard
        Sandia National Laboratories
        Division 7523
        P. O. Box 5800
        Albuquerque, NM 87185

        DCS - BARNARD


        It is available from the following sources:

        DECUS NLO TAPE TREE            DECUS LIBRARY
        c/o Robert N. Perry
        Tektronix, Inc.                DECUS Program Library
        PO Box 500                     BP02
        MS: 19-333                     249 Northboro Road
        Beaverton, OR  97077           Marlboro, MA 01752
        (503) 527-5410

        DCS - PERRY

        Selected portions of the tape are usually available for
        downloading, but will not be so temporarily.  Please be patient.

        Host: Not Available
        Phone:        
        Logon/PW:     
        Available:    
        Protocol: KERMIT and VTCOM/TRANSF

        For more information on Electronic Distribution of the tape,
        please see the May, 1986, issue of the DECUS US Chapter SIGs
        Newsletter, in the RT-11 SIG section.


        File date: 4-June-1987
        Printing date: June 4, 1987



                   SPRING, 1987, RT SIG TAPE DIRECTORY              Page 23


                             Cross-Reference Index

         ACODES  . . . . . . . . . . . . . . . . . . . . . 9
         ANSIR - Read unlabelled ANSI tape . . . . . . . . 8
         ANSIW - Write unlabelled ANSI tape  . . . . . . . 8
         Archiving system  . . . . . . . . . . . . . . . . 16, 19
         Area Codes  . . . . . . . . . . . . . . . . . . . 9

         Backup utilities  . . . . . . . . . . . . . . . . 8, 16, 19
         BAKALL  . . . . . . . . . . . . . . . . . . . . . 16
         Barnard, R. W.  . . . . . . . . . . . . . . . . . 3, 19, 22
         Beadel, E. F., Jr.  . . . . . . . . . . . . . . . 2
         Bencowitz, H. . . . . . . . . . . . . . . . . . . 5
         Bodmer, P. E. . . . . . . . . . . . . . . . . . . 14
         Bonner Lab RUNOFF macros  . . . . . . . . . . . . 17
         Bourgeois, N. A.  . . . . . . . . . . . . . . . . 11
         BUPRES  . . . . . . . . . . . . . . . . . . . . . 16

         CALEND  . . . . . . . . . . . . . . . . . . . . . 5
         Calendar Display  . . . . . . . . . . . . . . . . 5
         Comparison of speed of 11/73 and 11/23  . . . . . 10
         Comparison of speeds of SJ, XM, TSX+  . . . . . . 10
         Crapuchettes, J.  . . . . . . . . . . . . . . . . 10

         Database interface  . . . . . . . . . . . . . . . 7
         DataSouth printer plotting routines . . . . . . . 14
         DECUS library . . . . . . . . . . . . . . . . . . 22
         Determine which LD's are mounted  . . . . . . . . 19
         DFIND . . . . . . . . . . . . . . . . . . . . . . 6
         DIAL  . . . . . . . . . . . . . . . . . . . . . . 20
         DIR1.DSK  . . . . . . . . . . . . . . . . . . . . 3
         Directory of older SIG tapes  . . . . . . . . . . 3
         Directory of recent SIG tapes . . . . . . . . . . 3
         Disk librarian  . . . . . . . . . . . . . . . . . 19
         DOWN - IND Control File . . . . . . . . . . . . . 19
         DROIDS  . . . . . . . . . . . . . . . . . . . . . 12

         Electronic distribution of the RT SIG Tape  . . . 22
         EMT execution speeds  . . . . . . . . . . . . . . 10

         F77.IND - Compiler file for Fortran-77  . . . . . 15
         File search utility . . . . . . . . . . . . . . . 6
         Flatten, J. V.  . . . . . . . . . . . . . . . . . 18
         FLX.IND - Compiler file for FLECS . . . . . . . . 15
         FONT  . . . . . . . . . . . . . . . . . . . . . . 5
         Fonts for VT-200  . . . . . . . . . . . . . . . . 5
         Formatting commands for a thesis  . . . . . . . . 17
         Fortran-77 compiler control file  . . . . . . . . 15
         Fortran-77 Interface to RDM . . . . . . . . . . . 7
         FTS phone numbers . . . . . . . . . . . . . . . . 9

         Games . . . . . . . . . . . . . . . . . . . . . . 12
         Gaudine, D. . . . . . . . . . . . . . . . . . . . 8
         GKS . . . . . . . . . . . . . . . . . . . . . . . 18




                   SPRING, 1987, RT SIG TAPE DIRECTORY               Page 24


         Handler . . . . . . . . . . . . . . . . . . . . . 13
         Hendrickson, E. L.  . . . . . . . . . . . . . . . 15, 16
         How to get the SIG Tape . . . . . . . . . . . . . 22
         HP-7475A plotter routines . . . . . . . . . . . . 14, 18

         INCBUP - IND Control File . . . . . . . . . . . . 19
         Incremental backup  . . . . . . . . . . . . . . . 19
         IND control files . . . . . . . . . . . . . . . . 15, 16, 19
         INDEX - cross-reference program . . . . . . . . . 15

         KERMIT File transfer protocol . . . . . . . . . . 21
         Kermit, Version 2.44  . . . . . . . . . . . . . . 21
         Kubina, S. J. . . . . . . . . . . . . . . . . . . 8

         Leroy, W. . . . . . . . . . . . . . . . . . . . . 9
         Lowenstein, C.  . . . . . . . . . . . . . . . . . 6
         Lustgraaf, P. . . . . . . . . . . . . . . . . . . 16

         Magtape backup for specific-sized devices . . . . 8
         Marak, M. P.  . . . . . . . . . . . . . . . . . . 8
         Mehl, M.  . . . . . . . . . . . . . . . . . . . . 17
         Modem control package . . . . . . . . . . . . . . 20
         Multiware, Inc. . . . . . . . . . . . . . . . . . 4, 12

         NAB Software Services, Inc. . . . . . . . . . . . 11
         Nelson, Brian . . . . . . . . . . . . . . . . . . 21

         Omnex, Inc. . . . . . . . . . . . . . . . . . . . 10
         On-line Area Code Retrieval . . . . . . . . . . . 9

         PARSE - IND Control File  . . . . . . . . . . . . 19
         Perry, Robert . . . . . . . . . . . . . . . . . . 22
         Plotting routine  . . . . . . . . . . . . . . . . 14, 18
         PLT . . . . . . . . . . . . . . . . . . . . . . . 14
         PM.SYS  . . . . . . . . . . . . . . . . . . . . . 13
         Prompt "handler"  . . . . . . . . . . . . . . . . 13

         RDMF77 - RDM Interface  . . . . . . . . . . . . . 7
         Read individual files from BUP tape . . . . . . . 16
         READLD - Determine which LD's are mounted . . . . 19
         Redefine the RT-11 prompt symbol  . . . . . . . . 13
         RSTS program for reading subdevices . . . . . . . 2
         RT-11 Wish list survey  . . . . . . . . . . . . . 4
         RT/TSX Kermit . . . . . . . . . . . . . . . . . . 21
         RUNOFF  . . . . . . . . . . . . . . . . . . . . . 17

         Search a volume and subdevices  . . . . . . . . . 6
         Shpuntoff, W. . . . . . . . . . . . . . . . . . . 7
         SIG Tape Directory, Fall, 81  . . . . . . . . . . 3
         SIG Tape Directory, Fall, 82  . . . . . . . . . . 3
         SIG Tape Directory, Fall, 83  . . . . . . . . . . 3
         SIG Tape Directory, Fall, 84  . . . . . . . . . . 3
         SIG Tape Directory, Fall, 85  . . . . . . . . . . 3
         SIG Tape Directory, Fall, 86  . . . . . . . . . . 3
         SIG Tape Directory, Spring, 82  . . . . . . . . . 3



                   SPRING, 1987, RT SIG TAPE DIRECTORY               Page 25


         SIG Tape Directory, Spring, 83  . . . . . . . . . 3
         SIG Tape Directory, Spring, 84  . . . . . . . . . 3
         SIG Tape Directory, Spring, 85  . . . . . . . . . 3
         SIG Tape Directory, Spring, 86  . . . . . . . . . 3
         SPELL . . . . . . . . . . . . . . . . . . . . . . 5
         Spelling Checker  . . . . . . . . . . . . . . . . 5
         Subdevice directory utility . . . . . . . . . . . 6
         Subdevice file utilities  . . . . . . . . . . . . 19

         T20IBM - Read unlabelled EBCIDIC tape . . . . . . 8
         TAPCOP.TXT  . . . . . . . . . . . . . . . . . . . 1, 2
         TAPEDL - Back up a RL02 device  . . . . . . . . . 8
         TAPEDU - Back up a RD52 device  . . . . . . . . . 8
         TAPERK - Back up a RK05 device  . . . . . . . . . 8
         Tektronix 4107 plotter routines . . . . . . . . . 18
         Tektronix 4662 plotter routines . . . . . . . . . 14
         Telephone Area Codes  . . . . . . . . . . . . . . 9
         Terminal emulator control package . . . . . . . . 20
         THESIS  . . . . . . . . . . . . . . . . . . . . . 17
         TIMING - system timing tests  . . . . . . . . . . 1, 10
         TSX+ System Services  . . . . . . . . . . . . . . 11
         TSX+ Utilities  . . . . . . . . . . . . . . . . . 8, 11, 13
         TSXLIB, Version 6.2 . . . . . . . . . . . . . . . 11

         UCL+, Version 7.55 b  . . . . . . . . . . . . . . 13
         UP - IND Control File . . . . . . . . . . . . . . 19

         Van Swaay, M. . . . . . . . . . . . . . . . . . . 20
         Visual 550 plotter routines . . . . . . . . . . . 18
         VT-200 Font Generator . . . . . . . . . . . . . . 5

         Walker, W.  . . . . . . . . . . . . . . . . . . . 13
         Walraven, R.  . . . . . . . . . . . . . . . . . . 4, 12
         WSHLST - Wish list survey . . . . . . . . . . . . 4

