110307     Stage 2 for the PDP-11 Operating under RT-11  Version:
September 1976
 
Author: W. M. Waite, Univ. of Colorado, Peter H. Heinrich, Univ. of
Karlsruhe
 
Submitted by: D. M. Nessett, Australian National University, Canberra,
Australia
 
Operating System: RT-11 V2B  Source Language: MACRO-11  Memory
Required: 16K (assuming the S/J monitor)  Hardware Required: PDP-11/20
+ EAE, PDP-11/40 + EIS or PDP-11/45  Keywords: MACRO, Utilities -
RT-11
 
Abstract: Stage 2 is a general purpose MACRO processor designed to
port software written for abstract machines. The MACRO
processor is itself portable being written for an
abstract machine called "FLUB". This implementation
of STAGE 2 is a modification of the DOS-11 version
(DECUS NO. 11-158 by Peter H. Heinrich) so that it will
run under RT-11.
 
Restrictions: The Stage 2 command "Change I/O Channels and Copy
Text" is modified.
 
Media (Service Charge Code): Write-Up (AA), One RX01 Diskette (KA)
Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
