110924     HEATH  Version: 1, February 1989
 
Submitted by: John M. Crowell, Davis, CA
 
Operating System: RT-11 V5.5  Source Language: MACRO-11  Memory
Required: 8KB  Hardware Required: Heathkit Model GC1000 Digital Clock
and DL11-Type Serial Port  Keywords: Clock, Heath-11
 
Abstract: This program sets the RT-11 date and time from the ASCII
string produced by the Heathkit GC1000 WWV clock connected
to a DL11 type serial port.  It may be run from a startup
command file to set the system date and time at bootstrap.
 
Notes: Executable and/or object code is included.
 
Restrictions: Operating System RT-11 V5.0 or later is required.
 
Media (Service Charge Code): One RX50 Diskette (JA)  Format: RT-11,
One RX01 Diskette (KA)  Format: RT-11
 
 
