110908     RTCLOK/TSXCLK  Version: 1.17, 1.19, November 1991
 
Submitted by: James D. Whitlock, Woodcraft Components, San Antonio, TX
 
Operating System: RT-11 V5.5, TSX-Plus  Source Language: MACRO-11
Memory Required: RTCLOK - 706 Words, TSXCLK - 826 Words  Hardware
Required: DL(V)11 type Serial line, GCW1000 Heath/Zenith.  Most
accurate clock with RS232 interface.  Keywords: Clock
 
Abstract: RTCLOK automatically sets the date and time at boot-up and
can reset the date and time as required.  Since time is lost
during the TSX boot process, the TSXCLK variant is also
included.  These programs allow the Heath/Zenith GCW1000
Most Accurate Clock to properly set the system date and time
via DL(V)11 type serial interface lines.
 
Notes: Executable and/or object is included.
 
Changes and Improvements: Simplified, more formal coding, robust,
easier use under
TSX-Plus.
 
Media (Service Charge Code): One RX50 Diskette (JA)  Format: RT-11,
One RX01 Diskette (KA)  Format: RT-11, 600' Magnetic Tape (MA)
Format: RT-11
 
 
