110847     RTMULTI and Addons  Version: V2.2, July 1986
 
Author: Fermilab Computing Dept.
 
Submitted by: Fermi National Accelerator Laboratory, Batavia, IL
 
Operating System: RT-11 V4.0 or greater  Source Language: FORTRAN IV,
MACRO-11  Software Required: FORTRAN compiler  Hardware Required:
Jorway 411 Branch Driver, Tektronix 4010, DR11-C useful, DR11-W
useful.  Keywords: Physics Applications
 
Abstract: For over ten years, Fermi National Accelerator Laboratory in
Batavia Illinois has developed and used the software package
RTMULTI for use in high speed CAMAC data acquisition for
high energy physics experiments.  This submission includes
many of the most useful developments to RTMULTI as well as
the latest version of RTMULTI itself.
 
RTMULTI, originally created at Caltech and extensively
developed by Fermilab is a CAMAC based data acquisition and
monitoring system using the Jorway 411 Branch Driver.
Histogramming and analysis of the acquired data can be
formatted interactively to provide graphics output to
Tektronix 4010 type displays.  Over 150 experiments and
collaborations have used MULTI all over the world.
 
Restrictions: Requires overlaying
 
Media (Service Charge Code): 2400' Magnetic Tape (PA)  Format: RT-11
 
 
