110932     AS6816 Cross Assembler  Version: 1.5, February 1991
 
Submitted by: Alan R. Baldwin, Kent State University, Physics Dept.,
Kent, OH
 
Operating System: MS-DOS V3.3, RT-11 V5.3, TSX-PLUS V6.4  Source
Language: C  Memory Required: 30-50KB  Keywords: Cross-Assemblers
 
Abstract: The AS6816 Cross Assembler for the 68HC16 16-bit
microprocessor is a new member of the ASxxxx Cross
Assemblers.
 
The assembler and linker have been tested using DECUS C
under TSX-PLUS and RT-11, PDOS C V5.4B, and with TurboC V1.5
under MS-DOS.  Source code for the machine dependent portion
of the AS6816 assembler and documentation for the assembler
and linker is included with the distribution.  Additionally,
test code for the AS6816 assembler is included.
 
Notes: Executable and/or object code is included.  Runs on other
operating systems
supporting Kernigan and Ritchie C Language.
 
Restrictions: To recompile the assembler requires the DECUS C compiler
and the source
code in DECUS No. 110918.
 
Complete sources not included.
 
Media (Service Charge Code): One RX02 Diskette (LA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
