110933     Data PBX  Version: May 1991
 
Submitted by: Stanley J. Reynolds, Command Data Inc., Birmingham, AL
 
Operating System: RSTS/E V9.7  Source Language: MACRO-11  Memory
Required: 64K  Keywords: Data Communications
 
Abstract: This is data PBX or data Switch MACRO-11 code for a
PDP-11/34 with an RLO2 and one to eight DZ11 boards.  It is
written to boot from the RLO2 and would require change to
source code to boot from another device.  Change the symbol
LASTDZ to indicate the number of DZ11 boards.  The console
device should be a VT device, a status is output to this
screen.
 
Notes: Executable and/or object code is included.
 
Media (Service Charge Code): One RX50 Diskette (JA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
