110938     KERMIT-11 for RT-11/TSX-PLUS  Version: 3.61, December 1991
 
Submitted by: Billy Youdelman, Consulting Electrical Engr.
 
Operating System: RT-11 V5.5, TSX-PLUS V6.5  Source Language: MACRO-11
Memory Required: See Restrictions  Hardware Required: Serial Line
Interface  Keywords: KERMIT, TSX-PLUS, Utilities - RT-11/TSX-PLUS
 
Abstract: KERMIT-11 for RT-11/TSX-PLUS is a special version of PDP-11
KERMIT, which was written by Brian Nelson of the University
of Toledo (see DECUS No. 110830).  This package has been
enhanced for use with RT-11 or TSX-PLUS as a highly
reliable, general purpose communications program.  Included
are numerous new features and fixes of all known bugs.
It has been throughly tested and is a fully supported release.
 
Notes: Executable and/or object code is included.
 
Restrictions: Operating System TSX-PLUS V6.0 or later is required.
Operating System
RT-11 V5.1 or later is required.  RT-11SJ requires 51KB and RT-11XM
requires
163KB memory.
 
Media (Service Charge Code): Four RX50 Diskettes (JD)  Format: RT-11,
Four RX02 Diskettes (LD)  Format: RT-11, 600' Magnetic Tape (MA)
Format: RT-11
 
 
