110828     CGL to ReGIS VT240 Converter  Version: V1.1, March 1987
 
Submitted by: Kazuo Okumura, Murata Machinery, Ltd., Aichi, Japan 484
 
Operating System: RSX-11M V4.1E, VAX/VMS V3.6  Source Language:
FORTRAN 77  Hardware Required: VT240 Terminal is required.  Keywords:
Conversions, ReGIS, Utilities - RSX-11
 
Abstract: This Converter generates ReGIS calls.  In the FORTRAN
program, you can use CGL subroutines by calling CGL.  The
subroutine CGL then converts CGL data to ReGIS codes.  (CGL
is Core Graphic Library.)
 
You can use the window, viewport, text and other functions
of CGL easily on the terminal which executes only ReGIS
codes.  You don't have to think about ReGIS codes.
 
In task building you must add -CGLLIB, @CGLROT or @CGLOVR in
the xxx.ODL file.  CGLLIB is a root name of convert
subroutines.  CGLROT and CGLOVR are ODL file names.
 
Documentation and sample program are on magnetic media.
 
Notes: This library was compiled on VAX 11/730, VMS V3.6, PDP-11
compatibility mode,
FORTRAN 77, V5.0.
 
Changes and Improvements: Drawing speed is about 10% faster than V1.0.
 
Restrictions: ARC drawing is not complete.
 
Media (Service Charge Code): Two RX50 Diskettes (JB)  Format: FILES-11
 
 
