110776     MINC-11 Multi User Data Acquisition and Graphics Package
for TSX-PLUS  Version: December 1984
 
Submitted by: Gavin J. Ewin, West Brunswick, Australia
 
Operating System: RT-11 V4, TSX-PLUS V4.1  Source Language: FORTRAN IV
Memory Required: 64KW  Software Required: Graphics requires DECUS No.
11-537 for VT125 or 11-435 for VT105.  TSX-PLUS library DECUS No.
11-490 and REAL-11/MNC, DECUS No. 11-537 are also necessary.  Hardware
Required: MNCAD, MNCKW  Keywords: Graphics, MINC/RT-11 Software,
Scientific Applications
 
Abstract: This package provides a set of FORTRAN programs for
implementing a multiuser data acquisition and graphics
facility under TSX-PLUS.  The system can be accessed by 3
users each monitoring up to 6 channels.  Output is stored in
nominated files while simultaneously being displayed either
graphically and/or digitally.  Options are available for real
time scaling of data.  Deferred terminal output may also be
used thus allowing the use of the virtual terminal facility
of TSX-PLUS for further program development or execution.  A
small real time program runs as a detached job accumulating
the A/D data, this data is then buffered and sent to user
display jobs via system message channels.  A program is also
included for further graphical analysis of A/D data stored in
disc files.  Although this package has been written for a
MNCAD type converter, few changes would be necessary for
other A/D's.  This software is ideally suited for automation
and data analysis of laboratory instuments.
 
Media (Service Charge Code): Write-Up and Listing (DA), One RX01
Diskette (KA)  Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
