110426     SCAN: Single Channel ANalyzer  Version: 1, 1979
 
Submitted by: Digital Equipment Corporation
 
Operating System: MINC-11, RT-11 V3C  Source Language: FORTRAN IV,
MACRO-11  Memory Required: 30K words  Hardware Required: MINC-box +
MNCKW + MNCAD  Keywords: MINC/RT-11 Software
 
Abstract: The SCAN system is an easy-to-use software package that
includes the following signal acquisition and processing
functions:
 
. Analog sweep acquisition with rates up to
  20,000 samples per second (dwell-time of .00005
  seconds)
 
. Analog signal averaging with sweep rates up
  to 20,000 samples per second
 
. Power spectrum calculation (with frequency-domain display) using
  Cosine-bell windowed time-domain data
 
. Complete time-and frequency-domain parameter generation by moving
  a data display cursor
 
. Single- or multiple-channel analog input with throughput to a
  mass-storage file
 
The SCAN package is available for MINC-11 and DECLAB-11
systems which have an MNCKW programmable clock, and
MNCAD A/D (Analog-to-Digital) converter, and a VT105
video-graphing terminal.
 
Sources not included.
 
Media (Service Charge Code): User's Manual (EA), One RX01 Diskette
(KA)  Format: RT-11
 
 
