11S105     DECUS 'C' Compiler RSX  Version: November 1988
 
Author: Volker C. Huck, Techn. Hochschule Darnstadt
 
Operating System: RSX-11M-PLUS V4.0  Source Language: MACRO-11  Memory
Required: >28KW  Keywords: Compilers, Utilities - RSX-11
 
Abstract: The DECUS-C-RSX-Kit mainly consists of DECUS-C Kits from the
"Symposium Collection from the RSX SIG, Fall 1985, Anaheim",
DECUS Part No. 11S090, "Symposium Collection from the RSX
SIG, Spring 1986, Dallas", DECUS Part No. 11S092, and the
"Symposium Collection from the RSX SIG, Spring 1987
Nashville", DECUS Part No. 11S098.  All the updates have
been merged into the original DECUS-C-Kit, "C Language
System, Second Master Release", DECUS Part No. 11S018.
Slight modifications were made to the initialization routine
[5,16]INIT.MAC (RMS specific code and prompting for command
line).  Changes were made to [5,16] library routines.  You
now may also use a working version of RMS-Library, or the
FCS Library.
 
All the command files that will build the whole DECUS-C Kit
were completely rewritten (for MCR and DCL), use
[5,3]MBUILD.CMD.  Everything including the documentation
will be rebuilt.
 
Notes: Processor must have I/D Space, EIS and a Floating Point
Processor to be able
to use the already built libraries.
 
Media (Service Charge Code): 2400' Magnetic Tape (PC)  Format: BRU
 
 
