110470     VSV-01 Device Driver for RSX-11M  Version: March 1981
 
Submitted by: David M. Stern, Research Systems, Inc., Denver, CO
 
Operating System: GAMMA-11, RSX-11M  Source Language: MACRO-11
Hardware Required: DEC VSV-01 Image Display.  Keywords: Device
Handlers
 
Abstract: The VSV-01 Device Driver for RSX-11M allows RSX-11M
tasks full control of the DEC VSV-01 Nuclear Medicine
Image Display. Functions supported are: character
display; vector graphics on a 256 by 256 display grid;
image display; loading of color translation tables;
interactive joystick input (requires an NCV-11); and
cross-hair control.
 
The driver may be incorporated into any RSX-11M system
with loadable driver support without a SYSGEN.
Four bit maps must be present for 256 by 256
graphics while two bit maps allows 256 by 128 graphics.
 
Restrictions: Driver is written for one VSV-01 only.  Loadable Driver
Support is required.
 
Media (Service Charge Code): Write-Up and Listing (DA), One RX01
Diskette (KA)  Format: FILES-11, 600' Magnetic Tape (MA)  Format:
FILES-11
 
 
