110472     KB Handler  Version: 82L17B, December 1982
 
Submitted by: N. A. Bourgeois, Jr., Sandia National Laboratories,
Albuquerque, NM
 
Operating System: RT-11 V4.0 or later, TSX-PLUS V1.4 or later  Source
Language: MACRO-11  Keywords: Device Handlers, Terminal Handler
 
Abstract: This is an RT-11 V4.0 device independent terminal
handler. It can be used in either the foreground or the
background (but not both simultaneously) to read and
write to a DL11 controlled terminal. Conditional code is
included for use with eighteen bit addressing. Eleven
set options are also included to permit configuration of
the handler.
 
Restrictions: DL-11 lines only.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
