110517     System Device Handler For RM02, RM03, RP04, RP05, RP06 and
RT-11 V4  Version: January 1982
 
Submitted by: Sanford J. Zelkovitz, Rockwell International, El
Segundo, CA
 
Operating System: RT-11 V4  Source Language: FORTRAN IV, MACRO-11
Memory Required: 16KW  Hardware Required: The Handler uses the EIS
instruction set.  Keywords: Device Handlers
 
Abstract: The following modules are included in this package:
 
RP045.MAC 	 Conditional assembly file to instruct the
		 assembler to assemble code for RP04 or RP05
		 disk drive
RP06.MAC	 Conditional assembly file to instruct the
		 assembler to assemble code for the RP06
		 disk drive
RM023.MAC	 Conditional assembly file to instruct the
		 assembler to assemble code for the RM02 or RM03
		 disk drive
ERL.MAC		 Conditional assembly file to instruct the
		 assembler to include ERROR LOGGING code
DBDQ.MAC 	 MAIN ASSEMBLY CODE.
XM.MAC 		 Conditional assembly file to instruct the
		 assembler to generate the appropriate code
		 for an XM handler
HNDBLD.SAV 	 AN ASSEMBLY SAVE MODULE to generate an indirect
		 command file on the system disk (HNDBLD.COM).
		 This indirect command file will tailor the handler to
		 your needs
DB.SYS		 RP04 or RP05 system handler without error
		 logging
DBX.SYS 	 RP04 or RP05 XM system handler without error
		 logging
DQ.SYS 		 RM02 or RM03 system handler without error
		 logging
DQX.SYS 	 RM02 or RM03 XM system handler without error
		 logging
DBFRM.FOR 	 FORTRAN program to format an RP disk drive
HNDSAV.COM 	 Indirect command file to save files on
		 tape
BADBKS.FOR 	 FORTRAN source program to generate bad
		 block files on the requested device
 
Notes: Sources for HNDBLD.SAV (System Indirect Command Builder)
are not included.
 
Restrictions: Only DB0 or DQ0 can be the system device, the other
devices are slaves (non-bootable).
 
Complete sources not included.
 
Media (Service Charge Code): Source Listing (BA), One RX01 Diskette
(KA)  Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
