110806     SYSCOM: RSTS to RSTS Communications Utility  Version: V1.5,
March 1985
 
Submitted by: David Spencer, Spencer Associates, Orangevale Cir., CA
 
Operating System: RSTS/E V8.0  Source Language: MACRO-11  Memory
Required: 11KW  Hardware Required: VT100 compatible terminal
Keywords: Data Communications, Utilities - RSTS/E
 
Abstract: SYSCOM manages terminal lines connected between two RSTS
computers.  With SYSCOM, the user may either enter virtual
terminal mode and become an iteractive terminal on the remote
system, or go in file transfer mode.  In file transfer mode
file attributes, creation date, protection code, run-time
system name, and contiguity are all copied.  In addition,
SYSCOM will accept wildcard file specifications to allow
transfer of multiple files with one command.
 
Additional features include the ability to create a log of
the virtual terminal session, force mode to type through
files to the remote system, and indirect command support for
unattended batch operation.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: DOS-11
 
 
