110709     DECODE4: RT-11 SAV Files Disassembler  Version: V2,
February 1984
 
Submitted by: Henry O. Peterson, Bend, OR
 
Operating System: Heath HT-11 H101A-5, RT-11 V3  Source Language:
MACRO-11  Memory Required: 5.4KW  Software Required: If documentation
is reformatted or revised, RUNOFF (DECUS No. 11-530), is required.
Keywords: Disassemblers, LSI-11
 
Abstract: Now, even if your computer is the result of a pact
between the fortress at Maynard and an entity 1500 km to
its west (and slightly left); even if as might be
expected its software matured well before the LSI-11
revolution you can more likely, using that software, get
away with fitting the decoder to and using it more
efficiently with that computer.
 
No more are your programs at the mercy of unpredictable
or underdeveloped foreign systems! Now you can render
such a system user friendly (as well as capitalize on
it).
 
DECODE 4.0 is a modified version of DECODE 3.0 (DECUS
No. 11-342). The program provides some additional
features over version 3.0 at the expense of being
initially somewhat awkward to use. DECODE 3.0 may be
preferable in some cases.
 
DECODE 4.0 is intended to allow easier decoding of
relatively large .SAV files on a machine with relatively
small diskette capacity such as Heath HT-11 hardware
running either the Heath-supplied software or running
RT-11, version 3. DECODE 4.0 was developed from DECODE
3.0 using the above-mentioned Heath HT-11 system.
 
Restrictions: Has not been checked with LDA files.
 
Media (Service Charge Code): User's Manual (EA), One RX01 Diskette
(KA)  Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
