110911     VSET  Version: 1.2, August 1988
 
Submitted by: John M. Crowell, Multiware, Inc.
 
Operating System: RT-11 V5.4  Source Language: MACRO-11  Memory
Required: 16KB  Keywords: Device Handlers
 
Abstract: VSET performs SET options on RT-11 device handler files.
The handler's SET code is executed as if a normal SET
command had been issued, but the handler file need not be
that of a currently installed device, and need not have the
.SYS extension.  It may reside on a disk other than the
system disk.  VSET will also, optionally, display all the
possible SET options of a handler.
 
Restrictions: Operating System RT-11 V5.4 or later is required.
 
Media (Service Charge Code): One RX50 Diskette (JA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
