110872     LAP: Slave Print Utility  Version: 1.4, April 1987
 
Submitted by: Sel Ellis, Victorian Crops Research Institute, Horsham,
Victoria, Australia 3400
 
Operating System: RT-11 V5.1, TSX-PLUS V6.1  Source Language: MACRO-11
Memory Required: 4KB  Hardware Required: VT1XX, VT2XX terminal, LA50
printer.  Keywords: Utilities - RT-11
 
Abstract: This program simplifies the process of printing a file
on a LA50 compatible printer attached to a VT100 compatible
terminal.  The printer can be configured for 40, 80 or 132
columns and normal or enhanced density.  If the file is
unpaginated, a four line skip is inserted over page
perforations.  For paginated documents, the formfeed is
expanded to the required number of linefeeds to circumvent
the TT: handler's habit of gobbling up formfeeds.  The file
name is printed at the top of the first page.  The program
is set up for seventy lines per page with a four line skip,
i.e. sixty-six lines per page on A4 paper.  These parameters
can be readily altered.  The default options are normal
density, eighty columns.  Other combinations, if required,
are presented as yes/no choices.
 
Notes: TSX-PLUS V5 or later uses SYSGEN options word to determine if
under TSX or
RT-11.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
