110784     MCE/DCE CLI - Emulator  Version: March 1984
 
Submitted by: Hans-Joachim May, SEL Kontaktbauelemente, Nurnberg, West
Germany
 
Operating System: RSX-11M V4.1  Source Language: MACRO-11  Memory
Required: 2784 Words  Keywords: DCL, Emulators
 
Abstract: This program emulates MCR/DCL.  It stores CLI input lines up
to 24 lines in a ring buffer.  These lines will be restored
by typing the cursor keys on VT100/200 or the function keys
on others (LA120, LA38 or similar, able to send escape
sequences).  Mistyped commands can be substituted.
Optionally, CLI input can be written to the CONSOLE.LOG file.
 
System features needed:  RSX-11M V4.1, Escape-sequences in
TTDRV enabled, Parent-offspring-tasking SYSGENed.  For
console-logging you need the Console-Driver and Console-Task
(CO: and COT...) SYSGENed.
 
Media (Service Charge Code): Write-Up and Listing (DA), One RX01
Diskette (KA)  Format: FILES-11, 600' Magnetic Tape (MA)  Format:
FILES-11
 
 
