110665     PB: Device Handler for Data I/O System 19 Prom Programmer
Version: August 1987
 
Submitted by: Michael M. Iloff, Moses Electronic, D-7000 Stuttgart 1,
West Germany
 
Operating System: RT-11 V5.4, TSX+  Source Language: MACRO-11  Memory
Required: 365 words  Hardware Required: Data I/O System 19 Universal
Programmer 990-1900  Keywords: Device Handlers, PROM
 
Abstract: This handler was derived from Digital Equipment
Corporation's PC11 high speed paper tape handler in order
to allow for device independent execution of file and
command transfer via PIP.SAV to and from the DATA I/O
SYSTEM 19 UNIVERSAL PROGRAMMER 990-1900 via a DLV11-J
line. It needs a running line time clock under a monitor
with device timeout feature for reading from the
programmer device.
 
Notes: The RT-11 system is XM or generated with a device-timeout
feature.  German and
English user's instructions are included as PB.GER and PB.ENG.
 
Changes and Improvements: XM bug fixed, address set code added.  See
PB.MAC header.  Adapted to
operating system RT-11 version 5.4.  Adapted to operating system TSX+.
 
Restrictions: Running line time clock.  RT-11 version 5.4 is required
due to new device
handler macros.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
