110755     SCE:  Screen Command Editor for RSX-11M  Version: 5.0,
December 1988
 
Submitted by: Johann Mraz, AVL, Dept. Messtechnik, Kleiststrasse 48,
Austria, A-8020
 
Operating System: RSX-11M-PLUS V3.0  Source Language: MACRO-11  Memory
Required: 3KW  Keywords: Editors, Utilities - RSX-11
 
Abstract: SCE displays previously entered commands for reprocessing.
The functionality is identical to the VAX/VMS DCL Command
Line Editor.  There are also other more special functions
available.
 
All entered system commands are stored in a recall buffer
for later use or command error correction.  The recall
buffer can hold a variable amount of commands with a total
of up to 587 characters.  Special functions can be called
only by typing a control character or a function key.  SCE
works as a task, started from the user terminal and is an
interface to the actual CLI.
 
Notes: Operating system RSX versions with directives: STSE$, SREX$,
SPWN$, and GCII$.
Supports terminal types VT52, VT100, VT200-Series 7 BIT and 8 BIT
mode.  It is
necessary that the setting of the terminal line corresponds to the
hardware
setting of the terminal operation mode.
 
Changes and Improvements: Upgrade to VAX/VMS compatibility, special
for video terminals.
 
Restrictions: Command line editor only for video terminals.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: FILES-11,
600' Magnetic Tape (MA)  Format: FILES-11
 
 
