110741     VLOAD: A Program for RT-11 Extended Memory Monitor
Version: V3, August 1985
 
Submitted by: Raquel K. Sanborn, University of Hawaii, Honolulu, HI
 
Operating System: RT-11 V4  Source Language: MACRO-11  Memory
Required: 28KW  Software Required: Destination program, RT-11 Extended
Memory Monitor  Hardware Required: Memory Management Unit, more than
28KW of memory  Keywords: System Management - RT-11, Tools -
Applications Development, Utilities - RT-11
 
Abstract: This is a program for the RT-11 Extended Memory Monitor.
It
is an extension of the RT-11XM keyboard command FRUN (and
SRUN).  The purpose is to run an un-overlaid virtual
foreground (or system) job with 32KW of user memory.  As a
result, it only takes up 4KW in the background (kernal mapped
memory) job's space and makes the most of the extended
memory.  In the example, BASIC-11 is used to show the
installation procedure.  Full featured BASIC-11/RT-11 takes
up 12 KW and will end up with 20 words user memory.
 
Notes: This program will need to be adapted to each use and should
be installed by someone with MACRO-11 experience.  FORTRAN or
MACRO programs may be used instead of BASIC-11.
 
Restrictions: RT-11 time of day feature doesn't work.  All
restrictions of
virtual jobs apply; e.g. no interrupt routines; no access to
Kernal Mapped Monitor Memory; I/O page not valid unless
explicity mapped; MRKT requests won't work.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
