11S077       Symposium Tape from the RSX SIG, Fall 1984, Anaheim
Version: V1, February 1985
 
Author: Various
 
Submitted by: Glenn C. Everhart, Ph.D.
 
Operating System: IAS, RSX-11D, RSX-11M, RSX-11M-PLUS, VAX/VMS  Source
Language: BASIC-11, BASIC-PLUS-2, C, FORTRAN 77, FORTRAN IV, FORTRAN
IV-PLUS, MACRO-11, MACRO-32, PASCAL  Keywords: KERMIT, Networking,
RUNOFF, Symposia Tapes - RSX-11
 
Abstract: This is the Fall 1984 US RSX SIG Symposium Tape, available
in
either BRU or VMS/BACKUP format, 1600 BPI only.  Each account
has a README.1ST file describing contents.  A few of the
programs on the tape are:
 
PRO 3XX task images for ATT (set file attributes), FORTH,
PortaCalc spreadsheet, DOB Object Disassembler, many Rainbow
or MSDOS utilities including AME86 which allows CP/M-86
programs to run under MSDOS, LUT, TTPOOL displays, complete
DR11W communications system, DECUS C, virtual disks etc. for
IAS, King James Bible (all of it!), software and XMODEM for
RSX (terminal emulator/communications packages), reminder
systems, accounting packages, auto screen clear, task
attribute display, string library, WORD-11 interfaces, cross
assemblers for 8085, 1802, general utilities, DTC fixed up to
work correctly after 1/1/1985 (desktop calendar), new
PortaCalc spreadsheet system plus 1984 form 1040 template,
binary file transfers for TALK, Bonner Lab Runoff (large
superset of DSR), 4010 and Tetronix graphics packages (and
for many more devices), DECUS C routines for DECnet and
extended FCS capabilities, STAT-11 statistical analysis
package, CCL and alternate CLI codes, online pool analyzer
for M-PLUS, many new structures analyzed, switch device from RSX
to DECnet and back, encryptor, FPP test program, PHONE, MISH,
RSXNET, SNDRCV, and VTL (VTL is a video terminal lister with
many bells & whistles), SRD V6.4 super directory maintainer,
KERMIT updates since RSX84A, includes CP/M, UNIX (2
versions), KERMIT-11, CP/M-86, and Commodore 64 KERMITS.
Much more is on the tape.  Many of these submissions will run
on VMS, frequently in native mode.  Essentially all will run
on P/OS with few or no changes.  Sources are submitted where
received; most submissions have complete sources and
documents.
 
No guarantees are made as to the completeness, usability, or
quality of the programs on the tape and the programs have not
been checked or reviewed.
 
Complete sources not included.
 
Media (Service Charge Code): 2400' Magnetic Tape (PS)  Format: BRU,
1600 BPI ONLY
 
 
