110381     PLOT  Version: June 1980
 
Submitted by: Dr. R. N. Caffin, CSIRO Div. Textiles Physics, Australia
 
Operating System: LSI-11, RT-11  Source Language: MACRO-11  Memory
Required: OBJ file is 10 blocks  Hardware Required: Analog output card
and XY recorder or digital incremental plotter such as Houston HIPLOT
Keywords: Plotting
 
Abstract: PLOT is a MACRO program configured as a set of
FORTRAN-callable subroutines to allow a user with a
standard four channel digital to analog converter card
(such as the AAV-11 or similar) to use a laboratory XY
recorder to storage CRT as a graphics output.  The calls
include origin relocation, axes, point, vector and
character plotting.  An operating manual for the FORTRAN
programmer is provided.
 
PLOTH is a similar set of routines for use with a
digital incremental plotter such as the Houston HIPLOT.
 
Included with the software are a number of test programs
using the PLOT package:  a simple test routine, random
maze generator and an interactive game called Princess
and the Dragons (designed mainly for use with a high
speed terminal such as the VT52).
User instruction manuals for PLOT and PLOTH in RUNOFF
form are included.
 
Notes: There has been little change from the original version
of PLOT. PLOTH for HIPLOT added. Also FORTRAN utility
and RUNOFF versions of manuals.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
