110936     Parity Fixer (PFX)  Version: 1.3, July 1991
 
Author: Lawrence M. Baker and Gary L. Maxwell, U.S. Geological Survey,
345 Middlefield Rd  MS977, Menlo Park, CA  94025
 
Operating System: RSX-11M-PLUS V4.1  Source Language: MACRO-11  Memory
Required: 2KW  Software Required: TeX (for documentation only)
Keywords: Utilities - RSX-11, TeX
 
Abstract: The Parity Fixer (PFX) is a privileged utility program used
to decommission a block of memory in a system-controlled
partition so that it will no longer be available.  If a
portion of memory is known to be bad, or is suspected of
causing problems (e.g., the faulty locations identified by a
memory parity-error entry in the error log), PFX can be used
to disable allocations from the offending area so that RSX
will operate safely until a more thorough diagnosis and
repair can be scheduled.
 
Release notes distributed with each order.
 
Notes: Documentation is written in TeX.  The dvi and PostScript files
are included.
 
Restrictions: Operating system RSX-11M requires PLAS support.
Operating system
RSX-11M-PLUS V4.1 or later is required.  Operating system Micro/RSX
V4.1 or
later is required.
 
Media (Service Charge Code): User's Manual (EA), 600' Magnetic Tape
(MA)  Format: FILES-11
 
 
