110400     Three Dimension Tic-Tac-Toe  Version: 1.0, May 1979
 
Submitted by: Digital Equipment Corporation
 
Operating System: RSX-11M, RSX-11S, VAX/VMS V1.0  Source Language:
FORTRAN IV, FORTRAN IV PLUS  Memory Required: 51K bytes(FORTRAN IV);
52K bytes(FORTRAN IV-PLUS)  Hardware Required: VT52 or equivalent
Keywords: Games
 
Abstract: This program plays three dimensional (4x4x4) tic-tac-toe
on a VT52 (or compatible, i.e., VT100, VT61...) CRT.
It does direct cursor addressing for both computer and
opponent moves. Instructions are displayed on the CRT.
 
Notes: Object and .TSK files are supplied for both FORTRAN IV
and FORTRAN IV-PLUS.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: FILES-11,
600' Magnetic Tape (MA)  Format: FILES-11
 
 
