Pencilled in to Dick Weaver's copy of 229-2033, "Autocoder: A Program Analysis
for Customer Engineers."

Pass 2

Sequence 135, pglin 1/26: Delete (patch CC 1 => N1)

Pass 3

Sequence 408-9, pglin 3/76-77, replace by
                BCE  WMMCHK,HLDCD,R
                BCE  WMMCHK,HLDCD,S
Sequence 474, pglin 4/39, replace by
     OPBLK      BCE  OPBLNK,EQVADD,                    MOD 3 + 4
                B    FLAGOP
     OPBLNK     BCE  SAVCOD,EQVADD-1,A
                BCE  SAVCOD,EQVADD-1,1
                BCE  SAVCOD,EQVADD-1,P
                BCE  SAVCOD,EQVADD-1,J
                BCE  SAVCOD,EQVADD-1,X
     FLAGOP     MCW  EQVADD,FREE+15
                SBR  XL3
                C    XL3,+FREE+11
                BE   TLUXT
                MCW  @*@,0+X3-1
                B    TLUXT-7
     WMMCHK     BCE  BLNKX,SAVOP-6,&
                MCW  @  @,SAVOP-6
                MZ   WMMCHK+7,SAVOP-6
                B    BLNKX
                DCW  @*@

Pass 7

Sequence 540, pglin 5/28: Delete (patch CC 1 => N1)
Sequence 579, pglin 5/67, replace CARDNO by 332
After Sequence 924, pglin 9/06, insert
               BCE  BADOP,INPUT4+12,X
               BCE
Sequence 1016, pglin 9/98: Delete (patch CC K => NK)

