

TS - Non-TS POSSIBLE
16 august 65

TS:  assign field 10
     Yank, start at 0
     thereafter: 10u;0,4 or 2G
     start at 2 sets up for ET

Non-TS: Readin. Fresh copy will exist on field 10

Commands

a - alpha symbol punch/print; sw2 on for print
b - back to id (ts only)
c - continue (pass, punching)
d - drum output on field one
e - expensive typewriter input
f - forget everything & new inital symbols
g - get ... (assign)
i - (gx) input routine on next pass 2 tape
j - (gx) jump block on next tape if pass 2
k - konstants * variable areas printout
l - (gx) title on next tape if pass 2
m - modify source (re-edit, back to et)
n - numberic symbols as in a
o - off-line (reader) source
p - (gx) punch
r - (g, x) reader
s - start (newpass, block) supress punching after error
t - tape output
w - without output (no punching or drum writing)
x - cancel, get rid of, as in punch, or title
z - binary symbol punch of midas flavor symbols
1 - pass 1 forced
2 - pass 2 forced

sw1 -> no stop after errors
sw5 -> typewriter input, symbols printed
sw6 -> supress parity check, symbols in listing format


