TRAY01

dec-11-uodpa-a-pb 1/21/76; odt-11.lda v005a; sa=13026 ra=13030 re-enter=13032; replaces: dec-11-o1pa-pb
dec-11-uodpa-a-pb 1/21/76; odt-11.pal v005a; replaces: dec-11-o1pa-pa
dec-11-uodxa-a-pb 1/14/76; ddt-11x.lda; sa=12054 ra=12056; replaces: dec-11-02pb-pb
dec-11-uodxa-a-pa 1/14/76; odt-11x.pal: replaces: dec-11-o2pb-pa
dec-11-xioxa-a-pb 1/14/76; iox v006a; replaces: dec-11-yipb-pb
dec-11-xioxa-a-pa1 1/14/76; iox v006a; tape 1 of 2; replaces: dec-11-yipb-pa1
dec-11-xioxa-a-pa2 1/21/76; iox v006a; tape 2 of 2; replaces: dec-11-yipb-pa2
dec-11-y2pa-po 1/14/76; dumpad-v001a; sa=xx7500 ra=xx7500; "use special leader"
dec-11-y1pa-po 1/21/76; dumptt-v001a; sa=xx7440 ra=xx7440; "use special leader"
dec-11-y1pa-pb 1/20/76; dumptt-v001a; sa=load address; ra=load address
dec-11-y2pa-pb 1/21/76; dumpad-v001a; sa=load address; ra=load address
dec-11-ulksa-a-pr2 1/14/76; link-11s.obj v002a; tape 2 of 2; replaces: dec-11-zlqa-pr2; (c)1970,71,72
dec-11-ulksa-a-pr1 1/21/76; link-11s.obj v002a; tape 1 of 2; replaces: dec-11-zlqa-pr1; (c)1970,71,72
dec-11-ulksa-a-pl 1/14/76; link-11s.lda v002a; sa=22714 ra=22714; replaces: dec-11-zlqa-pl; (c)1969,70,72

TRAY02

maindec-11-dekbe-b-pb 07/10/78; pdp 11/70 memory; management diagnostic; (c) 1975
maindec-11-dekbf-b-pb 06/12/78; pdp 11/70 unibus map diagnostic; (c) 1975
maindec-11-demja-c-pb 11/07/77; pdp 11/70 memory test; (c)1973,77
maindec-11-deqkc-b1-pb 06/12/78; 11/70 cpu instruction; exerciser; (c)1975,76
maindec-11-dzkla-e-pb 09/27/77; kl11/dl11-a teletype tests; (c)1972,75
maindec-11-dzkwa-f-pb 06/09/78; line frequency clock test; (c)1970,78
maindec-11-dzm9a-d-pb 06/22/78; bootstrap/terminator (m9301)/(m9400); (c)1976,77
maindec-11-dzlac-d-pb 06/14/78; la36 terminal (dl11 & kl11 interface); (c)1974,77


TRAY03

dec-11-uplsa-a-pl 12/72; pal-11s.lda v003a; sa=2066; ra=2066; replaces: dec-11-asqa-pl; (c)1970,71,72
dec-11-uplaa-a-pb 12/72; pal-11a.lda v007a; sa=1516 ra=1516; replaces: dec-11-asxb-pb; (c)1970,72
dec-11-uplsa-a-pr1 12/72; pal-11s.obj v003a; tape 1 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr2 12/72; pal-11s.obj v003a; tape 2 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr3 12/72; pal-11s.obj v003a; tape 3 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr4 12/72; pal-11s.obj v003a; tape 4 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr5 12/72; pal-11s.obj v003a; tape 5 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72

TRAY04

dec-11-l2pc-po 1/11/71; absolute loader v006a; sa=load address; ra=load address; (c)1971
maindec-00-d2g4-pt 1/21/76; special binary count pattern; (c)1968
maindec-00-dzmmg-c-pb 1/21/76; ones and zeros test tape; (c) 1968
maindec-11-d0nc-pb 1/20/76; t14 trap test; (c)1970,71,72
maindec-11-d9ea-pb 1/21/76; maintenance loader; (c)1970
maindec-11-dzjaq-d-pb 1/21/76; pdp-11 power fail; swr not req; (c)1972,75
maindec-11-dzkla-e-pb 1/21/76; kl11/dl11-a teletype tests; (c)1972;75
maindec-11-dzkua-c-pb 1/14/76; unibus systems exerciser diagnostic; (c)1975
maindec-11-dzkwa-d-pb 1/21/76; line frequency clock test; (c)1970,75
maindec-11-dzmmd-b-pb 1/21/76; basic memory patterns test; (c)1972,75
maindec-11-dzmme-c-pb 3/21/75; moving ones; and zeros test; (c)1972,75
maindec-11-dzmmf-a-pb 5/15/72; 1's susceptability test; replaces: maindec-11-d1fb-pb; (c)1970,72
maindec-11-dzmmf-b-pb 1/21/76; one's susceptability test; (c)1972,75
maindec-11-dzmmg-c-pb 3/73; worst case noise test; (c)1970,71,72,73
maindec-11-dzmmg-d-pb 1/21/76; worst case noise test; (c)1972,73,75
maindec-11-dzmmh-b-pb 1/21/76; core heating test; (c)1970,72,73
maindec-11-dzmmi-b-pb 1/21/76; randat; (c)1972,75
maindec-11-dzmmk-b-pb 1/21/76; up-down address test; (c)1972,75
maindec-11-dzqkb-f-pb 1/21/76; t17-4k system exerciser; (c)1972,75
maindec-11-dzqkc-e-pb 1/20/76; 11 family instruction exerciser; (c)1973,74,75
maindec-11-dzqmb-g-pb 1/21/76; 0-124k memory exerciser; (c)1972,74,75
maindex-11-dzkub-a-pb 1/14/76; unibus exerciser module diagnostic; (c)1975


TRAY05

maindec-11-dzqma-b-pb 12/1/72; memory i/o exerciser; (c)1972

TRAY06

maindec-11-dqfpa-b-pb 12/13/77; pdp 11/6x fp11-e floating point basic instruction tests; (c)1977
maindec-11-dqfpb-b-pb 09/02/77; pdp-11/6x-fp11-e floating point unit advanced instruction tests; (c)1977
maindec-11-dqfpc-b-pb 10/17/77; pdp-11/6x fp11-e floating point unit instruction exerciser; (c)1977
maindec-11-dqfpd-b-pb 09/02/77; pdp-11/6x fp11 floating point unit add/sub/mul/div random operand exerciser; (c)1977
maindec-11-dqfpe-a-pb 11/10/77; pdp-11/60 fp11-e hardware diagnostic; (c)1977
maindec-11-dqkda-b-pb 01/06/78; kd11-k-basic logic tests; (c)1977
maindec-11-dqkdb-a-pb 01/06/78; pdp 11/6x traps test; (c)1977

TRAY07

dec-11-nfpma-a-pr1 8/72; fpmp-11 single precision package; replaces: dec-11-yqpc-pb; (c)1971,72
dec-11-nfpma-a-pr2 8/72; fpmp-11 double precision package; replaces: dec-11-yqpc-pb; (c)1971,72
dec-11-nfpma-a-pa1 8/72; fpmp-11 source; tape 1 of 6; replaces: dec-11-yqpc-pa; (c)1971,72
dec-11-nfpma-a-pa2 8/72; fpmp-11 source; tape 2 of 6; replaces: dec-11-yqpc-pa; (c)1971,72
dec-11-nfpma-a-pa3 8/72; fpmp-11 source; tape 3 of 6; replaces: dec-11-yqpc-pa; (c)1971,72
dec-11-nfpma-a-pa4 8/72; fpmp-11 source; tape 4 of 6; replaces: dec-11-yqpc-pa; (c)1971,72
dec-11-nfpma-a-pa5 8/72; fpmp-11 source; tape 5 of 6; replaces: dec-11-yqpc-pa; (c)1971,72
dec-11-nfpma-a-pa6 8/72; fpmp-11 source; tape 6 of 6; replaces: dec-11-yqpc-pa; (c)1971,72


TRAY08

dec-11-udmba-a-pb 5/30/78; ptsp v01 dumpab.lda; (c)1975
dec-11-udmba-a-po 5/30/78; ptsp v01 dumpab.po; (c)1975
dec-11-ulkia-a-pl 5/30/78; ptsp v01 link11.lda; (c)1975
dec-11-ulkia-a-pr 5/30/78; ptsp v01 link11.obj; (c)1975
dec-11-uoxia-a-pr 5/30/78; ptsp v01 odt11x.obj; (c)1975
dec-11-uedia-a-pb 5/30/78; ptsp v01 ed-11.lda; (c)1975
dec-11-uoxia-a-pa 5/31/78; ptsp v01; odt11x.pal; (c)1975
dec-11-uplia-a-pr1 5/31/78; ptsp v01 relmem.obj; tape 1 of 5; (c)1975
dec-11-uplia-a-pl 5/30/78; ptsp v01 pal11s.lda; (c)1975
dec-11-uplia-a-pr2 5/31/78; ptsp v01 pal11s.obj; tape 2 of 5; (c)1975

TRAY09

dec-11-cgpa-pa1 1/21/76; pdp-11 checkout package; tapdup.asc.(2); tape 1 of 2; (c)1970
dec-11-cgpa-pa2 1/21/76; pdp-11 checkout package; tapdup.asc.(1); tape 2 of 2; (c)1970
dec-11-cgpa-pb1 1/21/76; pdp-11 checkout package; test b sa=none ra=none; tape 1 of 2; (c)1970
dec-11-cgpa-pb2 1/21/76; pdp-11 checkout package; test 1 sa=none ra=none; tape 2 of 2; (c)1970
dec-11-uabla-a-po 1/21/76; pdp-11 absolute loader; replacees: dec-11-p2pc-po; (c)1971,75
dec-11-uedpa-a-pb 1/14/76; ed-11 v005a; replaces: dec-11-e1pa-pb; (c)1970,72
dec-11-uplaa-a-pb 1/14/76; pal-11a.lda v007a; sa=1516 ra=1516; replaces: dec-11-e1pa-pb; (c)1970,72
dec-11-uplsa-a-pl 1/14/76; pal-11s, lda v003a; sa=2066 ra=2066; replaces: dec-11-asqa-pl; (c)1970,71,72
dec-11-uplsa-a-pr1 1/21/76; pal-11s.obj v003a; tape 1 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr2 1/14/76; pal-11s.obj v003a; tape 2 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr3 1/14/76; pal-11s.obj v003a; tape 3 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr4 1/14/76; pal-11s.obj v003a; tape 4 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr5 1/14/76; pal-11s.obj v003a; tape 5 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72
dec-11-uplsa-a-pr6 1/14/76; pal-11s.obj v003a; tape 6 of 6; replaces: dec-11-asqa-pr; (c)1970,71,72


TRAY10

ak-8002d-mc 05/08/78; cerhad0 rh70 ctlr diag; replaces: md-11-derha-c-pb; (c)1975,78
ak-e197d-mc 06/12/78; cerhad0 rh70 ctrlr diag 2/2; (c)1975,78
dec-11-uabla-a-po 03/31/78; pdp-11 absolute loader; replaces: dec-11-l2pc-po
maindec-11-dcktf-c-pb 03/02/78; memory management abort tests; (c)1972,73,75
maindec-11-dekba-b-pb 08/16/77; pdp 11/70 cpu diagnostic part 1; (c)1975
maindec-11-dekbb-c-pb 02/17/78; pdp 11/70 cpu diagnostic part 2; (c)1975,76
maindec-11-dekbc-b-pb 07/11/78; pdp 11/70 cache diagnostic part 1; (c)1975
maindec-11-dekbd-c-pb 06/12/78; pdp 11/70 cache diagnostic (part 2); (c)1975,76

TRAY11

maindec-11-dxqad-f-pb 1/23/76; dec/x11 configurator program; (c)1974,1975
maindec-11-dxqla-e1-pr 1/23/76; dec/x11 monitor library #1; (c)1974,1975
maindec-11-dxqlb-h-pr 1/23/76; dec/x11 general products library #1; (c)1974,75
maindec-11-dxqlc-h1-pr 1/23/76; dec/x11 general products library #2; (c)1974,1975
maindec-11-dxqld-i-pr 1/23/76; dec/x11 communications options; library #1; (c)1975
maindec-11-dxqle-e-pr 1/23/76; dec/x11 communications options; library #2; (c)1975
maindec-11-dxqlf-e-pr 1/23/76; lab & industrial options module; library #1; (c)1974,75
maindec-11-dxqlg-g-pr 1/23/76; dec/x11 lab and industrial; options library #2; (c)1975
maindec-11-dxqlj-b-pr 1/23/76; dec/x11 11/70; monitor library; (c)1975


TRAY12

ak-8208c-mc 4/14/78; cvkafc0 drv11 test; replaces: md-11-dvkaf-b-pb; (c)1975,78
dec-11-uablb-a-po 4/26/78; non-switch register pdp-11; absolute loader vb07.00; (c)1975
maindec-11-dvaaa-a-pb 3/27/78; aav11 diagnostic test; (c)1976
maindec-11-dvada-a1-pb 2/13/78; adv11 performance test; (c)1976,77
maindec-11-dvdra-a-pb 1/13/78; drv11b diagnostic test; (c)1976
maindec-11-dvdrb-a-pb 3/6/78; drv11b inter-processor; exerciser; (c)1976
maindec-11-dvkwa-b-pb 12/8/77; kwv11a diagnostic; (c)1976,77
maindec-11-dvm8a-a-pb 2/21/78; bdv11-aa bootstrap diagnostic; (c)1977
maindec-11-dxqlh-g1-pr 1/23/76; dec/x11 new options module library #1; (c)1974,75
maindec-11-dxqli-b-pr 1/23/76; dec/x11 new options; library #2; (c)1975


TRAY13

maindec-11-dzdha-a-pb 4/8/76; dh11 static logic test; (c)1972
maindec-11-dzdhb-a-pb 4/21/76; dh11 memory test; (c)1972
maindec-11-dzdhc-b-pb 5/10/76; dh11 transmitter and receiver; logic test; (c)1972,76
maindec-11-dzdhd-b-pb 4/8/76; dh11 speed selection; logic test; (c)1972,73
maindec-11-dzdhe-a-pb 4/21/76; dh11 character length; and basic data test; (c)1972
maindec-11-dzdhf-a-pb 3/26/76; dh11 single line data test; (c)1972
maindec-11-dzdhg-b-pb 3/25/76; dh11 single line parity check; and multi-line data test; (c)1972,73
maindec-11-dzdhh-b-pb 4/21/76; dh11 auto-echo test; (c)1972,73
maindec-11-dzdhi-a-pb 3/22/76; dh11 break and half duplex test; (c)1972
maindec-11-dzdhj-b-pb 4/21/76; single line/echo/online; for dh11; (c)1973,75
maindec-11-dzdhk-a-pb 3/24/76; modem control multiplexer diagnostic; (c)1974
maindec-11-dzdhl-a-pb 4/21/76; dh11 overlay for interprocessor; test program; (c)1975
maindec-11-dzdhm-a-pb 4/27/76; dh11 diagnostic; (c)1976
maindec-11-dzdhn-a-pb 5/7/76; dh11 data reliablity tests/single; line echo and patterns/cable tests; (c)1976
maindec-11-dzita-b-pb 5/5/76; interprocessor test program; (itp); (c)1974,75


TRAY14

ak-b011b-mc 6/26/78; czrmgb0 rm03/02 du por lgc 1; tp 1 of 3; replaces: md-11-dzrmg-a-pb1; (c)1977
ak-b014b-mc 4/24/78; czrmhb0 rm03/02 du por lgc 2; replaces: md-11-dzrmh-a-pb; (c)1977
ak-b017b-mc 4/27/78; czrmib0 rm03/02 dr cpt tst; replaces: md-11-dzrmi-a-pb; (c)1977
ak-b020b-m1 5/8/78; czrmjb1 rm03/2 dskls diag; replaces: ak-b020b-mc; (c)1977,78
ak-e012b-mc 5/4/78; czrmgb0 rm03/02 du por lgc 1; tp 2 of 3; replaces: md-11-dzrmg-a-pb2; (c)1977
ak-e015b-m2 6/2/78; czrmcb2 rm03/2 fctnl tst 1; replaces: ak-e015b-mc; (c)1977,78
ak-e013b-mc 2/24/78; czrmgb0 rm03/02 du por lgc 1 tp; 3 of 3; replaces: md-11-dzrmg-a-pb3; (c)1977
ak-e016b-m2 6/1/78; czrmcb2 rm03/02 fctnl tst 1; replaces: ak-e016b-mc; (c)1977,78

TRAY15

TMO2/TU16 RDC FA&T PT KIT ZJF10-PB

ak-9449h-mc 9/21/78; cztuah0 tm02-tu16/te16 reliab; replaces: md-11-dztua-g1-pb; (c)1974,78
ak-9453g-m1 9/13/78; cztubg1 tm02-tu16/te16 bsc fc; (c)1974/78
ak-9457f-m1 8/16/78; cztucf1 tm02/tu16 ctrl lgc; (c)1974,78
ak-8474c-m1 11/9/78; cztugc1 tm02/te16 dr fcnt tmr; (c)1977,78
maindec-11-dztud-d-pb; tm02 drive function timer; (c)1974,77
maindec-11-dztue-d-pb 1031/78; tu16 utility driver; (c)1974,76

TRAY16

ak-b005b-m1 6/14/78; czrmeb1 rm03/2 fctnl tst 3; replaces: ak-b005b-mc; (c)1977,78
ak-b014b-mc 4/24/78; czrmhb0 rm03/02 du por lgc 2; replaces: md-11-dzrmh-a-pb; (c)1977
ak-a999b-m2 6/23/78; czrmcb2 rm03/2 fctnl tst 1; replaces: ak-a999b-mc; (c)1977,78
ak-9255c-mc 5/26/78; cztmac0 rm03/2 formatter; replaces: md-11-dzrma-b-pb; (c)1977
ak-b002b-m1 6/14/78; czrmdb1 rm03/2 fctnl tst 2; replaces: ak-b002b-mc; (c)1977,78
ak-b011b-mc 6/14/78; czrmgb0 rm03/02 du por lgc 1 tp; 1 of 3; replaces: md-11-dzrmg-a-pb1; (c)1977
ak-a996b-mc 5/1/78; czrmbb0 rm03/2 perf exer; replaces: md-11-dzrmb-a-pb; (c)1977
ak-b008b-mc 4/27/78; czrmfb0 rm03/02 extd drive tst; replaces: md-11-dzrmf-a-pb; (c)1977

TRAY17

option number ZJ180-PB
RP04/5/6 DIAG PAPERTPAE ONLY KIT

ak-9184c-mc 09/14/78; czrjac0 rp04/5/6 rd/wt; (c)1976,78
ak-9189c-mc 09/14/78; czrjbc0 rp04/5/6 fmtr; (c)1974,78
ak-9194b-mc 10/13/78; czrjcb0 rp04/5/6 head almnt.; replaces: md-11-dzrjc-a1-pb; (c)1974,77
ak-9199c-mc 07/17/78; czrjgb1 rp04/5/6 dskls 1; (c)1974,78
ak-9202c-mc 07/26/78; czrjec0 rp04/5/6 dl ctrlr 1/2; (c)1976,78
ak-9211b-m1 2/21/78; czrjdc0 mlt-dr lgc; replaces: md-11-dzrjd-b-pb; (c)1974,77
ak-9216-mc 06/29/78; czrjhb0 rp04/5/6 dskls ctrlr 2; replaces: md-11-dzrjh-a-pb; (c)1974,77
ak-9221b-mc 06/14/78; czrj1b1 rp04/5/6 ctrlr1; (c)1974,78
ak-9226b-mc 08/23/78; czrjjb0 rp04/5/6 tp 1 of 2; replaces: md-11-dzrjj-a-pb; (c)1974,77
ak-e116b-m1 06/14/78; czrjgb1 rp04/5/6 dskls 1; (c)1974,78
ak-e117b-m1 06/14/78; czrjib1 rp04/5/6 ctrlr1; (c)1974,78
ak-e123c-mc 06/21/78; czrjec0 rp04/5/6 dl ctrlr; (c)1976,78
ak-e124b-mc 07/12/78; czrjjb0 rp04/5/6 ctrlr2 tp 2 of 2; (c)1977
ak-e196c-mc 10/06/78; czrjac0 rp04/5/6 rd/wt; (c)1976,78
maindec-11-dzrjf-a-pb 09/08/78; rp04/5/6 dual controller logic test - part 2; replaces: md-11-dzrpq-a-pb;(c)1976

TRAY18

ak-9396i-mc; cztmai0 tm,a,b-11 instr tst; (c)1971,79
dec-11-ggtsa-a-pb 3/19/73; focal-gt; (C)1973
maindec-11-ddgta-b-pb 11/1/73; gt40/gt44 instruction test 1; (c)1973
maindec-11-ddgtb-b-pb 11/1/73; gt40/gt44 instruction test II; (c)1973
maindec-11-ddgtc-b-pb 11/1/73; gt40/gt44 visual display test with vr14 display; (c)1973
maindec-11-ddgtd-b-pb 11/1/73; gt40 rom verify test; (c)1973
maindec-11-ddgte-b-pb 11/1/73; gt40 quick verify test; (c)1973
maindec-11-ddgtf-a-pa 3/1/73; gt-40 overlay for gtp-11; (c)1973
maindec-11-ddgtg-a-pb 11/1/73; gt40/gt44 visual display test with vr17 display; (c)1973


