C	HYBRID STATIC ANALOG TEST
C	NOVEMBER, 1968
C	C.L. CROSS
C	CARNEGIE-MELLON UNIVERSITY
C	HYBRID COMPUTATION LABORATORY
C
	INTEGER ANSWER,COL,ERROR,OU,S,TOLER,TYPE,VALUE
	LOGICAL ERRORS,ERRSW,REPSW,SAVESW,SKIP,STATE,SWITCH,Z
	LOGICAL RSAC,RSCS,TGPI,TRSL
	REAL IFIELD(8),ILCODE(8),INAME(2),IREP(8),LMODE(3),INVARG(8)
	REAL IERROR(8,5),MODES(3,3),MESS1(5,3),MESS2(3,3)
	REAL MFIELD,NFIELD,ATOD
	DIMENSION ONAME(2),AMODE(3),TCON(3),UFIELD(8),TYPES(8)
	DIMENSION COMP(5),SLINE(5),GPI(5),WSTATE(3),OCCURI(3),FOCCUR(3)
	EXTERNAL HANDLE
	COMMON/A/CHAR(72)
	COMMON/B/VALUE
	COMMON/C/COL,TYPE
	COMMON/D/ANSWER
	COMMON/E/Z
	COMMON/F/INPUT
	EQUIVALENCE (IERROR(1,1),UFIELD(1))
	EQUIVALENCE (IERROR(1,2),ILCODE(1))
	EQUIVALENCE (IERROR(1,3),IFIELD(1))
	EQUIVALENCE (IERROR(1,4),IREP(1))
	EQUIVALENCE (IERROR(1,5),INVARG(1))
	EQUIVALENCE (MODES(1,1),AMODE(1))
	EQUIVALENCE (MODES(1,2),TCON(1))
	EQUIVALENCE (MODES(1,3),LMODE(1))
	EQUIVALENCE (MESS1(1,1),COMP(1))
	EQUIVALENCE (MESS1(1,2),SLINE(1))
	EQUIVALENCE (MESS1(1,3),GPI(1))
	EQUIVALENCE (MESS2(1,1),WSTATE(1))
	EQUIVALENCE (MESS2(1,2),OCCURI(1))
	EQUIVALENCE (MESS2(1,3),FOCCUR(1))
	DATA AMODE(1)/5H ANAL/
	DATA AMODE(2)/5HOG MO/
	DATA AMODE(3)/5HDE   /
	DATA ATOD/2HAD/
	DATA COMP(1)/5HCOMPA/
	DATA COMP(2)/5HRATOR/
	DATA COMP(3)/5H     /
	DATA COMP(4)/5H     /
	DATA COMP(5)/5H     /
	DATA FOCCUR(1)/5HFAILE/
	DATA FOCCUR(2)/5HD TO /
	DATA FOCCUR(3)/5HOCCUR/
	DATA GPI(1)/5HGENER/
	DATA GPI(2)/5HAL PU/
	DATA GPI(3)/5HRPOSE/
	DATA GPI(4)/5H INTE/
	DATA GPI(5)/5HRRUPT/
	DATA IFIELD(1)/5HILLEG/
	DATA IFIELD(2)/5HAL FI/
	DATA IFIELD(3)/5HELD  /
	DATA IFIELD(4)/5H     /
	DATA IFIELD(5)/5H     /
	DATA IFIELD(6)/5H     /
	DATA IFIELD(7)/5H     /
	DATA IFIELD(8)/5H     /
	DATA ILCODE(1)/5HILLEG/
	DATA ILCODE(2)/5HAL CO/
	DATA ILCODE(3)/5HMMAND/
	DATA ILCODE(4)/5H CODE/
	DATA ILCODE(5)/5H     /
	DATA ILCODE(6)/5H     /
	DATA ILCODE(7)/5H     /
	DATA ILCODE(8)/5H     /
	DATA INVARG(1)/5HINVAL/
	DATA INVARG(2)/5HID AR/
	DATA INVARG(3)/5HGUMEN/
	DATA INVARG(4)/5HT IN /
	DATA INVARG(6)/5HLD   /
	DATA INVARG(7)/5H     /
	DATA INVARG(8)/5H     /
	DATA IREP(1)/5HINCON/
	DATA IREP(2)/5HSISTE/
	DATA IREP(3)/5HNT RE/
	DATA IREP(4)/5HPETIT/
	DATA IREP(5)/5HION S/
	DATA IREP(6)/5HPECIF/
	DATA IREP(7)/5HICATI/
	DATA IREP(8)/5HON   /
	DATA LMODE(1)/5H LOGI/
	DATA LMODE(2)/5HC MOD/
	DATA LMODE(3)/5HE    /
	DATA MFIELD/5HM FIE/
	DATA NFIELD/5HN FIE/
	DATA OCCURI(1)/5HOCCUR/
	DATA OCCURI(2)/5HRED  /
	DATA OCCURI(3)/5H     /
	DATA SLINE(1)/5HSENSE/
	DATA SLINE(2)/5H LINE/
	DATA SLINE(3)/5H     /
	DATA SLINE(4)/5H     /
	DATA SLINE(5)/5H     /
	DATA TCON(1)/5H TIME/
	DATA TCON(2)/5H CONS/
	DATA TCON(3)/5HTANT /
	DATA TYPES(1)/2HA /
	DATA TYPES(2)/2HD /
	DATA TYPES(3)/2HF /
	DATA TYPES(4)/2HT /
	DATA TYPES(5)/2HP /
	DATA TYPES(6)/2HPP/
	DATA TYPES(7)/2HD /
	DATA TYPES(8)/2HQ /
	DATA UFIELD(1)/5HUNREC/
	DATA UFIELD(2)/5HOGNIZ/
	DATA UFIELD(3)/5HABLE /
	DATA UFIELD(4)/5HFIELD/
	DATA UFIELD(5)/5H     /
	DATA UFIELD(6)/5H     /
	DATA UFIELD(7)/5H     /
	DATA UFIELD(8)/5H     /
	DATA WSTATE(1)/5HIN WR/
	DATA WSTATE(2)/5HONG S/
	DATA WSTATE(3)/5HTATE /
C	CONSOLE INITIALIATION
	CALL INIT(ERROR)
	IF (ERROR.EQ.0) GO TO 10
	WRITE (4,99999)
	STOP 1
C	PROGRAM INITIALIZATION
10	TOLER=5
	ERRSW=.TRUE.
	SAVESW=.FALSE.
	WRITE(4,10010)
C	INPUT UNIT SPECIFICATION
20	IF (RSAC(0)) GO TO 21
	WRITE (4,10020)
	GO TO 22
21	WRITE(4,10021)
22	WRITE(4,10000)
	READ (4,11000) IU
	IF (IU.LT.1) GO TO 60
	IF (IU-3) 70,30,80
C	DECTAPE INPUT
30	IF (.NOT.RSAC(0)) WRITE(4,10030)
40	IF (RSAC(0)) GO TO 41
	WRITE(4,10040)
	GO TO 42
41	WRITE(4,10041)
42	WRITE(4,10000)
	READ(4,11010) IU,INAME
	IF (IU.GT.0.AND.IU.LT.4) GO TO 50
	WRITE(4,12000)
	GO TO 40
50	CALL SEEK(IU,INAME)
	GO TO 100
C	ILLEGAL IU
60	WRITE(4,12000)
	GO TO 20
C	TELETYPE OR PAPER TAPE INPUT
70	IU=IU+3
	GO TO 100
C
80	IF (IU-4) 60,90,60
C	DCT-2000 CARD READER
90	IU=7
C	OUTPUT UNIT SPECIFICATION
100	IF (RSAC(0)) GO TO 101
	WRITE(4,10050)
	GO TO 102
101	WRITE(4,10051)
102	WRITE(4,10000)
	READ(4,11000) OU
	IF (OU-1) 120,110,130
C	TELETYPE OUTPUT
110	OU=4
	GO TO 200
C	ILLEGAL OU
120	WRITE(4,12010)
	GO TO 100
C
130	IF (OU-3) 140,150,180
C	PAPER TAPE OUTPUT
140	OU=6
	GO TO 200
C	DECTAPE OUTPUT
150	IF (.NOT.RSAC(0)) WRITE(4,10060)
160	IF (RSAC(0)) GO TO 161
	WRITE(4,10040)
	GO TO 162
161	WRITE(4,10041)
162	WRITE(4,10000)
	READ(4,11010) OU,ONAME
	IF (OU.GT.0.AND.OU.LT.4) GO TO 170
	WRITE(4,12010)
	GO TO 160
170	CALL ENTER(OU,ONAME)
	GO TO 200
C
180	IF (OU-4) 120,190,120
C	DCT-2000 LINE PRINTER
190	IF (IU.NE.7) GO TO 195
C	BOTH IU AND OU ARE THE DCT-2000
	WRITE(4,12030)
	GO TO 20
195	OU=8
C	TEST INITIALIZATION
200	INPUT=IU
	S=1
	IF (.NOT.RSAC(0)) WRITE(4,10070)
210	IF (RSAC(0)) GO TO 211
	WRITE(4,10080)
	GO TO 212
211	WRITE(4,10081)
212	WRITE(4,10000)
	READ(4,11000) L
C
C	DATA STATEMENT INTERPRETER
C
C	READ NEXT EXECUTABLE RECORD
1000	IF (SKIP) GO TO 1001
	IF (ERRORS) GO TO 1010
	GO TO 1020
1001	IF (ERRORS) GO TO 1020
1010	S=1
1020	IF (RSAC(7).OR.RSAC(8).OR.RSAC(9)) GO TO 9990
	IF (RSAC(10)) GO TO 2140
	JINPUT=INPUT
	IF ( RSAC(11)) JINPUT=4
	DO 1030 L=1,S
	IF (JINPUT.EQ.4) WRITE(4,10000)
1030	READ(JINPUT,11020) CHAR
C	GET COMMAND CODE
1040	COL=1
	CALL DECODE
	IF (TYPE) 2500,1050,1060
1050	IF (VALUE.NE.0) GO TO 2520
C	BLANK STATEMENT - RESTORE IU
	INPUT=IU
	GO TO 1010
C
1060	IF (TYPE-3) 2520,1070,1150
1070	IF (VALUE+5) 1080,1090,1100
C	YES STATEMENT
1080	ERRSW=.TRUE.
	GO TO 1010
C	NO STATEMENT
1090	ERRSW=.FALSE.
	GO TO 1010
C
1100	IF (VALUE+3) 1110,1120,1130
C	ON STATEMENT
1110	SAVESW=.TRUE.
	GO TO 1010
C	OFF STATEMENT
1120	SAVESW=.FALSE.
	GO TO 1010
C	END,COMMENT,OTHER
1130	IF (VALUE+1) 2140,1140,1150
C	COMMENT
1140	WRITE(OU,11030) CHAR
	GO TO 1010
C	SAVE COMMAND CODE AND INITIALIZE ALL VALUES
1150	IVALUE=VALUE
	ITYPE=TYPE
	I=-1
	J=0
	M=0
	N=0
	S=1
	STATE=.TRUE.
	SWITCH=.FALSE.
	ERRORS=.FALSE.
	IF (ITYPE.NE.3) GO TO 1380
C	GET (N)
	CALL DECODE
	IF (TYPE) 2500,1200,1160
1160	IF (TYPE-2) 1170,1410,2540
1170	N=VALUE
	IF (IVALUE-25) 1210,1180,1190
C	ERROR TOLERANCE STATEMENT
1180	TOLER=N
	GO TO 1020
C	SKIP STATEMENT
1190	S=N+1
1195	INPUT=IU
	GO TO 1020
C
1200	IF (VALUE.NE.0) GO TO 1230
	IF (IVALUE-25) 1210,1180,1195
C	GET (SIGN)
1210	CALL DECODE
	IF (TYPE) 2500,1220,1260
1220	IF (VALUE.EQ.0) GO TO 1240
1230	IF (IVALUE.GE.25) GO TO 2540
	IF (VALUE.EQ.1) GO TO 1240
C	MINUS SIGN
	STATE=.FALSE.
C	PLUS SIGN
1240	IF (IVALUE.GE.15) GO TO 1290
C	GET (M)
	CALL DECODE
	IF (TYPE) 2500,1250,1270
1250	IF (VALUE) 2540,1290,2540
1260	IF (IVALUE.GE.15) GO TO 1310
1270	IF (TYPE-2) 1280,1410,2540
1280	M=VALUE
C	GET (I)
1290	CALL DECODE
	IF (TYPE) 2500,1300,1310
1300	IF (VALUE) 2540,1330,2540
1310	IF (TYPE-2) 1320,1410,2540
1320	I=VALUE
C	GET (J)
1330	CALL DECODE
	IF (TYPE) 2500,1340,1350
1340	IF (VALUE) 2540,1370,2540
1350	IF (TYPE-2) 1360,1410,2540
1360	J=VALUE
1370	IF (IVALUE.EQ.11.OR.IVALUE.GE.20) GO TO 1600
C	GET (ERROR SWITCH)
1380	CALL DECODE
	IF (TYPE) 2500,1390,1400
1390	IF (VALUE) 2540,1600,2540
1400	IF (TYPE-2) 2540,1420,2540
1410	IF (IVALUE.EQ.11.OR .IVALUE.GE.20) GO TO 2540
1420	IF (VALUE) 1430,1440,1450
C	E ERROR SWITCH
1430	SKIP=.TRUE.
	GO TO 1460
C	H ERROR SWITCH
1440	SWITCH=.TRUE.
	GO TO 1600
C	S ERROR SWITCH
1450	SKIP=.FALSE.
C	GET (S)
1460	CALL DECODE
	IF (TYPE) 2500,1470,1480
1470	IF (VALUE) 2540,1600,2540
1480	IF (TYPE-2) 1490,2540,2540
1490	S=VALUE+1
C	END OF DATA STATEMENT INTERPRETER
C
C	DATA STATEMENT EXECUTION
1600	IF (ITYPE.EQ.3) GO TO 1650
1605	IF (ITYPE-5) 1610,1630,1640
C	ANALOG MODE STATEMENT
1610	CALL SAMO(IVALUE,ERROR)
C	15 MILLISECOND PAUSE
	DO 1620 L=1,1100
1620	CONTINUE
	GO TO 1642
C	TIME CONSTANT STATEMENT
1630	CALL STCO(IVALUE,ERROR)
	GO TO 1642
C	LOGIC MODE STATEMENT
1640	CALL SLMO(IVALUE,ERROR)
C	ERRORX SECTION
1642	IF (ERROR.EQ.0) GO TO 1000
	ERRORS=.TRUE.
	IF (SWITCH.OR.RSAC(4).OR.RSAC(6)) GO TO 1644
	IF (ERRSW.AND..NOT.RSAC(5)) GO TO 1644
	IF (RSAC(1)) GO TO 1605
	GO TO 1000
1644	WRITE(OU,12040) (MODES(J,I),J=1,3)
	IF (SWITCH.OR.RSAC(1).OR.RSAC(6)) GO TO 1645
	GO TO 1000
1645	IF (OU.NE.4) WRITE(4,12040) (MODES(J,I),J=1,3)
	ANSWER=0
	CALL DECIDE
	IF (ANSWER) 1605,1000,1040
C	TRANSLATE COMPONENT INDEX TO ALPHANUMERIC CODE
1650	IF (IVALUE-10) 1652,1654,1656
1652	CTYPE=TYPES(IVALUE+1)
	GO TO 1656
1654	CTYPE=ATOD
C	ANALYZE ADDRESS (N) AND VALUE (M)
1656	IF (IVALUE-10) 1680,1690,1660
1660	IF (IVALUE-15) 1710,1730,1670
1670	IF (IVALUE-17) 1730,1740,1740
C	ANALOG COMPONENT
1680	NMAX=119
	GO TO 1700
C	A-TO-D
1690	NMAX=14
1700	IF (RSAC(2)) GO TO 1725
	IF (RSAC(3)) GO TO 1701
	IF (SAVESW) GO TO 1725
1701	IF (IVALUE.EQ.10) GO TO 1720
	IF (M.GT.11999) GO TO 2600
	IF (IVALUE.NE.4) GO TO 1725
	CALL RAMO(MODE)
	IF (MODE.NE.7) GO TO 1725
	IF (.NOT.STATE) GO TO 2600
	GO TO 1720
C	D-TO-A
1710	NMAX=11
1720	IF (M.GT.9999) GO TO 2600
1725	IF (N.GT.NMAX) GO TO 2610
	IF (IVALUE.EQ.11) M=FLOAT(M)*13.1072
	IF (.NOT.STATE) M=-M
	GO TO 1770
C	SL OR GP
1730	NMAX=7
	GO TO 1750
C	CS, FR, OR CL
1740	NMAX=15
1750	IF (N-NMAX-1) 1770,1760,2610
C	ALL COMPONENTS
1760	IF (I.GE.0) GO TO 2560
	N=0
	J=NMAX+1
	GO TO 1790
C	ANALYZE REPETITION SPECFICATIONS
1770	IF (I) 1780,1800,1810
C	(I) IS BLANK - NO REPETITIONS
1780	J=N+1
1790	I=1
	GO TO 1820
C	(I) IS ZERO - J REPETITIONS OF N
1800	L=N
	N=1
	I=1
	REPSW=.FALSE.
	GO TO 1830
C	(I) IS GREATER THAN ZERO - INCREMENT N BY I TO J
1810	IF (N.GT.J.OR.J.GT.NMAX) GO TO 2560
	J=J+1
1820	N=N+1
	REPSW=.TRUE.
C	MAIN EXECUTION LOOP
1830	DO 2130 K=N,J,I
	IF (REPSW) L=K-1
	IF (IVALUE-10) 1870,1900,1840
1840	IF (IVALUE-15) 1910,1920,1850
1850	IF (IVALUE-17) 1930,2060,1860
1860	IF (IVALUE-21) 2070,2110,2540
C	ANALOG COMPONENT SELECTION STATEMENT
1870	IF (RSAC(2)) GO TO 1880
	IF (RSAC(3)) GO TO 1871
	IF (SAVESW) GO TO 1880
1871	IF (IVALUE.EQ.4.AND.MODE.EQ.7) GO TO 1890
1880	CALL RAVA(IVALUE,L,VALUE,ERROR)
	TYPE=-1
	GO TO 1901
C	SET A POT
1890	CALL SPOT(L,M,TOLER,ERROR)
	IF (ERROR.EQ.0) GO TO 2130
	TYPE=0
	GO TO 1905
C	A-TO-D STATEMENT
1900	CALL CRAC(L,VALUE,ERROR)
	VALUE=FLOAT(VALUE)/13.1072
	TYPE=1
C	ERRORZ SECTION
1901	IF (ERROR.NE.0) GO TO 1905
	IF (RSAC(2)) GO TO 1904
	IF (RSAC(3)) GO TO 1902
	IF (SAVESW) GO TO 1904
1902	VALUE=VALUE-M
	IF (TOLER-IABS(VALUE).GE.0) GO TO 2130
	ERRORS=.TRUE.
	IF (SWITCH.OR.RSAC(4).OR.RSAC(6)) GO TO 1903
	IF (ERRSW.AND..NOT.RSAC(5)) GO TO 1903
	IF (RSAC(1)) GO TO 1908
	GO TO 2130
1903	WRITE(OU,12050) CTYPE,L,VALUE
	IF (SWITCH.OR.RSAC(1).OR.RSAC(6)) GO TO 19031
	GO TO 2130
19031	IF (OU.NE.4) WRITE(4,12050) CTYPE,L,VALUE
	GO TO 1907
C	STATUS READOUT MODE
1904	WRITE(OU,11060) CTYPE,L,VALUE
	GO TO 2130
C	ERRORY SECTION
1905	ERRORS=.TRUE.
	IF (SWITCH.OR.RSAC(4).OR.RSAC(6)) GO TO 1906
	IF (ERRSW.AND..NOT.RSAC(5)) GO TO 1906
	IF (RSAC(1)) GO TO 1908
	GO TO 2130
1906	WRITE(OU,12060) CTYPE,L,ERROR
	IF (SWITCH.OR.RSAC(1).OR.RSAC(6)) GO TO 19061
	GO TO 2130
19061	IF (OU.NE.4) WRITE(4,12060) CTYPE,L,ERROR
1907	ANSWER=0
	CALL DECIDE
	IF (ANSWER) 1908,2130,1040
1908	IF (TYPE) 1880,1890,1900
C	D-TO-A STATEMENT
1910	CALL LTDA(L,M,ERROR)
	GO TO 2130
C	SENSE LINE STATEMENT
1920	Z=TRSL(L)
	IF (STATE) GO TO 1921
	IF (Z) GO TO 1922
	GO TO 2130
1921	IF (Z) GO TO 2130
1922	TYPE=2
	GO TO 2064
C	GENERAL PURPOSE INTERRUPT STATEMENT
1930	Z=TGPI(L)
	IF (STATE) GO TO 1931
	IF (Z) GO TO 1932
	GO TO 1940
1931	IF (Z) GO TO 1940
1932	VALUE=1
	GO TO 2050
1940	Z=.FALSE.
	CALL IGPI(L,HANDLE,ERROR)
	CALL DGPI(L,ERROR)
	IF (Z) GO TO 2031
	IF (STATE) GO TO 2040
	GO TO 2130
2031	IF (STATE) GO TO 2130
	VALUE=2
	GO TO 2050
2040	VALUE=3
2050	TYPE=3
	GO TO 2065
C	COMPARATOR STATUS STATEMENT
2060	Z=RSCS(L)
	IF (STATE) GO TO 2061
	IF (Z) GO TO 2062
	GO TO 2130
2061	IF (Z) GO TO 2130
2062	TYPE=1
2064	VALUE=1
C	ERRORT SECTION
2065	ERRORS=.TRUE.
	IF (SWITCH.OR.RSAC(4).OR.RSAC(6)) GO TO 2066
	IF (ERRSW.AND..NOT.RSAC(5)) GO TO 2066
	IF (RSAC(1)) GO TO 2067
	GO TO 2068
2066  WRITE(OU,12070) (MESS1(COL,TYPE),COL=1,5),L,(MESS2(COL,VALUE),
     1 COL=1,3)
	IF (SWITCH.OR.RSAC(1).OR.RSAC(6)) GO TO 20661
	GO TO 2068
20661 IF (OU.NE.4) WRITE(4,12070) (MESS1(COL,TYPE),COL=1,5),L,
     1 (MESS2(COL,VALUE),COL=1,3)
	ANSWER=0
	CALL DECIDE
	IF (ANSWER) 2067,2068,1040
2067	IF (IVALUE-16) 1920,1930,2060
2068	IF (IVALUE.EQ.16.AND.VALUE.EQ.1) GO TO 1940
	GO TO 2130
C	FUNCTION RELAY STATEMENT
2070	IF (STATE) GO TO 2080
	CALL SSRM(L,ERROR)
	GO TO 2090
2080	CALL SSRP(L,ERROR)
C	2 MILLISECOND PAUSE
2090	DO 2100 M=1,150
2100	CONTINUE
	GO TO 2130
C	CONTROL LINE STATEMENT
2110	IF (STATE) GO TO 2120
	CALL RSCL(L,ERROR)
	GO TO 2130
2120	CALL SSCL(L,ERROR)
2130	CONTINUE
	GO TO 1000
C	END OF DATA STATEMENT EXECUTION
C
C	END STATEMENT
2140	WRITE(4,10090)
	IF (OU.NE.4) WRITE(OU,10090)
	IF (IU.LT.4) CALL CLOSE(IU)
	IF (OU.LT.4) CALL CLOSE(OU)
C	CONTINUATION DIRECTIVE
2150	IF (RSAC(0)) GO TO 2151
	WRITE(4,10100)
	GO TO 2152
2151	WRITE(4,10101)
2152	WRITE(4,10000)
	READ(4,11000) I
	IF (I-1) 2160,2170,2180
C	CONTINUE
2160	IF (IU.LT.4) CALL SEEK(IU,INAME)
	IF (OU-4) 150,210,210
C	TERMINATE
2170	STOP 2
C	RESTART, CHANGE IU AND OU, ILLEGAL CONTINUATION DIRECTIVE
2180	IF (I-3) 10,20,2190
2190	WRITE(4,12020)
	GO TO 2150
C
C	INPUT ERRORS CONTROL
2500	I=1
	GO TO 2700
2520	I=2
	GO TO 2700
2540	I=3
	GO TO 2700
2560	I=4
	GO TO 2700
2600	INVARG(5)=MFIELD
	GO TO 2620
2610	INVARG(5)=NFIELD
2620	I=5
C	ERRORA SECTION
2700	WRITE(4,11040) (IERROR(J,I),J=1,8)
	IF (INPUT.NE.4) WRITE(4,11030) (CHAR(J),J=1,40)
	IF (OU.EQ.4) GO TO 2710
	WRITE(OU,11040) (IERROR(J,I),J=1,8)
	WRITE(OU,11050) (CHAR(J),J=1,40)
2710	INPUT=4
	IF (RSAC(0)) GO TO 2711
	WRITE(4,10110)
	GO TO 1010
2711	WRITE(4,10111)
	GO TO 1010
C	ABORTS
9990	IF (IU.LT.4) CALL CLOSE(IU)
	IF (OU.LT.4) CALL CLOSE(OU)
	IF (RSAC(7)) GO TO 2170
	IF (RSAC(8)) GO TO 10
	IF (RSAC(9)) GO TO 20
	GO TO 2150
C	END OF INPUT ERROR CONTROL
C
C	OUTPUT FORMATS (HYSAT DIRECTIVES)
10000 FORMAT(1H ,1H$)
10010 FORMAT(1H1,5HHYSAT)
10020 FORMAT(1H0,64HTYPE INPUT DIRECTIVE- 1-TTY,2-PAPER TAPE,3-DECTAPE,4
     1-CARD READER)
10021 FORMAT(1H0,3HIU-)
10030 FORMAT(1H ,16HMOUNT INPUT TAPE)
10040 FORMAT(1H ,38HTYPE UNIT NUMBER,FILE NAME- NFILENMEXT)
10041 FORMAT (1H ,11HNFILENMEXT-)
10050 FORMAT(1H0,66HTYPE OUTPUT DIRECTIVE- 1-TTY,2-PAPER TAPE,3-DECTAPE,
     14-LINE PRINTER)
10051 FORMAT(1H0,3HOU-)
10060 FORMAT(1H ,17HMOUNT OUTPUT TAPE)
10070 FORMAT(1H0,27HENGAGE PATCH PANEL FOR TEST)
10080 FORMAT(1H ,18HTYPE CR WHEN READY)
10081 FORMAT (1H ,3HCR-)
10090 FORMAT(1H0,11HEND OF TEST)
10100 FORMAT(1H0,28HTYPE CONTINUATION DIRECTIVE-/1H ,47H0-CONTINUE,1-TER
     1MINATE,2-RESTART,3-CHANGE IU/OU)
10101 FORMAT(1H0,13HCONTINUATION-)
10110 FORMAT(1H ,21HCORRECT STATEMENT(S)-)
10111 FORMAT(1H ,8HCORRECT-)
C
C	INPUT FORMATS
11000 FORMAT(I1)
11010 FORMAT(I1,A5,A4)
11020 FORMAT(72A1)
11030 FORMAT(1H ,72A1)
11040 FORMAT(1H ,5HCO **,8A5)
11050 FORMAT(1H ,3HCO ,40A1)
11060 FORMAT(1H ,A2,I3,I6)
C
C	OUTPUT FORMATS (ERROR MESSAGES)
12000 FORMAT(1H ,12H**ILLEGAL IU)
12010 FORMAT(1H ,12H**ILLEGAL OU)
12020 FORMAT(1H ,32H**ILLEGAL CONTINUATION DIRECTIVE)
12030 FORMAT(1H ,39H**IU AND OU CANNOT BOTH BE THE DCT-2000)
12040 FORMAT(1H ,2HCO,3A5,22HFAILED TO SET PROPERLY)
12050 FORMAT(1H ,13HCO COMPONENT ,A2,1X,I3,10H WRONG BY ,I6,11H MILLIVOL
     1TS)
12060 FORMAT(1H ,13HCO COMPONENT ,A2,1X,I3,16H GAVE ERROR NO. ,I1)
12070 FORMAT(1H ,3HCO ,5A5,1H ,I2,1H ,3A5)
C
99999 FORMAT (1H ,24HCONSOLE FAILED TO SELECT)
	END
