.001           /SAMPLING INTERVAL
130000.              /NUMBER OF SAMPLES IF NO S-S
.1              /UPPER BOUND IF S-S (NEG IF NO S-S WANTED)
-.1             /LOWER BOUND FOR S-S
5.              /REFERNCE VALUE FOR SYNCHRONIZATION OPTION
40              /NUMBER OF S-S'S WANTED
30              /CHANNEL NUMBER IF SYNCHONIZATION WANTED (NEG IF NOT)
30                 /INITIAL CHANNEL USED
 1                /NUMBER OF CHANNELS USED
F               /SEE OPTION
F               /PROGRAM INFORMATION FLAG
T               /BATCH MODE FLAG
F               /NO CLOCK FLAG
T               /BOUNDARY FLAG FOR S-S: T=OUTSIDE; F=INSIDE BOUNDARY
