ENGINEERING COMPUTER CENTER 
===========================
 
LIBRARY DUMP TAPE
-----------------
 
THE LIBRARY DUMP TAPE IS A LIBRARY OF USER PROGRAMS
AND SUBROUTINES, PLACED THERE BY THE ECC AND VARIOUS
USERS WHO FELT THAT THEY HAD A PROGRAM OR ROUTINE
OF USE TO OTHER USERS, WITH THE AIM OF PROMOTING SOFTWARE
DEVELOPMENT IN COMPUTER GRAPHICS AT THE UNIVERSITY OF
WATERLOO.
 
TO INCLUDE A PROGRAM ON THIS TAPE,TRY TO MAKE THE PROGRAM
AS BUG FREE AS POSSIBLE, BEING LIBERAL WITH COMMENT 
STATEMENTS THROUGHOUT.  AT THE HEAD OF EACH PROGRAM
SHOULD BE A COMMENT PARAGRAPH, EXPLAINING PURPOSE
OF THE PROGRAM, NATURE OF INPUT ARGUEMENTS, IF ANY; AND
THE NAME OF THE ORIGINAL PROGRAMER,DEPARTMENT, AND DATE
OF CREATION.  FINALLY,THE PROGRAM NAME SHOULD BE INCLUDED
IN THE 'INDEX' FILE, WITH A BRIEF DESCRIPTION.
 
NOTE:  SOURCE VERSIONS OF PROGRAMS ONLY!!!
       NO BINARY VERSIONS TO BE PLACED ON LIBRARY DUMP TAPE
  
 
FOLLOWING IS THE INDEX FOR THE ECC LIBRARY DUMP TAPE:
 
**********************************************************
 
	INDEX SRC	-THIS FILE, AN INDEX OF THE ECC
			LIBRARY DUMP TAPE.
	DEMO1 SRC	-A DEMONSTRATION OF TWO DIMENSIONAL
			GRAPHICS PROGRAMMING.
	DEMO2 SRC	-A DEMONSTRATION OF THREE DIMENSIONAL
			GRAPHICS PROGRAMMING.
	DEMO3 SRC	-A DEMONSTRATION OF DISPLAY FILE
			MANAGEMENT SUBROUTINES.
	MENU SRC	-A SUBROUTINE THAT DISPLAYS PAGES
			OF TEXT MATERIAL CREATED BY MENUX
			THAT FOLLOWS.
	MENUX SRC	-A PROGRAM, THAT, AS DESCRIBED IN
			ECC HANDBOOK, GENERATES DISPLAY
			FILES CONSISTING OF STRINGS OF
			CHARACTERS.
	BOX SRC		-A SUBROUTINE FOR INPUTING INTEGER
			NUMBERS FROM THE FUNCTION BOX.
	SPACE1 SRC	-A VERSION OF SPACE WAR,A REAL
			TIME COMPUTER GRAPHICS DEMONSTRATION
			GAME.
	STMAP SRC	-A STEREOSCOPIC VISION VERSION
			OF THE SYSTEM PROGRAM 'MAPPER'
			USED INCONJUNCTION WITH STDRW &
			STEREO, ALSO ON THIS TAPE.
	STDRW SRC	-A 'VECTOR' & 'DISPLY' CALLING
			SUBROUTINE FOR DISPLAYING THE STEREOSCOPIC
			IMAGES GENERATED BY 'STMAP'.
	STEREO		-COMPLETE STEREOVISION PROGRAM TO
			FACILITATE THE USE OF 'ROTER','STMAP','STDRW'
			WITHOUT HAVING TO CALL THEM INDIVIDUALLY.
       CAMERA          - A ROUTINE THAT CONTROLS THE BOLEX 16 MM
                       MOVIE CAMERA. IT ACCEPTS 9 COLOURS
                       AND 4 TINT LEVELS
                       THE CAMERA IS AUTOMATICALLY
                       ADVANCED, OR FRAMES CAN BE OVER
                       WRITTEN
       MENUW           - IS THE WATRAN VERSION OF MENU
       BOXW            - IS THE WATRAN VERSION OF BOX
