	.TITLE ERRSET	-ARITH. ERROR MSG. PRINT CONTROL
/ 
/ 
/                   FIRST PRINTING, FEBRUARY 1974
/ 
/ THE INFORMATION IN THIS DOCUMENT IS SUBJECT TO 
/ CHANGE WITHOUT NOTICE AND SHOULD NOT BE CONSTRUED
/ AS A COMMITMENT BY DIGITAL EQUIPMENT CORPORATION.
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPON-
/ SIBILITY FOR ANY ERRORS THAT MAY APPEAR IN THIS
/ DOCUMENT.
/ 
/ THE SOFTWARE DESCRIBED IN THIS DOCUMENT IS FUR-
/ NISHED TO THE PURCHASER UNDER A LICENSE FOR USE ON
/ A SINGLE COMPUTER SYSTEM AND CAN BE COPIED (WITH
/ INCLUSION OF DIGITAL'S COPYRIGHT NOTICE) ONLY FOR 
/ USE IN SUCH SYSTEM, EXCEPT AS MAY OTHERWISE BE PRO-
/ VIDED IN WRITING BY DIGITAL.
/ 
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPONSIBILITY
/ FOR THE USE OR RELIABILITY OF ITS SOFTWARE ON EQUIP-
/ MENT THAT IS NOT SUPPLIED BY DIGITAL.
/ 
/ COPYRIGHT (C) 1974, BY DIGITAL EQUIPMENT CORPORATION
/ 
/ 
        .EJECT
/COPYRIGHT 1971, DIGITAL EQUIPMENT CORP.,MAYNARD, MASS.
	.GLOBL ERRSET,.AERTB,.DA
/CALLING SEQUENCE:      CALL ERRSET(N)---N IS INTEGER ARG.
/	JMS* ERRSET
/	JMP .+2
/	CAL/XCT ADDR	ADDR OF ARG.(XCT IF INDIRECT
ERRSET	0
	JMS* .DA
	JMP .+2
ERRCNT	0		/ADDR OF ARG
	LAC .AERTB	/INIT PTR AND CNT.
	DAC ERRSE1
	LAW -10
	DAC ERRSE2
	LAC* ERRCNT	/GET ARG.  SET TABLE ENTRIES IN OTSER
/TO -N-1 IF N IS .GE. 0.  SET TO -1(I.E. ASSUME N=0) IF N .LT. 0
	CMA
	SMA
	CLC
ERRAG	DAC* ERRSE1	/LOOP
	ISZ ERRSE1
	ISZ ERRSE2
	JMP ERRAG	/AGAIN
	JMP* ERRSET	/EXIT
ERRSE1	0	/PTR.
ERRSE2	-10	/LOOP CNT(8(10) OTS MSG.)
	.END
