	.SYSID <	.TITLE DTE. >,< 108>
/
/COPYRIGHT (C) 1975
/DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASS.
/
/THIS SOFTWARE IS FURNISHED UNDER A LICENSE FOR USE ONLY
/ON A SINGLE COMPUTER SYSTEM AND MAY BE COPIED ONLY WITH
/THE INCLUSION OF THE ABOVE COPYRIGHT NOTICE.  THIS
/SOFTWARE, OR ANY OTHER COPIES THEREOF, MAY NOT BE PRO-
/VIDED OR OTHERWISE MADE AVAILABLE TO ANY OTHER PERSON
/EXCEPT FOR USE ON SUCH SYSTEM AND TO ONE WHO AGREES TO
/THESE LICENSE TERMS.  TITLE TO AND OWNERSHIP OF THE
/SOFTWARE SHALL AT ALL TIMES REMAIN IN DEC.
/
/THE INFORMATION IN THIS DOCUMENT IS SUBJECT TO CHANGE
/WITHOUT NOTICE AND SHOULD NOT BE CONSTRUED AS A COM-
/MITMENT BY DIGITAL EQUIPMENT CORPORATION.
/
/DEC ASSUMES NO RESPONSIBILITY FOR THE USE OR RELIABILITY
/OF ITS SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.
	.EJECT
/ 107	06-JUN-75 (RCHM)	MAKE XVM CHANGES.
/ 108	12-NOV-75 (RCHM)	ONE LAST TIME FOR THE IOPS67 BUG.
/M. SIFNAS
/10-8-70	EDIT 6
/8-26-70 (SWITCH CLEARING ON ERRORS SO CAN RESTART ON ^P)
/9-16-69 (TIMING BUG, REMOVAL OF XX ON IOPS15)
/P OLYNK (.MTAPE DELETE 7-28-69)
/ 4-9-68 (IOPS 23 5-8-68)(56 FILES 5-8-68)
/(EOF 5-22-68) (PARITY 6-3-68)
/DTE.=IOPS DECTAPE HANDLER-READ, WRITE, ALL MODES
/ALL FUNCTIONS EXCEPT .MTAPE
/1-256 WD. BUF.
/1 FILE BIT MAP (32 WDS) + 1 DIRECTORY BIT MAP (32 WDS)
/1 FILE ACTIVE AT ANY GIVEN TIME
/CALLING SEQUENCE
/CAL+.DAT SLOT(9-17)+I(7-8)/.INIT
/UNIT (0-2)+1
/RESTART ADDR. (ONLY MEANINGFUL FOR TTY HANDLER)
/BUF SIZE (255)
/CAL+X(6-8)+.DAT SLOT (9-17) /.OPER	(X=1=.DLETE)
/UNIT (0-2)+2		(X=2=.RENAM)
/			(X=3=.FSTAT)
/DIR TYPE(0-2)=1+CORE ADDR. (3-17)
/CAL+.DAT SLOT (9-17)  /.SEEK
/UNIT (0-2)+3
/USER DIRECTORY ENTRY POINTER
/SAME AS .SEEK(FUNCTION=4) /.ENTER
/CAL+.DAT SLOT (9-17)  /.CLEAR
/UNIT(0-2)+5
/CAL+.DAT SLOT(9-17)  /.CLOSE
/UNIT(0-2)+6
/CAL+SUBFUNCTION(5-8)+.DAT SLOT /.MTAPE (0=REWIND)            (ILLEGAL FUNCTION)
/UNIT(0-2)+7			(2=BACKSPACE RECORD)  (ILLEGAL FUNCTION)
/CAL+D.M.(6-8)+.DATSLOT(9-17)  /.READ
/UNIT (0-2)+10
/LINE BUF ADDR
/-WC OF L.B. (2'S COMP)
/SAME AS .READ(FUNCTION=11)  /.WRITE
/CAL+.DAT SLOT(9-17)	/.WAIT
/UNIT(0-2)+12
/CAL+1000+.DAT SLOT(9-17)		/.WAITR
/UNIT(0-2)+12
/15BIT BUSY ADDR
/CAL+Y(7)+X(8)+.DAT SLOT (9-17) /.TRAN	(X=0=READ)(Y=0=FORWARD)
/UNIT (0-2)+13			(X=1=WRITE) (Y=1=REVERSE)
/BLOCK#
/CORE ADDRESS
/-WC
/
	.EJECT
	.GLOBL	DTE.
.MED=3
/IOT ASSIGNMENTS
DTCA=707541
DTXA=707544
DTLA=707545
DTRA=707552
DTEF=707561
DTRB=707572
DTDF=707601
DELTA=5
DTE.	DAC	DTCALP		/CAL POINTER
	DAC	DTARGP		/ARG. POINTER
	LAC* DTCALP			/.DAT SLOT IN BITS 9-17.
	AND (777
	DAC DATSLT		/SAVE FOR COMPARISON WITH PREVIOUS .DAT SLOT.
	LAW	7000
	AND*	DTCALP		/(6-8) TO (15-17)
	RAR!CLL
	RTR
	RTR
	RTR
	RTR
	DAC	DTCT		/T STORE DATA MODE OR SUBFUNCTION
	ISZ	DTARGP		/INDEX TO FUNCTION (AND UNIT#)
	LAC*	DTARGP
	AND	DTUMSK
	DAC	DTUNIT		/T. SAVE UNIT#
	LAC*	DTARGP		/FUNCTION (3-17)=1-13
	ISZ	DTARGP		/INDEX TO ARG.3
	AND	(77
	DAC DTSTPA		/TEMP STORAGE OF FUUCTION.
	TAD	(JMP DTTABL
	DAC	DTTABL
	LAC DATPST		/SEE IF TRYING TO USE MORE THAN 1 .DAT SLOT
	SAD DATSLT		/(THEREFORE HAVING MORE THAN 1 FILE OPEN CONCURRENTLY).
	JMP DTTABL-1		/NO - OK.
	SNA
	JMP FIXDAT		/IF 0, FIRST TIME THRU OR ON AN .INIT.
	LAW -3
	TAD DTSTPA		/ALLOW THE FOLLOWING FUNCTIONS THRU:
	SPA			/.INIT,.OPEN, .WAIT AND .TRAN.
	JMP FIXDAT
	TAD (-7
	SMA
	JMP FIXDAT
DTER17	JMS DTIOU		/CAN'T LEAVE ON ERROR TILL NOT BUSY.
	LAW 17			/IOPS 17: TOO MANY FILES.
	JMP DTEROT
FIXDAT	LAC DATSLT		/OK - RESET PAST .DAT SLOT.
	DAC DATPST
	CLA			/AC MUST=0 FOR DISPATCH
	.EJECT
DTTABL	XX
	JMP	DTIN	/1=.INIT
	JMP	DTOPER	/2=.OPER
	JMP	DTSEEK	/3=.SEEK
	JMP	DTENTR	/4=.ENTER
	JMP	DTCLER	/5=.CLEAR
	JMP	DTCLOS	/6=.CLOSE
	JMP	DTER6	/7=.MTAPE
	JMP	DTREAD	/10=.READ
	JMP	DTWRIT	/11=.WRITE
	JMP	DTWAIT	/12=.WAIT,.WAITR
	JMP	DTAPE	/13=.TRAN
DTBUSY	LAC	DTCALP		/BUSY-DTA I/O GOING ON
	DAC	DTARGP		/RETURN TO USER CAL
	JMP	DTDBK
/I/O UNDERWAY CHECK SUBR.
DTIOU	0
	LAC	DTUND		/I/O UNDERWAY
	SZA			/NO
DTBUSB	JMP	DTBUSY		/WAIT
	LAC	DTWRWT		/CONTINUE MORE I/O
	SZA!CMA
	JMP*	DTWRWT		/YES
	JMP*	DTIOU		/OK-EXIT
IOPS67	LAW 67			/(RCHM-106) FETCH ILLEGAL MEMORY MESSAGE NUMBER.
	JMP DTEROT		/(RCHM-106) GO PRINT MESSAGE.
/
	.EJECT
/DTA INTERRUPT SERVICE
DTINT	JMP DTPIC		/PIC ENTRY.
	DAC DTAC		/PIC ENTRY
	LAC DTDVSW-1	/LEAVE PIC ALONE ON EXIT
	DAC DTDVSW
	LAC	DTINT		/API PC, L, EM, MP
	JMP DTCOM
DTPIC	DAC	DTAC		/SAVE AC
	LAC (ION		/TURN ON PICAT EXIT
	DAC DTDVSW
	LAC*	(0	/PIC PC,L,EM,MP
DTCOM	DAC DOUT		/SAVE FOR EXIT
	LAC	DTUND		/I/O UNDERWAY SWITCH STILL ON?
	SZA			/NO-STOP TAPE
	JMP	DTRBB
	DTLA			/CLEAR CONTROL
	JMP	DTDISM
/STATUS B-0=EF
/	1=MK. TK. ERR.
/	2=EOT
/	3=SELECT ERR
/	4=PARITY ERR.
/	5=TIMING ERR.
/	11=DTF
/STATUS A-0-2=UNIT#
/	3=FORW.(0),REV(1)
/	4=GO(1),STOP(0)
/	5=NORM.(0),CONT.(1)
/	6-8=FUNCTION
/	9=DISABLE DTF,EF(0),ENABLE(1)
/	10=CLEAR EF(0)
/	11=CLEAR DTF(0)
DTRBB	DTRB			/READ DTA STATUS B
	SMA
/DTDIS = JMP DTSRCK ON SEARCH
/DTDIS = JMP DTRDWT ON READ OR WRITE
DTDIS	XX
	AND	(330000
	SZA!RTL			/SELECT ERROR
/DTERJ=	JMP	DTERS		/ON SEARCH
/	JMP	DTERT		/ON READ OR WRITE
DTERJ	XX
	DTRA
	AND DTLNOP		/740000
	DAC	DTT2		/SAVE STATUS A
	DTLA+10			/CLEAR A,FLAGS,DISABLE FROM INT.
	LAC	(DTRYAG		/GO TO .MED FOR MANUAL READY
	DAC*	DLIT3		/(.MED)
	DZM	DTUND		/SO CAN RESTART WITH ^P.
	LAC	DLIT4
	JMP*	DLIT4		/(.MED+1)
DTRYAG	LAW	-1
	DAC	DTUND		/RESET I/O UNDERWAY SWITCH.
	JMS DTSRCH		/SET UP FOR SEARCH
	LAC DTT2
	XOR (21400
	JMP	DTXIOT		/EXECUTE IOT AGAIN
/
/ERROR IN SEARCH MODE
DTERS	SPA
	JMP	DTEOT		/EOT-CHANGE DIRECTION
	SNL			/MK .TK. ERR. IRREC.
	JMP	DTRWEN		/TIMING ERR.-TRY AGAIN(SETTING GO BIT)
DTERS1	DTRA		/GET UNIT #
	RTL
	RTL
	AND (7		/INTO 15-17
	DTRB-10		/IOR STATUS B
	DAC*	DLIT3		/(.MED=3)
	CLA			/IRREC. DTA ERROR
	JMP	DTER12		/MK. TK. OR EOT DURING READ OR WRITE
/
/ERROR DURING READ OR WRITE
DTERT	SZL!SPA!RTL		/PARITY OR TIMING
	JMP	DTERS1		/MK. TK. OR EOT DURING TRANSFER
	SMA!STL			/PARITY
	JMP	DTTIM		/TIMING ERROR. (LINE MUST BE 1)
DTPART	ISZ	DTERCT		/INDEX PARITY ERROR CT.
	JMP DTTIM-1		/TRY AGAIN
	LAC* (30		/WC OVERFLOW?
	SMA		/NO, MUST GET REST OF DATA
	JMP DTRDWT	/ACCEPT DATA AS IS
	DAC DTCCA	/TEMP STORE REMAINDER
	LAC DTWC	/(ORIG WC - REMAINDER)
	CMA!STL		/LINK WILL BE COMPLEMENTED ON TAD DTCCA
	TAD DLIT1
	TAD DTCCA
	RTR
	RTR
	RTR
	RTR
	TAD DTBLC	/FORMER BLK #
	DAC DTBLC	/NEW BLK #
	LAC DTCCA	/RESET WC FOR REMAINDER
	DAC DTWC
	LAC* (31	/RESET CURR ADDR
	DAC DTCCA
	LAW -10		/RESET PARITY RETRY COUNT
	DAC DTERCT
	.EJECT
	CLL			/LINK MUST BE 0 FOR PARITY ERROR
DTTIM	JMS	DTSRCH		/SET UP FOR SEARCH
	LAC	DTTR		/CLEAR OUT READ OR WRITE BITS
	SZL			/PARITY
	XOR	(20000		/SET GO BIT IF TIMING
	DTXA
	JMP	DCHK2		/SEARCH AGAIN FOR RETRY
DTRDWT	DZM	DTUND		/CLEAR I/O UNDERWAY
	DZM	DTEOTZ		/SET DOUBLE ENDZONE SWITCH
L7777	LAW	-100		/WAS DIR. (BL 100) READIN
	TAD	DTBLC
	SZA
	JMP	DTRWEN		/YES
	LAC	DTDRGT		/GET DIR SWITCH SET
	SZA!CLC			/YES-CLEAR
	JMP	DTRWEN
	DAC	DTDRGT
	LAC	DTUNIT		/UNIT# IN BITS 0-2
	DAC	DTNCOR		/SET DIR IN CORE SW.
DTRWEN	LAC	(20000		/CLEAR (SET IF TIMING) GO BIT
	JMP	DTXIOT
/SEARCH INTERRUPT SERVICE
DTSRCK	CLC
	DAC	DTEOTZ		/CLEAR DOUBLE END ZONE SWITCH
	LAC	DTBCA		/BLK# JUST READ
	SAD	DTBLC		/BLK SEARCHED FOR
	JMP	DCHKF		/MAYBE-CHECK DIRECTION
	CMA
	TAD	DTBLC		/BLK# SEARCHED FOR-BL# READ
DCHKC	SMA!CLA			/OVERSHOOT-FORW; SPA!CLA=REV.
	JMP	DTXIOT		/CONT. SEARCH, SAME DIRECTION
DTEOT	DAC	DTEOTS		/SET (0) OR CLEAR (-) EOT SWITCH
DCHK2	LAC	DTBLNC		/FORW: SUB. 2 FROM BL# TO SEARCH
DCHKC3	TAD	DTNXBK		/REV; AND 2 FROM BL# TO SEARCH
	DAC	DTBLC
	CLC			/CHANGE SIGN OF BLK INCR.
	TAD	DTBLNC		/FOR NEXT DIRECTION CHANGE
	CMA
	DAC	DTBLNC
	LAC	DTEOTS		/END ZONE ENTERED SWITCH
	SMA
	JMP	DCHKC4		/NO ENTERED
	ISZ	DTEOTZ		/DOUBLE END ZONE SWITCH SET
	JMP	DCHKC4		/NO
	LAC	DTNXBK		/STORE BL# TO TRANSFER
	DAC	DTBLC		/INTO BL# TO SEARCH FOR
	.EJECT
/THIS ROUTINE INSURES CORRECT SETTING OF DTBLC
/ON 1ST ENTRY INTO END ZONE
DCHKC4	LAC	DCHKC
	XOR	(1000		/OR VICE VERSA
	DAC	DCHKC
	LAC	DTEOTS		/EOT SWITCH
	RAL			/L = 1 = EOT
	LAC (40000		/MOTION BIT
	SZL			/NO EOT
	XOR	(20000		/SET GO BIT
	DZM	DTEOTS		/CLEAR EOT SWITCH
	JMP	DTXIOT		/CHANGE SEARCH DIRECTION
/SET UP FOR SEARCH MODE
DTSRCH	0
	LAC	(DTBCA		/SET UP CA AND WC
	DAC*	(31		/FOR SEARCH
	DZM*	(30
	LAC	(JMP DTSRCK	/SET UP INT. SERVICE
	DAC	DTDIS		/FOR SEARCH
	LAC	(JMP DTERS
	DAC	DTERJ
	JMP*	DTSRCH
DCHKF	LAC	DTDTR
	XOR	DTBLNC
DLITSM	SMA!CLA			/SEARCH DIRECT.=TRANSF. DIR.
	JMP	DCHKC3		/CHANGE SEARCH DIR. AGAIN
	LAC	DTWC		/SET UP-WC
	DAC*	(30
	LAC	DTCCA		/CA-1
	DAC*	(31		/FOR TRANSFER
	LAC	(JMP DTRDWT	/SET UP TRANSFER COMPLETE JMP
	DAC	DTDIS
	LAC	(JMP DTERT		/SET UP ERROR JMP
	DAC	DTERJ
	LAC	DTTR		/READ (13000) OR WRITE (15000)
DTXIOT	DTXA
DTDISM	LAC	(JMP DTPIC	/RESTORE PIC INTERR. ENTRY
	DAC	DTINT
	LAC	DTAC		/RESTORE AC
DTDVSW	XX		/ION IF PIC, LAC DTAC IF API
	DBR
	XCT .+1
	XCT .+1
	JMP*	DOUT		/INTERR. EXIT
/
/INIT DTA ROUTINE - MAINSTREAM
DTIN	ISZ	DTARGP		/INDEX TO BUF. SIZE ARG.
	LAC	(377		/RETURN 255 AS BUF. SIZE
	DAC*	DTARGP
	LAC	DTCT		/I OR O
	DAC	DTIOSW		/OUTPUT=1, INPUT=0
	ISZ	DTARGP		/INDEX TO NORM. EXIT
	LAC	DLMBIT		/(DTMBIT) = FILE BIT MAP POINTER
	JMS	DTBFC2		/CLEAR FILE BIT MAP (L=0)
DTONCE	CAL	44		/API CORE ADDR.-MODIFIED
/DTONCE+1 TO 11 USED FOR TEMP. STORE. AFTER 1ST .INIT
/DTAC=AC STORAGE CELL DURING INTERRUPT
/DOUT=INTERRUPTED RETURN ADDRESS
/DTT2=STATUS A STORAGE CELL
/DTBCA=BL.# STORAGE CELL DURING SEARCH
/DTERCT=PARITY COUNTER (INIT. TO-10)
/DTBLC=BL# BEING SEARCHED FOR
/DTBLNC=BL. INCR. TO CHANGE DIRECTION,-2=F,+2=R.
/DTNXBK=BL.# TO BE TRANSFERRED
/DTDTR=TRANSFER DIRECTION SWITCH, 0=F,-1=R
DTAC	16			/.SETUP
DOUT	DTDF			/DONE FLAG
DTT2	DTINT			/DTA INT. SERV. ADDR.
DTBCA	CAL	44
DTERCT	16
DTBLC	DTEF			/ERR. FLAG
DTBLNC	DTINT
DTNXBK	LAC	DJSTOP
DTDTR	DAC	DTONCE
DTBMIN=DTFAKE			/BIT MAP BLOCK IN SWITCH (NON0=IN)
DTBMOT=DTFAKE+1			/BIT MAP BLOCK OUT SWITCH (NON0=OUT)
DTSTOP	JMS	DTSTPA
	JMP	DTDBK
/STOP DTA ROUTINE
DTSTPA	0
	DZM DATPST
	DZM	DTWRWT		/CLEAR OUTPUT WAIT SWITCH
	DZM	DTEOF		/CLEAR EOF SWITCH
	DZM	DTCLSS		/SET CLOSE SWITCH
	DZM	DTSKNT		/CLEAR .SEEK, ENTER SWITCH
	DZM	DTWREX		/CLEAR WRITE  EXECUTED SWITCH
	DZM	DTBMIN		/BIT MAP IN SWITCH (FOR CLOSE)
	DZM	DTBMOT		/BIT MAP OUT SWITCH (FOR CLOSE)
	LAC	DTMTP4		/JMP DTAPE1
	DAC	DTOUT
	DAC	DTNCOR		/CLEAR DIR. IN CORE SWITCH
	LAC	DTWRCL		/INIT DUMP MODE WRITE
	DAC	DTDUMX		/TO CLEAR OUT BUF (JMS DTBUFC)
	JMP*	DTSTPA
/WAIT DTA ROUTINE
DTWAIT	SAD DTCT		/1 IF .WAITR
	JMP DTDBKW	/0 IF .WAIT
	LAC (700000	/LINK,ETC
	AND DTCALP
	DAC DTCALP
	LAC* DTARGP	/15 BIT BUSY ADDR
	AND (77777
	XOR DTCALP
	ISZ DTARGP
	DAC DTCALP
DTDBKW	JMS	DTIOU		/CHECK I/O UNDERWAY
DTDBK	DBR
	XCT .+1
	XCT .+1
	JMP*	DTARGP		/NORM. EXIT
/
/.OPER ROUTINE INTERPRETS
/.DLETE (SUBFUNCTION 1)
/.RENAME (SUBFUNCTION 2)
/.FSTAT (SUBFUNCTION 3)
DTOPER	LAC	DTDLUN		/DELETE OR RENAM UNDERWAY
	SZA			/NO, IF 1ST PASS THRU
	JMP	DTLET3		/YES
	JMS	DTCKCL		/CHECK DIRECTORY FOR THIS FILE
	DAC	DTNXBK		/SAVE FOR 0 AC WHEN NOT FOUND
	SNA
	JMP	DTFST		/NOT FOUND-RETURN WITH AC=0
	XCT	DTSK5		/PICK UP 1ST BLK# OF FILE
	XOR	(400000		/CLEAR FILE COMPLETE BIT
	DAC	DTNXBK		/1ST BLK# OF FILE
	LAC	DTCT		/SET UP SUBFUNCTION DISPATCH
	TAD	(JMP DTOPTB
	DZM	DTESAV		/SETUP FOR DELETE
	DZM	DTESAV+1
	DZM	DTESAV+2
	DZM	DTESAV+3
	DAC	DTOPTB-1
	LAW	-4
	TAD	DTCT		/CHECK SUBFUNCTION
	SPA!CLA			/1-3 LEGAL ONLY
	XX			/DISPATCH TO SUBFUNCTION
DTOPTB	JMP	DTER6		/ILL. HANDLER FUNCTION
	JMP	DTLET		/1= .DLETE
	JMP	DTREN		/2=.RENAM
DTFST	LAC*	DTARGP		/3=.FSTAT
	XOR	(100000		/RETURN TYPE (1 IN 0-2)
	DAC*	DTARGP 		/TO USER
	LAC	DTNXBK		/PICK UP BL#, RETURN TO USER IN  AC
	DZM	DTCLSS
	JMP	DTAPE1
/.RENAM ROUTINE
DTREN	JMS	DTNTRZ		/NEW NAME INTO DTESAV
	XCT	DTSK5		/GET 4TH WD OF OLD ENTRY
	XCT	DTNTR3		/SAVE IN DTESAV+3
	DAC	DTBMIN		/NO NEED TO RERECORD
	DAC	DTBMOT		/FILE BIT MAPS
	.EJECT
/.DELETE ROUTINE
DTLET	CLC
	DAC	DTNCOR
	DAC	DTDLUN	/SET DELETE UNDERWAY SWITCH
	DAC	DTIOSW		/SIMULATE WRITE
	DAC	DTWREX		/USE .CLOSE TO MODIFY
DTLET3	ISZ	DTARGP		/INDEX ENTRANCE ARG. POINTER
	JMP	DTCLOS		/FILE BIT MAP+DIRECTORY
/CHECK DIRECT. IN CORE SUBR.
DTDRCK	0
	JMS	DTIOU		/I/O UNDERWAY
	LAC	DTNCOR		/D IN 
	SAD	DTUNIT		/NO
	JMP	DTDRC1		/YES - CHECK PARITY
DTDRC2	LAC	(13000		/READ PARAM
	JMS	DTDRIN		/BRING IN DIRECTORY
	JMP	DTDRCK+1		/WAIT FOR DIRECTORY
DTDRC1	LAC	DTERCT		/DIRECTORY UNACCEPTABLE WITH PARITY ERR.
	SZA
	JMP*	DTDRCK
DTER61	LAW	61		/DIRECTORY OR FILE BIT MAP PARITY ERROR
	JMP	DTEROT
/CALL IN DIRECTORY SUBR.
DTDRIN	0
	DAC	DTTR		/TRANSFER DIRECTION SWITCH
	LAC	DLT100		/(100
	DAC	DTNXBK		/BL# TO TRANSFER
	DZM	DTDTR		/TRANSFER FORWARD
	DZM	DTDRGT
	LAC	DTCLSS		/0 IF SEEK, ENTER
	SZA
	LAC	(40		/NOT 0 IF CLOSE (DTBUF-1
	TAD	DLTDR1		/(DTRDIR-1
	JMS	DTWCS		/SETUP WC,CA
	JMP*	DTDRIN
DTDRGT	777777			/GET DIR INDIC. (+0=GET)
/DIRECTORY SEARCH SUBR.
DTSK1	0
	DAC	DTUDRR		/USER DIR. ENTRY POINTER
	DZM	DTDTR		/SET TRANSF. DIRECTION=FORWARD
	CLC		/SYSTEM TAPE?
	XOR* DLTSYS		/WD3 0F SYS BIT MAP
	SNA!CLA		/NO, 56 FILES
	LAW -30		/YES, 24 FILES MAX
	SMA
	LAW -70
	DAC	DTFPCT
	XOR L7777		/777700
	DAC DBLKLC	/50 IF 24;10 IF 56
	LAC	DLTBUF		/DIR. POINTER=DTDIR+40=DTBUF
DTSK3	DAC	DTDES		/ENTRY SECTION POINTER
	DAC	DTCURE		/CURR. ENTRY, WD0, POINTER
	.EJECT
/NEXT FILE NAME ENTRY
	LAC	DTUDRR		/USER DIR. ENTRY POINTER
	DAC	DTUDRP
	LAW	-4
	DAC	DTCT1S		/MATCH COUNT
	DAC	DTCTS		/COUNT OF ENTRY WDS TO CHECK
	ISZ	DTCTS
/NEXT WORD OF CURRENT ENTRY
DTSK5	LAC*	DTDES		/DTA DIR. ENTRY (D.E.)
	SAD*	DTUDRP		/USER D.E.
	ISZ	DTCT1S		/WD N OF ENTRY MATCHES
	ISZ	DTDES		/NEXT WD OF DTA ENTRY
	ISZ	DTUDRP		/NEXT WD OF USER ENTRY
	ISZ	DTCTS		/ENTRY WD COUNT
	JMP	DTSK5		/CONT. MATCH CHECK
DTSK6	LAC	DTCURE
	ISZ	DTCT1S		/MATCH
	SKP			/N
	JMP*	DTSK1		/YES-1ST BL# IN AC
	TAD	DLIT4		/INDEX TO NEXT ENTRY
	ISZ	DTFPCT		/INDEX FILE ENTRY CT.
	JMP	DTSK3		/NEXT ENTRY
	CLA
	JMP*	DTSK1		/YES-CAN'T FIND FILE NAME
/
/CLOSE FILE SUBR
DTCLOS	JMS	DTIOU		/I/O UNDERWAY WAIT
	LAC	DTIOSW		/I OR O
	SNA
DJSTOP	JMP	DTSTOP		/INPUT-CLEAR SWITCHES EXIT
	LAC	DTWREX		/ANYWRITE EXECUTED AFTER .ENTER
	SZA
	JMP	DTCLS2		/YES
	JMS	DTCBIT		/NO-CLEAR BIT FROM MAPS
	JMP	DTSTOP
DTCLS2	LAC	DTEOF		/EOF BUF IS OUT
	SPA!CLC
	JMP	DTCLS3
	DAC	DTEOF		/SET EOF SWITCH
	DZM	DTCT		/FAKE DATA MODE=IOPS BIN
	LAC (SKP!CLA)		/(RCHM-108)
	DAC CL.SW		/(RCHM-108)
	LAC (15000)		/OUTPUT
	JMS	DTMCK
	LAC	DLEOFH		/EOF HEADER POINTER (DTEOFH
DTROOM	377		/DUMP MODE BUF SIZE(INIT=377)
/PRECEDING LINE=FAKE ARG,USED AS VARIABLE
	JMP	DTWRT1
	.EJECT
DTCLS3	LAC	DTBMIN	/CHECK IF FILE BIT MAP IS IN
	SZA!CLC
	JMP	DTCLS4
	DAC	DTBMIN		/SET BIT MAP IN SWITCH
	LAW -50		/START WITH BLK 77 IF 56 FILES,73 IF 24
	TAD DBLKLC	/50 IF 24;10 IF 56
	SNA!CLA		/56
	LAW -4		/24
	TAD DLIT77
DTCLT	DAC	DTNXBK		/BIT MAP BLOCK #
	LAC	DTFPCT		/FILE COUNT
	TAD	(10
	DAC	DTFPCT
	SMA!CLC
	JMP	DTCLQ		/IN THIS BLOCK
				/DECR. BIT MAP BLOCK # BY 1
	TAD	DTNXBK
	JMP	DTCLT
DTCLQ	LAC	DTBUSB
	DAC	DTOUT
	DZM	DTDTR		/SET TRANSF. DIRECT. SWITCH TO FORW.
	LAC	(13000
DTCLQ1	DAC	DTTR
	JMP	DTCOUB		/READ BIT MAP BLOCK INTO BUF. AREA
DTCLS4	LAC	DTBMOT		/FILE BIT MAP BLOCK OUT
	SZA!CLA
	JMP	DTCLS6
	SAD	DTERCT		/SET BIT MAP OUT SWITCH
	JMP	DTER61		/PARITY ERR ON FILL BIT MAP
	LAC	DTFPCT		/REL. BIT MAP POINTER
	CLL!RAL			/X 40
	RTL
	RTL
	TAD	DLTBUF		/(DTBUF
	DAC	DTBMOT		/SET BIT MAP OUT SWITCH
DTOLBM=DTOBCK			/REL. BIT MAP ADDRESS
DTXROL=DTMPS			/OLD BIT MAP POINTER
	DAC	DTOLBM
	DAC	DTXROL		/OLD BIT MAP ADDR.
	LAC	DLTDIR		/DIR. BIT MAP ADDR. 
	JMS	DTXOR		/XOR OLD FILE BIT MAP INTO DIR. BIT MAP
	LAC	DLMBIT		/NEW FILE BIT MAP ADDR.
	DAC	DTXROL
	LAC	DTOLBM		/OLD BIT MAP ADDR
	JMS	DTXOR		/XOR NEW INTO OLD BIT MAP
	LAC	(15000
	JMP	DTCLQ1		/OUTPUT BIT MAP BLOCK
/
	.EJECT
/SUBR. TO XOR BIT MAP 1 INTO BIT MAP 2
/ALSO CLEARS BIT MAP 1
DTXOR	0
DTXRNW=DTMPP			/NEW BIT MAP POINTER
	DAC	DTXRNW		/BIT MAP 2 ADDR
	LAW	-40
	DAC	DTCTS
DTXOR1	LAC*	DTXROL		/BIT MAP 1 POINTER
	XOR*	DTXRNW		/BIT MAP 2 POINTER
	DAC*	DTXRNW
	DZM*	DTXROL		/CLEAR BIT MAP 1
	ISZ	DTXROL
	ISZ	DTXRNW
	ISZ	DTCTS
	JMP	DTXOR1
	JMP*	DTXOR
/
DTCLS6	SAD	DTCLSS		/AC=0 ON ENTRY
	JMP	DTSTOP
	JMS	DTDRCK		/LOAD DIRECTORY INTO DTBUF
	LAC	DTLB40		/(DTBUF+40
	DAC	DTCLCT		/INIT. DIR ENTRY SECT. POINTER
	LAW	-340		/DIR. ENTRY SECTION COUNT
	DAC	DTCT
	LAC	DLTBUF		/(DTDIR+40=DTBUF)
	DAC	DTCT1
DTCLS5	LAC*	DTCLCT		/TRANSF. DIR ENTRY SECTION (+200)
	DAC*	DTCT1		/UP TO BIT MAP
	ISZ	DTCLCT
	ISZ	DTCT1
	ISZ	DTCT
	JMP	DTCLS5
	LAC	DLSAV		/(DTESAV
DTFIN=DTBFC2			/DTESAV POINTER
	DAC	DTFIN
	LAW	-4
	DAC	DTCT
DTCLS7	LAC*	DTFIN		/NEW FILE NAME (4 WDS)
	DAC*	DTCURE		/INTO DIRECTORY ENTRY SECTION
	ISZ	DTFIN
	ISZ	DTCURE
	ISZ	DTCT
	JMP	DTCLS7
	DZM	DTCLSS		/CLEAR CLOSE IND.
	LAC	(15000		/REWRITE DIRECTORY
	JMS	DTDRIN
	JMP	DTCLOS
/
	.EJECT
/.TRAN ROUTINE
DTAPE	JMS	DTIOU		/I/O UNDERWAY
	LAC*	DTARGP		/BL#
	JMS	DTSET		/SETUP BL#, ETC R/W, FOR/REV
	ISZ	DTARGP
	CLC
	DAC DTNCOR
	TAD*	DTARGP		/CORE ADDR. -1
	ISZ	DTARGP
	JMS	DTWCS		/SETUP CA AND START SEARCH
	LAC*	DTARGP		/WC
	DAC	DTWC
DTAPE1	ISZ	DTARGP
	JMP	DTDBK		/INDEX TO NORM EXIT
/SUBROUTINE TO SET UP BLOCK #, TRANSFER DIRECTION
DTSET	0
	DAC	DTNXBK
	LAC	DTCT		/TRANSFER DIRECTION
	RTR
	SMA!CLC			/OUTPUT
	LAC	(11000		/INPUT
	XOR	(2000
	AND	(17000
	DAC	DTTR		/WRITE (15000) OR READ (13000)
	SZL!CLA			/FORWARD
	CLC			/REVERSE
	DAC	DTDTR		/TRANSFER DIRECTION SWITCH
	JMP*	DTSET
/SUBR. TO SET UP CA, WC, AND TRANSFER
DTWCS	0
	DAC	DTCCA		/ADDR.-1(BIT 0-2 DO NOT MATTER)
DTUMSK	LAW	-400
	DAC	DTWC		/WORD COUNT (2'S COMP)
	LAW	-10
	DAC	DTERCT		/PARITY ERROR RETRY COUNT
	DAC	DTUND		/SET I/O UNDERWAY
	LAC	DTDTR		/TRANS. DIRECT. SWITCH
	AND	(1000		/AND
	XOR	DLITSM		/SMA!CLA=SEARCH FORW.
	DAC	DCHKC		/SPA!CLA=SEARCH REV.
	LAC	DTNXBK
	DAC	DTBLC
	LAC	DTDTR
	SMA!CLA			/-2 ON TRANSFER FORW.
	LAW	-4		/+2 ON TRANSFER REV.
	TAD	DLIT2		/(2
	DAC	DTBLNC		/SEARCH BLOCK INCREMENT
	JMS	DTSRCH		/SET UP FOR SEARCH
	LAC	DTDTR		/DIRECTION SWITCH
	AND	(40000
	XOR	(21400		/UNIT+21400=SEARCH FORW.
	XOR	DTUNIT		/UNIT+61400=SEARCH REV.
	DTLA
	JMP*	DTWCS		/EXIT SUBR
	.EJECT
/.READ, .WRITE COMMON SETUP SUBR.
DTMCK	0
	DAC	DTTR		/READ (13000) OR WRITE (15000)
	DAC	DTNCOR		/.SEEK, .ENTER  NOT EXECUTED
	XCT*	DTMCK		/L.B. OR DTA BUF. L.B. ADDR.
	DAC	DTUHP		/HEADER POINTER
	DAC	DTUDP		/DATA POINTER
	LAC* DTARGP		/(RCHM-107)
	DAC DTUBUF		/(RCHM-107)
	XCT CL.SW		/(RCHM-108)
	AND (700000)		/(RCHM-106) EXTRACT EXTENDED MEMORY BITS.
	SZA			/(RCHM-106) ANY SET?
	JMP IOPS67		/(RCHM-106) YES, GO PRINT ERROR.
	ISZ	DTARGP
	LAC*	DTARGP		/USER WC
	DAC	DTUWC
	LAC	DTCT		/DATA MODE
	DAC	DTDMOD
	ISZ	DTMCK		/INDEX TO DUMP EXIT
	SAD	DLIT4
	JMP	DTMCK2		/DUMP EXIT
	LAC (NOP)		/(RCHM-108)
	DAC CL.SW		/(RCHM-108)
	LAC*	DTUHP		/COMPUTE W.C. FROM L.B.H. W.P.C
	JMS	DTGWPC
	ISZ	DTMCK		/INDEX TO IOPS OR IMAGE EXIT
	JMP*	DTMCK		/IOPS OR IMAGE EXIT
DTMCK2	LAC	DTUWC		/SAVE USERWC
	DAC	DTWCSV
	CMA!IAC			/(RCHM-106) CONVERT TO A POSITIVE NUMBER.
	TAD DTUBUF		/(RCHM-107) ADD IN BUFFER STARTING ADDRESS.
	XCT CL.SW		/(RCHM-108)
	AND (700000)		/(RCHM-106) EXTRACT EXTENDED MEMORY BITS.
	SZA			/(RCHM-106) ANY SET?
	JMP IOPS67		/(RCHM-106) YES, GO PRINT ERROR MESSAGE.
	LAC (NOP)		/(RCHM-108)
	DAC CL.SW		/(RCHM-108)
	DZM	DTWPC
	XCT*	DTMCK	/JMP DTRDUM OR JMP DTWDUM
DTUBUF	XX			/(RCHM-107)
CL.SW	NOP			/(RCHM-108)
/SUBR. TO TRANSF. WPC FROM HEADER TO DTWPC
DTGWPC	0
	RTR
	RTR
	RTR
	RTR
	AND	(776
	DAC	DTWPC		/T. STORE L.B.W.P.C.
	SNA		/ILLEG. WPC (0 OR GREATER THAN 177)
	JMP DTER23
	AND (400
	SNA!CLA
	JMP*	DTGWPC		/L.B.W.C. INAC
DTER23	TAD	(5		/IOPS 23
	JMP	DTER16
/
	.EJECT
/SUBR. TO CHECK ACTIVE FILE
DTCKCL	0
	LAC	DTCLSS		/PREVIOUS FILE CLOSED
	SZA!CLA
	JMP	DTER10		/NO-FILE STILL ACTIVE
	JMS	DTDRCK		/CHECK FOR DIRECTORY IN CORE
	LAC*	DTARGP		/USER D.E. POINTER
	JMS	DTSK1		/DIR. SEARCH FOR FILE
	DAC	DTCLSS		/CLEAR OR SET CLOSE SWITCH
	JMP*	DTCKCL
/.SEEK ROUTINE
DTSEEK	LAC	DTIOSW
	SZA!CLC
	JMP DTER17		/TOO MANY FILES OPEN.
	JMS	DTCKCL		/CHECK DIRECTORY FOR THIS FILE
	SNA!CLC			/DTA DIR. ENTRY POINTER IN AC
	JMP	DTER14		/FILE NOT FOUND (DTER13)
	XCT	DTSK5		/PICK UP 1ST BLK # OF FILE
	XOR	(400000		/CLEAR FILE COMPLETE BIT
	DAC	DTNXBK		/1ST BLK # TO READ
	DAC	DTSKNT		/SET .SEEK, .ENTER EXECUTED SWITCH
	LAC	(13000
	DAC	DTTR		/INPUT
	DAC	DTNCOR		/CLEAR DIRECTORY IN CORE SWITCH
	DZM DTDMOD	/CLEAR DATA MODE TO BYPASS DUMP CHECK
	JMP	DTRNX1		/TRANSFER 1ST BLOCK
/
	.EJECT
/L.B. TO DTA BUF (.WRITE) OR DTABUF TO L.B. (.READ)
DTRWT	0
DTWT2	LAC*	DTUDP		/USER L.B.
	DAC*	DTHPT		/TO DTA BUFOR VICE VERSA
	JMS	DTUPTR		/ADD TO CKSUM, INDEX CTS, ETC
	ISZ	DTDATC		/DATA WORD COUNT
	ISZ	DTHPT
	ISZ	DTUWC		/DONE
	JMP	DTWT2
	JMP*	DTRWT
/.WRITE ROUTINE
DTWRIT	JMS	DTIOU		/I/O UNDERWAY
	LAC	DTMTP4		/SET EXIT TO
	DAC	DTOUT		/JMP DTAPE1
	DAC	DTWREX		/SET WRITE EXECUTED SWITCH
	LAC	(15000
	JMS	DTMCK		/READ/WRITE COMMON SETUP
	LAC*	DTARGP
	JMP	DTWDUM		/DUMP
/RETURN HERE FOR IOPS OR IMAGE MODES
DTWRT1	CLC
	TAD	DTWPC		/REMAINING BUF. AREA SIZE
	TAD	DTBFCT		/REMAINING BUF. AREA SIZE
	SMA!CLA
	JMP	DTCOUT		/NO ROOM FOR THIS LINE
	DAC	DTWRWT		/OUTPUT WAIT SWITCH-CLEAR
	LAC*	DTUHP
	AND	(7
	SAD	(5
	JMP	DTWRT4
	LAC*	DTUHP		/USER LBH., WD0
	AND	(377000
	XOR	DTDMOD		/DATA MODE
	DAC*	DTUHP
DTWRT4	ISZ	DTUHP		/CLEAR USER CKSM
	DZM*	DTUHP
	DZM	DTCKSM		/INIT CHECKSUM
	LAW	-377
	JMS	DTOBCK		/OUTPUT BUF. SIZE CHECK
	CLC			/EXCLUDE L.B.H.; WD0
	TAD	DTWPC		/FROM COUNT
	CMA
DTWT1	DAC	DTUWC		/ACTUAL WC (2'S COMP)
	LAC	DTHPT		/SETUP CKSM POINTER
	DAC	DTUCKP		/FOR .WRITE
	ISZ	DTUCKP
	JMS	DTRWT
	LAC	DTDMOD
	SAD	DLIT4
	JMP	DTDUMK		/DUMP MODE - CHECK FULL BUFF
/
	.EJECT
	CLC
	TAD	DTCKSM
	CMA
	DAC*	DTUCKP		/STORE 2'S COMP CKSUM IN DTABUF
DTWT5	LAC DTEOF		/EOF?
	SZA
	JMP DTCOUY		/YES, ALWAYS OUTPUT BLOCK
DTMTP4	JMP	DTAPE1		/IOPS WRITE COMPLETE
DTWRCL	JMS	DTBUFC		/CLEAR DTA BUF
	ISZ	DTARGP		/INDEX TO WC
	JMP	DTWRT1		/PUT LINE IN DTA BUF
/
/OUTPUT BUFFER SIZE CHECK
DTOBCK	0
	TAD	DTWPC		/L.B. W.C.
	SPA!CLA			/OUTPUT BUF OVERFLOW
	JMP*	DTOBCK
/
/ERROR ROUTINE
/
DTER16	TAD	DLIT2	/OUTPUT BUFFER OVERFLOW
			/DECTAPE FULL
DTER14	TAD	DLIT2	/DTA DIRECTORY FULL
			/FILE NOT FOUND
DTER12	TAD	DLIT2	/IRREC. DTA ERR. MK. TK., EOT DURING TRANSFER
			/.SEEK, .ENTER NOT EXECUTED
DTER10	TAD	DLIT2	/FILE STILL ACTIVE
			/ILL. DATA MODE
DTER6	TAD	(6		/ILL. HANDLER FUNCTION
/ALL ERRORS COME THRU HERE.
DTEROT	DAC	DTBUFC		/T. STORAGE.
	JMS	DTSTPA		/CLEAR SWITCHES
	DZM	DTUND
	LAC	DTBUFC		/AC=ERROR #.
	JMP*	DLIT4	/KM-9 ERR. LOC (.MED+1=4)
/
/CLEAR I/O BUF. SUBR., POINTERS
DTBUFC	0
	LAC	(377		/INIT DUMP MODE
	DAC	DTROOM		/BUF SIZE
	LAC DTIOSW
	RAR		/INPUT: L=0; OUTPUT: L=1
	LAC	DLTBUF		/BUF. (WD0) POINTER (DTBUF
	SZL!STL		/DO NOT MODIFY DTHPT ON INPUT
	/ALSO SET LINK TO CLEAR 400 CELLS
	DAC	DTHPT		/DTA BUF HEADER POINTER
	DAC	DTRHPT		/FOR READ
	JMS	DTBFC2	/CLEAR BUF
	JMP*	DTBUFC
/
	.EJECT
/CLEAR SPECIFIED AREA SUBR.
DTBFC3=DDIRAL
DTBFC2	0
	DAC	DTBFC3
	LAW	-40
	SZL		/CLEAR 40
	AND	DTUMSK	/CLEAR 400, DTUMSK=777400
	DAC	DTCLCT	/DZM COUNT
	DAC	DTBFCT		/INIT BUF SIZE CT.
	ISZ	DTBFCT
DTBFC1	DZM* DTBFC3
	ISZ	DTBFC3
	ISZ	DTCLCT
	JMP	DTBFC1
	JMP*	DTBFC2
/
/OUTPUT CURR. IOPS BUFFER
DTCOUT	LAC	(DTWRCL		/SET RETURN FROM INT.
	DAC	DTWRWT		/SET OUTPUT WAIT SWITCH
DTCOUY	LAC	DTBUSB
	DAC	DTOUT
DTCOUZ	LAC	DTCNBK		/CURR. BL# TO WRITE
	DAC	DTNXBK
	SPA!CLC
	JMP	DTER16		/DECTAPE FULL (DTER15)
	LAC DTWRWT	/IF DTWRWT NON 0,ALWAYS GET NEXT BLK #
	SNA!CLA
	LAC DTEOF
	JMS DTMAP		/FIND NEXT FREE BLOCK
	DAC DTBUF+377	/DATA LINK
DTCOUB	LAC	DLTBF1		/(DTBUF-1
	JMS	DTWCS		/SETUP WC,CA AND BEGIN TRAN.
DTOUT	JMP	DTAPE1
	.EJECT
/
/DUMP MODE OUPUT
DTWDUM	JMS	DTDUMB
DTDUMX	XX			/JMS DTBUFC OR NOP
	JMP	DTWT1
/
DTDUMB	0
	XCT*	DTDUMB		/JMS DTBUFC (WRITE) OR NOP (READ)
	ISZ	DTDUMB
	LAC DTWRCL	/SET SWITCH TO CLEAR
	DAC DTDUMX	/OUTPUT BUFF (JMS DTBUFC)
	LAC	DTROOM
	TAD	DTWCSV
	SMA			/MORE THAN 377 TO TRANSFER
	JMP	DTDUMZ		/LAST ELEMENT OF TRANSFER
	DAC	DTWCSV		/SAVE REMAINDER
	LAW	-2
	TAD	DTDUMB		/RET. ADDR. FOR TRANS. COMP
	DAC	DTWRWT		/=I/O WAIT SWITCH
	LAC	DTBUSB		/JMP DTBUSY
	DAC	DTOUT
	CLC
	TAD	DTROOM		/FILL IN BUFF
	CMA
DTDUMY	XCT*	DTDUMB		/JMP DTWT1(WRITE) OR JMP DTNSH1
DTDUMZ	DZM	DTWRWT		/CLEAR I/O WAIT SWITCH
	DAC	DTROOM		/SPACE LEFT FOR NEXT DUMP
	SNA
	JMP .+3		/FULL BUFF, DO NOT NOP CLEAR BUFF
	LAC DTLNOP	/SET SWITCH NOT TO CLEAR OUTPUT BUFF
	DAC DTDUMX
	LAC	DTMTP4
	DAC	DTOUT
	LAC	DTWCSV		/REMAINDER
	JMP	DTDUMY
DTDUMK	LAC DTROOM	/IF DTROOM=0, BUFF FULL
	SZA!CMA
	LAC DTWRWT	/IF DTWRWT=0,  BUFF NOT FULL
	SZA			/NO
	JMP	DTCOUZ		/YES - OUTPUT
	JMP	DTWT5		/CHECK EOF
/
	.EJECT
/.READ ROUTINE
DTREAD	LAC	DTEOF		/EOF SWITCH SET?
	SZA
	JMP	DTEFX		/YES - IGNORE CALL (AC MUST BE NON-0)
	JMS	DTIOU		/I/O UNDERWAY CHECK
	LAC*	DTARGP		/USER L.B. POINTER
	DAC	DTHPT
	DAC	DTHPTS
	LAC	DTMTP4		/JMP DTAPE1
	DAC	DTOUT
	LAC	(13000
	JMS	DTMCK		/READ/WRITE COMMON SETUP
	LAC	DTRHPT		/DTA BUF HEADER POINTER
	JMP	DTRDUM		/DUMP
/RETURN HERE FOR IOPS OR IMAGE MODES
	CLC
	TAD	DTWPC		/IOPS ASCII OR BIN
	TAD	DTUWC
	DZM	DTDVS		/CLEAR SHORT LINE FLAG
	SMA!CLC			/WPC INTO WC, NO SHORT LINE
	DAC	DTDVS		/SET SHORT LINE FLAG
	TAD	DTWPC
	CMA			/2'S COMP HEADER W.C.
	DAC	DTWPC
DTRD2	DZM	DTDATC		/DATA COUNT
	DZM	DTCKSM		/CLEAR CHECKSUM
	JMS	DTRWT		/TRANSFER LINE TO USER L.B.
	LAC	DTDMOD
	SAD	DLIT4
	JMP	DTRDM1		/DUMP
	LAC*	DTUDP		
	JMS	DTUPTR		/BYPASS EXCESS DATA
	JMP	.-2		/MORE
DTRDM1	LAC	DTROOM		/DUMP MODE BUF SIZE
	SZA!CMA		/IF DTROOM=0 OR DTWRWT = NON 0,
	LAC DTWRWT
	SZA!CLC
	JMP	DTRNEX		/GET NEXT DUMP BLOCK
	JMP	DTAPE1		/NORM EXIT
/
/SUBR. TO ADD TO CHKSUM AND INDEX COUNTS
DTUPTR	0
	TAD	DTCKSM		/ADD DATA WD TO CKSM.
	DAC	DTCKSM
	ISZ	DTUDP		/INDEX AREA POINTERS
	ISZ	DTRHPT
	ISZ	DTBFCT		/INCR DTA BUF COUNT
	ISZ	DTWPC		/GO TO DRDE ON OVERFLOW-DONE
	JMP*	DTUPTR
/
	.EJECT
/END INPUT LINE ROUTINE
	LAC*	DTHPTS		/HEADER WD 0-IOPS
	AND	(7
	SAD	(5		/EOF?
	JMP	DTREOF		/YES
	ISZ	DTDVS		/SHORT LINE FLAG SET
	JMP	DTRDE1		/NO
	LAC	(60
	JMS	DTDVS		/SET D.V. FOR  SHORT LINE
DTRDE1	LAC	DTERCT		/PARITY RETRY COUNT	
	SMA!CLA
	JMP	DTRDP		/SET D.V. BITS=PARITY
	LAC	DTCKSM
	SNA			/SET D.V. BITS=CKSUM ERROR
	JMP	DTRDN
	LAC	(20		/CHECKSUM ERR. IN LINE, 12,13=10
DTRDP	TAD	(20		/PARITY ERROR IN DTA BLOCK, 12,13=01
	JMS	DTDVS		/12,13=10
DTRDN	LAC*	DTUDP		/NEXT WORD IN DTA BUF
	SNA!CLC			/IF NOT 0, OK
	JMP	DTRNEX		/NO MORE DATA-GET NEXT BL.
	ISZ	DTBFCT		/DATA BUF. CT = GET NEXT BL.
	JMP	DTRNOR		/NORM EXIT, AC=777777
DTRNEX	SAD	DTBUF+377		/DATA LINK=-0?
	JMP	DTREOF		/LAST BLOCK -SET EOF SWITCH
	LAC	DTNXBK
	CMA
	TAD	DTBUF+377
	SPA!CLA			/READ FORW
	CLC			/READ REV.
	DAC	DTDTR		/TRANSF. DIRECTION SWITCH
	LAC	DTBUF+377
	DAC	DTNXBK		/DATA LINK INTO NEXT BLOCK
	DAC DTCNBK	/SET UP FOR .WRITE AFTER BACKSPACE
DTRNX1	JMS	DTBUFC	/INIT. BUFFER
	LAC DTDMOD	/DUMP?
	XOR DLIT4
	SZA
	JMP DTCOUB	/NO
	LAC DTRHPT	/RESET BUFF POINTER
	DAC DTUDP
	JMP DTCOUB
/
	.EJECT
/
/SUBR. TO SET DATA VALIDITY BITS
DTDVS	0
	DAC	DTDVSM		/SAVE MASK
	LAW	17717		/MASK ALL BUT BITS 0,12,13
	AND*	DTUHP
	XOR	DTDVSM
	DAC*	DTHPTS		/HEADER, WD0
	JMP*	DTDVS
DTEFX	ISZ	DTARGP
DTREOF	DAC	DTEOF		/SET EOF SWITCH
	JMP	DTAPE1		/EXIT
DTRNOR	TAD	DTBFCT		/DECR. (BY 1) DTFCT
	DAC	DTBFCT		/BUF COUNT
	JMP	DTAPE1		/NORM EXIT
DTNSH1	DAC	DTUWC
	JMP	DTRD2		/TRANSFER LINE
/
/DUMP MODE INPUT
DTRDUM	JMS	DTDUMB		/SET UP FOR DUMP INPUT
DTLNOP	NOP
	JMP	DTNSH1
/
/SUBROUTINE TO SAVE NEW D.E. IN DTESAV AREA
DTNTRZ	0
	LAC	DLSAV	/(DTESAV
	DAC	DTFIN	/DTFIN=DTBFC2
	LAW	-3		/SET DTA D.E.
	DAC	DTCT		/TRANSFER COUNTER
DTNTR2	LAC*	DTUDRP		/SAVE USER D.E. (4 WORD ENTRY)
DTNTR3	DAC*	DTFIN
	ISZ	DTFIN
	ISZ	DTUDRP
	ISZ	DTCT
	JMP	DTNTR2
	JMP*	DTNTRZ
/
	.EJECT
/DTA ENTER FILE ROUTINE
DTENTR	LAC	DTIOSW		/I/O SWITCH
	SNA!CLC
	JMP DTER17		/TOO MANY FILES OPEN.
	JMS	DTCKCL		/CHECK DIRECTORY FOR THIS FILE
	SZA			/NOT FOUND UNDER THIS FILE NAME
	JMP	DTNTR1		/FOUND-WILL BE MODIFIED ON .CLOSE
	LAC	DLFAKE		/INIT FOR EMPTY SLOT SEARCH (DTFAKE
	JMS	DTSK1		/D SEARCH FOR EMPTY FILE ENTRY
	DAC	DTCLSS		/CLEAR OR SET CLOSE SWITCH
	SNA			/EMPTY SLOT FOUND
	JMP	DTER14		/DIRECTORY FULL
DTNTR1	LAC*	DTARGP		/USER D.E. POINTER
	DAC	DTUDRP
	JMS	DTNTRZ		/SAVE USER D.E. IN DTESAV
	LAW -40		/INIT BIT MAP SEARCH
	DAC DTWMCT	/BIT MAP WORD COUNT
	LAC DLTDIR	/DIRECTORY BIT MAP POINTER
	DAC DTMTRX	/CURR DIR BIT MAP WORD POINTER
	LAC DLMBIT	/FILE BIT MAP POINTER
	DAC DTPONT	/CURR FILE BIT MAP WORD POINTER
	DZM DTRELB	/BLOCK NUMBER FOUND
	LAW -1100
	DAC DTBLOK	/BLOCK COUNT
	LAW -1		/INIT BIT MAP SEARCH TO PICK UP
	DAC DTREM	/FIRST EMPTY BLOCK
	DAC DTSKNT	/SET SEEK,ENTER EXECUTED SWITCH
	LAC DLIT1	/SET BIT MAP DIRECTION SWITCH
	DAC DTDIRA
	DAC DTDIRL	/TO FORWARD (+1)
	JMS DTMPS	/SET UP TO EXAMINE WD 0 OF MAP
	JMS DTMAP	/FIND FREE BLOCK #
	XOR	(400000
	XCT	DTNTR3		/STORE BL#+COMPLETION BIT IN DTESAV+3
	SMA!CLC
	JMP	DTER16		/DECTAPE FULL (DTER15)
	JMS	DTBUFC
	JMP	DTAPE1		/NORM EXIT
DTESAV	0			/NEW FILE ENTRY
	0
	0
	0
DTFAKE	0			/EMPTY SLOT FOR ENTER SEARCH (LAST WD. UNUSED)
	0
	0
DTEOFH	1005			/EOF HEADER FOR CLOSE
/
	.EJECT
/SUBR TO SET UP FOR EXAM OF NEXT BIT MAP WORD
DTMPS	0
	LAW	-22
	DAC	DTRBIT		/18 BIT COUNT
	LAC*	DTMTRX		/NEXT BIT MAP WD
	CMA!STL
	DAC	DTSBIT
	LAC	DTDIRA		/BIT MAP DIRECTION SWITCH
	SMA!CLA!RAL			/REVERSE-SEARCH BIT 18-0
	RTR			/FORWARD-SEARCH BIT 0-18
	DAC	DTTBIT		/FORWARD(0=1); REVERSE (18=1)
	JMP*	DTMPS
/
/END OF CURRENT BIT MAP WORD SUBR.
DTMPP	0
DTMPP1	LAC	DTDIRA		/INCR. (IF FORWARD) OR
	TAD	DTMTRX		/DECR. (IF REV) BY 1
	DAC	DTMTRX		/CURR. DIR BIT MAP WD. POINTER
	LAC	DTDIRA
	TAD	DTPONT
	DAC	DTPONT
	JMS	DTMPS		/SETUP FOR NEXT WD
	ISZ	DTWMCT		/BIT MAP WORD CT
	JMP*	DTMPP		/EXIT
	LAW	-1100	/LIT.
	DAC	DTBLOK		/DECTAPE FULL?
	DZM DTBMCT	/CLEAR BIT MAP SEARCH COUNT
	JMS DDIRAL	/FLIP DTDIRA,NEW DTDIRA IN AC ON RETURN
	TAD DTRELB		/REINIT
	DAC DTRELB
/ROUTINE TO SET DTREM FOR TURN AROUND CASE
	LAC DTDIRA
	RAL		/L=1=REV.,L=0=FORW.
	LAC DTNXBK	/LAST BL # RECORDED FOR THIS FILE
	SNL!CMA		/REV
	JMP DTMPP3
	TAD (1100
	CMA
DTMPP3	DAC DTREM		/LAW TO CHECK ENOUGH SPACE BETW. BL
	LAW -41
	DAC	DTWMCT		/MATRIX COUNT
	JMP	DTMPP1		/START REV. SEARCH
/SUBR TO FLIP DTDIRA AT DECTAPE TURNAROUND
DDIRAL	0
	CLA
	ISZ DTDIRA	/1 OR -1
	LAW -2		/SET TO REVERSE
	TAD DLIT1	/SET TO FORW
	DAC DTDIRA	/NEW DTDIRA MUST BE IN AC ON EXIT
	JMP* DDIRAL
	.EJECT
/BLOCK AVAILABILITY BIT MAP SEARCH
DTMAP	0
	DAC DTCLR2	/SAVE AC FOR -1 CASE
	DZM	DTBMCT	/BIT MAP SEARCH COUNT
DTMAP1	LAC	DTTBIT	/TEST BIT
DTMAP2	AND	DTSBIT		/MATRIX WORX
	SZA!CLC
DTMAP3	JMP	DTREM		/BLOCK AVAILABLE
	ISZ	DTBLOK		/INCREMENT DT BLOCK COUNT
	JMP DTMAP4
	DAC DTBLOK
	JMP DTREM5
DTMAP4	ISZ	DTBMCT
	LAC	DTDIRA		/IF FORW, INCR. BL#
	TAD	DTRELB		/IF REV., DECR. BL.# BY1
	DAC	DTRELB
	LAC	DTDIRA
	RAL			/L=0=FORW; L=1=REV.
	LAC	DTTBIT		/SHIFT TEST BIT RIGHT IF FORW,
	SNL!CLL!RAL			/LEFT IF REV.
	RTR
	DAC	DTTBIT
	ISZ	DTRBIT		/INDEX-18 BIT COUNT
	JMP	DTMAP2		/NEXT BIT
	JMS	DTMPP		/END OF MATRIX WD. SUBR.
	JMP	DTMAP1		/NEXT WORD
DTREM	XX		/DELTA BLOCKS IN BETWEEN
	TAD	DTBMCT
	SPA!CLC			/OK-DELTA BLOCKS IN BETWEEN
	JMP	DTMAP4		/CHECK BIT MAP AGAIN
	SAD DTCLR2	/IF ENTRY AC = -1, NO DTCBIT
	JMP DTREM6
	JMS	DTCBIT		/SET BIT IN MAPS.
	CMA
	DAC	DTSBIT
DTREM6	LAW -DELTA	/RESTORE BLOCK DISTANCE TO DELTA
	DAC DTREM
	LAC	DTDIRL		/SET TRANSF DIRECTION  SWITCH
	SPA!CLA
	CMA
	DAC	DTDTR
	LAC	DTDIRA		/UPDATE DTDIRL
	DAC	DTDIRL
	LAC	DTRELB		/T. STORE BL# TO BE  USED
DTREM5	DAC	DTCNBK		/EXIT
	LAW -1		/WAS AC = -1 ON ENTRY?
	SAD DTCLR2
	SKP		/YES, USE - 1 (EOF)
	LAC DTCNBK
	JMP*	DTMAP		/EXIT -BL ! FOUND(777777=DTA FULL)
	.EJECT
/CHANGE BIT IN MAPS SUBR.
DTCBIT	0
	LAC	DTTBIT		/SET BIT IN FILE BIT MAP
	XOR*	DTPONT
	DAC*	DTPONT
	LAC DTTBIT		/SET BIT IN DIRECTORY BIT MAP
	XOR*	DTMTRX
	DAC*	DTMTRX
	JMP*	DTCBIT	/C(*DTMTRX) MUST BE IN AC ON EXIT
/CLEAR DIRECTORY ROUTINE
DTCLR2	XX			/LAC DTBLBT = BLOCK TABLE
	DZM	DTCT
	ISZ	DTCT	/WRITE FORWARD
	JMS	DTSET		/SET BL# ETC
	LAC DLTBF1
	JMS	DTWCS		/SET UP CA,WC+BEGIN TRANSFER
	ISZ	DTCLR2		/INDEX FOR NEXT TRANSFER
DTCLER	JMS	DTIOU		/WAIT FOR I/O TO FINISH
	LAC	DTCLSS		/CLOSE SWITCH CLEAR?
	SZA!CLA			/YES
	JMP	DTER10		/FILE STILL ACTIVE
	LAC	(DTCLR1		/SET RETURN AND
	DAC	DTWRWT		/I/O WAIT SWITCH
	DAC	DTNCOR		/CLEAR DIR IN CORE SWITCH
	LAC	(LAC DTBLBT
	DAC	DTCLR2		/INIT TABLE REF
	JMS DTBUFC	/CLEAR BUFFER TO ZERO BLK 71-77
	LAW -10
	DAC DTREM	/COUNT FOR FILE BIT MAP BLOCKS
	LAW	-11
	DAC	DTCLCT		/COUNT OF BLOCKS TO CLEAR+1
DTCLR1	ISZ DTREM	/FILE BIT MAP BLOCKS CLEARED?
	JMP .+4
	LAC (77600	/YES, INIT DIRECTORY TO 8 SYS BLKS
	DAC DTBUF+3
	DAC DTBUF+203	/BASIC DIRECTORY BIT MAP
	ISZ	DTCLCT		/DONE
	JMP	DTCLR2
	DZM	DTWRWT		/YES-CLEAR I/O WAIT SWITCH
	JMP	DTDBK
/DTCLER BLOCK TABLE
DTBLBT	71			/BLOCKS 71-73 CONTAIN
	72			/24 BIT MAPS ORDERED ACCORDING
	73		/TO THE FILE NAMES IN THE DIR. ENTRY SECTION
	74
	75
	76
DLIT77	77
DLT100	100			/BLOCK 100 = DIRECTORY
/
/
/DTMBIT=FILE BIT MAP, MUST INITIALLY = 0
DTMBIT	0
	.LOC	DTMBIT+40
DTDIR	0			/DTA DIRECTORY
	.LOC	DTDIR+40
DTBUF	0			/DTA BUFFER
	.LOC	DTBUF+400
DLTDIR	DTDIR			/DIRECTORY POINTER
DLTDR1	DTDIR-1			/DIRECTORY POINTER-1 (FOR LOADING C.A.)
DLTSYS	DTDIR+203	/WD 3 OF SYS BIT MAP
DLTBF1	DTBUF-1			/DTA BUFF POINTER-1
DLTBUF	DTBUF			/DTA BUF. POINTER
DLEOFH	DTEOFH			/EOF HEADER POINTER (FOR .CLOSE)
DTLB40	DTBUF+40			/DIR. ENTRY POINTER (.CLOSE)
DLSAV	DTESAV		/POINTER TO 1ST CELL OF NEW DIR. ENTRY
DLFAKE	DTFAKE			/POINTER TO EMPTY FILE NAME
DLMBIT	DTMBIT			/FILE BIT MAP ADDR. POINTER
DTARGP	0			/ENTRANCE ARG. POINTER
DTCCA	0			/CURRENT ADDR. (C.A.) POINTER FOR TRANSFER
DTCALP	0			/USER CAL POINTER
DTCNBK	0			/DATA LINK (NEXT BL.#)
DTCURE	0			/DIR. POINTER TO CURR. FILE ENTRY EXAMINED
DTDIRA	0			/BIT MAP DIRECTION SWITCH (CURR. BL.)+1=F,-1=R
DTDIRL	0			/BIT MAP DIRECTION SWITCH (LAST.BL.),+1=F,-1=R
DTDMOD	0			/DATA MODE (15-17)
DTEOF	0			/EOF SWITCH, -0=EOF
DTFPCT	0			/FILE POSITION COUNTER
DTHPT	0			/DTA BUF. LINE HEADER POINTER (INDEXED)
DTHPTS	0			/DTA BUF. LINE HEADER POINTER
DTIOSW	0			/I/O SWITCH, 0=INPUT, 1=OUTPUT
DTMTRX	0			/CURRENT BIT MAP WD. POINTER
DTPONT	0			/CURR. FILE BIT MAP WD. POINTER
DTWREX	0			/0=NO WRITE EXECUTED, NON 0=EXECUTED
DTNCOR	077777			/DIRECTORY IN CORE SWITCH, (0-2)=UNIT=IN
DTRBIT	0			/18 BIT (2'S COMP) COUNTER FOR BIT MAP SEARCH
DTRELB	0			/FREE BL.# AFTER BIT MAP SEARCH
DTRHPT	0			/DTA BUF. LINE HEADER POINTER (.READ)
DTSBIT	0			/-(MATRIX WORD)
DTSKNT	0			/.SEEK,.ENTER EXECUTED SWITCH (NON 0=EXECUTED)
DTTBIT	0			/TEST BIT FOR BIT MAP SEARCH
DTTR	0			/DTA SEARCH-READ(13000) OR SEARCH-WRITE(15000)CONVERSION FACTOR
DTUCKP	0			/USER LINE BUF. CHECKSUM POINTER
DTUDP	0			/USER LINE BUF DATA POINTER (MODIFIED)
DTUND	0			/I/O UNDERWAY SWITCH,-=BUSY,0=NOT BUSY
DTUNIT	0			/(0-2)=DTA UNIT# FOR TRANSFER
DTWC	0			/2'S COMP TRANSFER WORD COUNT
DTWMCT	0			/BIT MAP WORD COUNT
DTWRWT	0			/CONTINUED I/O SWITCH (NON-0=CONT),0=DONE)
DTCKSM	0			/LINE CHECKSUM
DTCLSS	0			/FILE OPEN, CLOSE SWITCH(NON-0=OPEN,0=CLOSED)
DTCT	0			/GEN. PURPOSE COUNTER=T.STORE
DTBFCT	0			/BUFFER COUNT (INIT=-377)
DTEOTS	0			/END ZONE (EOT) ENTERED SWITCH (0=NOEOT. -0=EOT)
DTEOTZ	0			/DOUBLE END ZONE SWITCH (0=SET) (-0=CLEAR)
DBLKLC	0		/24 OR 56 FILE SWITCH(50=24;10=56)
DTBLOK	0		/BLOCK COUNT
DATSLT	0			/CURRENT .DAT SLOT
DATPST	0			/PAST .DAT SLOT.
DLIT1	1
DLIT2	2
DLIT3	3
DLIT4	4
DTUDRR=DTDVS			/USER DIR. ENTRY POINTER (FIXED)
DTUDRP=DTCKSM			/USER DIR. ENTRY POINTER (INDEXED)
DTCTS=DTCCA			/ENTRY COUNT (-3)
DTCT1=DTUPTR			/GEN. PURP. COUNTER AND T. STOR.
DTDATC=DTTABL			/LINE DATA COUNT
DTUHP=DTDRIN			/USER LINE BUF. HEADER POINTER
DTCT1S=DTWC			/MATCH COUNT (-4)
DTDES=DTWCS			/DTA DIR. ENTRY SECTION POINTER (INDEXED)
DTUWC=DTCCA			/USER 2'S COMP WC FOR ARG. LIST
DTDVSM=DTCALP			/DATA VALIDITY BIT MASK
DTBMCT=DTOBCK			/BIT MAP SEARCH COUNT (MUST BE 5 OR MORE TO EXIT)
DTCLCT=DTMPP			/CLEAR COUNT (INIT=-200)
DTWCSV=DTGWPC
DTWPC=DTSET			/WORD PR. COUNT FROM HEADER
DTDLUN=DTEOF			/RENAME OR DELETE UNDERWAY
	.END
