/ 
/ 
/                   FIRST PRINTING, FEBRUARY 1974
/ 
/ THE INFORMATION IN THIS DOCUMENT IS SUBJECT TO 
/ CHANGE WITHOUT NOTICE AND SHOULD NOT BE CONSTRUED
/ AS A COMMITMENT BY DIGITAL EQUIPMENT CORPORATION.
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPON-
/ SIBILITY FOR ANY ERRORS THAT MAY APPEAR IN THIS
/ DOCUMENT.
/ 
/ THE SOFTWARE DESCRIBED IN THIS DOCUMENT IS FUR-
/ NISHED TO THE PURCHASER UNDER A LICENSE FOR USE ON
/ A SINGLE COMPUTER SYSTEM AND CAN BE COPIED (WITH
/ INCLUSION OF DIGITAL'S COPYRIGHT NOTICE) ONLY FOR 
/ USE IN SUCH SYSTEM, EXCEPT AS MAY OTHERWISE BE PRO-
/ VIDED IN WRITING BY DIGITAL.
/ 
/ DIGITAL EQUIPMENT CORPORATION ASSUMES NO RESPONSIBILITY
/ FOR THE USE OR RELIABILITY OF ITS SOFTWARE ON EQUIP-
/ MENT THAT IS NOT SUPPLIED BY DIGITAL.
/ 
/ COPYRIGHT (C) 1974, BY DIGITAL EQUIPMENT CORPORATION
/ 
/ 
        .EJECT
/	SLIOT SRC(SLIP COMPONENT)  EDIT #1  6/30/73  G. COLE
/	COPYRIGHT DIGITAL EQUIPMENT CORP. 1973
SLIOUT	0		/ROUTINE TO OUTPUT A LINE WITHOUT CHARRIAGE 
	JMS*	.DA
	JMP	.+1+3
LUN	0
BUF	0
LEN	0
	LAC*	LEN	/GET # OF WORD PAIRS
	IAC		/ADD ONE FOR HEADER
	IAC		/ADD ONE FOR TRAILER CR
	SWHA		/MOVE TO PROPER PLACE
	AAC	2	/SET THE MODE IOPS ASCII
	DAC*	BUF	/PUT INTO HEADER
	LAC*	LUN
	DAC	LN	/BUILD CAL
	LAC	BUF	/ADDRESS OF BUFFER
	DAC	BF
	LAC	BUF
	TAD*	LEN
	TAD*	LEN
	AAC	2
	DAC	ZZ
	LAC	CRLF
	DAC*	ZZ
	ISZ	ZZ
	DZM*	ZZ
	CAL	WRITE
	CAL	WAIT
	DZM*	ZZ
	JMP*	SLIOUT
ZZ	0
WRITE	2700
	EV
LN	0
MODE	2
BF	0
WAIT	20
	EV
EV	0
CRLF		064240
	.GLOBL	SLIOUT,.DA
	.END
