;microcrox for SCI system

;Initialize switch settings
.INSERT SWINIT.SLO

; SET F2SW = 1 FOR F2,  F2SW = 0 FOR F3

XUCODE = 1

F2SW = 1

NEWMAP = 0

TLXTAPE = 0		;Down: THIS IMPLIES TELEX TAPE CTRLR

NTP = 1
TAPE = 1

DLS = 1			;Set to 1 to include DLS
DLSDEB = 1		;Set to 1 for debugging
DLS2 = 1
DLSDEV = 20

IMP = 1			;Set to 1 to include IMP

VC = 1
 VCDEV = 14

XLIST

.INSERT CFDEF.SLO

LIST

.INSERT CFNEW

LIST-LABELS
LIST-CORMAP
