;F2 with 8K micro-memory

;Initialize switch settings
.INSERT SWINIT.SLO

; F2 VERSION OF MICROCODE

; SET F2SW = 1 FOR F2,  F2SW = 0 FOR F3

F2SW = 1

;;XUCODE = 1	;8K u-mem present

XLIST

NEWMAP = 0

.INSERT CFDEF.SLO

LIST

TIMER = 0

IMP = 0

DLSDEV = 20	; udevice code for TTY scanner

DLS = 1

DLSDEB = 1

DLS2 = 0

NTP = 1

;;;VID = 1

VC = 1		; Set to 1 for Versatec
VCDEV = 14	; udevice code for Versatec

CROCK = 1		;for now!!

.DEFINE DLIST [] [LIST]	;Define as LIST to enable FOOLIST
.DEFINE DXLIST [] [XLIST]	;Define as XLIST for FOOLIST stuff
.INSERT CFMAIN

LIST-LABELS
LIST-CORMAP
