;F2 with 4K micro-memory

;Initialize switch settings
.INSERT SWINIT.SLO

; F2 VERSION OF MICROCODE

; SET F2SW = 1 FOR F2,  F2SW = 0 FOR F3

F2SW = 1


XLIST

.INSERT CFDEF.SLO

LIST

NEWMAP = 1

TIMER = 1

IMP = 1

DLSDEV = 20	; udevice code for TTY scanner


TYMNET = 1

DLS2 = 1

NTP = 1


VCDEV = 14	; udevice code for Versatec

CROCK = 1		;for now!!

.DEFINE DLIST [] [LIST]	;Define as LIST to enable FOOLIST
.DEFINE DXLIST [] [XLIST]	;Define as XLIST for FOOLIST stuff
.INSERT CFMAIN

LIST-LABELS
LIST-CORMAP
